NXP Software Content Register

Package:                   AN14808.7z

Version:                   1.0
Outgoing License:          BSD-3-Clause
License File:              COPYING-BSD-3
Type of content:           source code
Description and comments:  This application code is to demonstrate how to connect to USB 4G module.
Release Location:          https://www.nxp.com/products/processors-and-microcontrollers/arm-microcontrollers/i-mx-rt-crossover-mcus/i-mx-rt1170-crossover-mcu-dual-core-arm-cortex-m7-and-cortex-m4-operating-up-to-1-ghz:i.MX-RT1170
Origin:                    Software_release_for_AN14808 (BSD-3-Clause) - https://www.nxp.com/products/processors-and-microcontrollers/arm-microcontrollers/i-mx-rt-crossover-mcus/i-mx-rt1170-crossover-mcu-dual-core-arm-cortex-m7-and-cortex-m4-operating-up-to-1-ghz:i.MX-RT1170"
						   nxp-mcuxpresso/mcux-sdk (BSD-3-Clause) - https://mcuxpresso.nxp.com
                           FreeRTOS Real Time Kernel (MIT) - https://sourceforge.net/projects/freertos
						   lwIP (BSD-3-Clause) - http://savannah.nongnu.org/projects/lwip  
						   CMSIS_5 (Apache-2.0) - https://github.com/ARM-software/CMSIS_5/releases/tag/5.9.0						   
                           