===============================================================
MSC8144 ADS Stationery

Copyright 2006 Freescale Semiconductor
===============================================================

Important
---------------------------------------------------------------
When using MSC8144ADS boards revision 2.5 or higher
please make sure that your project is including the initialization file

StarCore_Support\Initialization_Files\RegisterConfigFiles\MSC8144_ADS\MSC8144_Pacsun_Init_without_m3_patch.cfg
---------------------------------------------------------------

Default Project Settings:
---------------------------------------------------------------
  - Compiler Target Architecture = MSC8144
  - Debugger Target = MSC8144ADS 
  - Remote Connection = StarCore CSS - MSC8144 ADS
  - In "Remote Debugging" panels for all MSC8144 projects, 
    set Connection to "StarCore CCS - MSC8144 ADS".
  - Enable "Reset On Connect" for the Core 0 project
    in the SC100 Debugger Target Panel.

Pacsun only JTAG chain
---------------------------------------------------------------
  - Board jumper SW2.3 should be OFF

Pacsun+Dracon(e500) JTAG chain
---------------------------------------------------------------
  - Board jumper SW2.3 should be ON
  - Edit "StarCore CCS - MSC8144 ADS" connection and change
    the JTAG configuration file from ...\MSC8144ADS_JTAG.cfg to 
    ...\MSC8144ADS_WITH_e500_JTAG.cfg
  - A CodeWarrior for EPPC compatible initialization file for
    the host is available in:
    StarCore_Support\Initialization_Files\RegisterConfigFiles
    \8560Pacsun_init.cfg
  - Disable "Reset On Connect" in the SC100 Debugger Target Panel
    of the second project

Multi-core support
---------------------------------------------------------------

  The default stationery comprises projects for each 8144 core
of the Pacsun.  Starting with Alpha 3.1, the master (core 0) 
project launches automatically all 4 debug sessions.