Analog Sensing for AC Motors (ASAC) eTPU Function
AC Motor Control
eTPU Function Set
The ASAC function is useful for preprocessing up to four analog values that are measured by an AD converter and transferred to the eTPU data memory by DMA transfer. The ASAC function is also useful for triggering the AD converter and synchronizing other eTPU functions.

For full description refer to AN2970.
Designed by Roznov Czech System Center, Freescale Semiconductor, Inc. 2005.
eTPU Product Summary Page