## Project Name: ramISR

### Date Created: Dec 9, 2014, 11:56:25 PM

## PIN Assignments for MC56F82748VLH 64 LQFP64 package

|  | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 |  |
|  | GPIOA3 | GPIOA2 | GPIOA1 | GPIOA0 | GPIOA4 | GPIOA5 | GPIOA6 | GPIOA7 | GPIOC4 | GPIOC3 | GPIOF8 | GPIOC2 | GPIOC1 | GPIOC0 | RESETB/VPP | TCK |  |
17 | GPIOB7 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | TDI | 64
18 | GPIOC5 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | TMS | 63
19 | GPIOB6 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | TDO | 62
20 | GPIOB5 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | VSS | 61
21 | GPIOB4 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | VDD | 60
22 | VDDA |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | GPIOF7 | 59
23 | VSSA |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | GPIOF6 | 58
24 | GPIOB0 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | VCAP | 57
25 | GPIOB1 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | GPIOC15 | 56
26 | VCAP |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | GPIOC14 | 55
27 | GPIOB2 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | GPIOE7 | 54
28 | GPIOB3 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | GPIOE6 | 53
29 | VDD |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | GPIOE5 | 52
30 | VSS |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | GPIOE4 | 51
31 | GPIOC6 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | GPIOF1 | 50
32 | GPIOC7 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | GPIOC13 | 49
|  | GPIOC8 | GPIOC9 | GPIOC10 | GPIOF0 | GPIOC11 | GPIOC12 | GPIOF2 | GPIOF3 | GPIOF4 | GPIOF5 | VSS | VDD | GPIOE0 | GPIOE1 | GPIOE2 | GPIOE3 |  |
|  | 33 | 34 | 35 | 36 | 37 | 38 | 39 | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47 | 48 |  |

## Pin Allocation Report

Peripheral | Custom peripheral name | Peripheral description
--- | --- | ---
ADC | ADC | Analog-to-Digital Converter
AOI | AOI | AND/OR/INVERT module
CAN | CAN | Freescale's Scalable Controller Area Network
CMPA | CMPA | High-Speed Comparator (CMP), Voltage Reference (VREF) Digital-to-Analog Converter (DAC), and Analog Mux (ANMUX)
CMPB | CMPB | High-Speed Comparator (CMP), Voltage Reference (VREF) Digital-to-Analog Converter (DAC), and Analog Mux (ANMUX)
CMPC | CMPC | High-Speed Comparator (CMP), Voltage Reference (VREF) Digital-to-Analog Converter (DAC), and Analog Mux (ANMUX)
CMPD | CMPD | High-Speed Comparator (CMP), Voltage Reference (VREF) Digital-to-Analog Converter (DAC), and Analog Mux (ANMUX)
DACA | DACA | 12-Bit Digital-to-Analog Converter
DACB | DACB | 12-Bit Digital-to-Analog Converter
DMA | DMA | DMA Controller
EONCE | EONCE | Enhanced On-Chip Emulation
EWM | EWM | EWM device
GPIOA | GPIOA | General Purpose Input/Output
GPIOB | GPIOB | General Purpose Input/Output
GPIOC | GPIOC | General Purpose Input/Output
GPIOD | GPIOD | General Purpose Input/Output
GPIOE | GPIOE | General Purpose Input/Output
GPIOF | GPIOF | General Purpose Input/Output
I2C | I2C | Inter-integrated circuit bus
OCCS | OCCS | On-Chip Clock Synthesis
PIT0 | PIT0 | Periodic Interrupt Timer Module
PIT1 | PIT1 | Periodic Interrupt Timer Module
PWMA | PWMA | Pulse Width Modulator with nano edge placement
QSCI0 | QSCI0 | Serial Communications Interface Module QSCI0
QSCI1 | QSCI1 | Serial Communications Interface Module QSCI1
QSPI0 | QSPI0 | Queued Serial Peripheral Interface
QSPI1 | QSPI1 | Queued Serial Peripheral Interface
SIM | SIM | System Integration Module
TMR | TMR | Quad Timer Module
XBARA | XBARA | Crossbar Switch

## Routed Pins

| Assigned Pin Function(s)
Package Pin # | Pin Name | User Assigned Signal Name | Assigned Peripheral | Assigned Function | Package Function | Dir
--- | --- | --- | --- | --- | --- | ---
1 | TCK/GPIOD2 | same | EONCE | TCK | alt0 | Input
2 | RESETB/VPP/GPIOD4 | same | non-peripheral | RESET | alt0 | Not Specified
non-peripheral | vpp | alt0 | Not Specified
3 | GPIOC0/EXTAL/CLKIN0 | same | GPIOC | port0 | gpio_function | Not Specified
4 | GPIOC1/XTAL | same | GPIOC | port1 | gpio_function | Not Specified
5 | GPIOC2/TXD0/XB_OUT11/XB_IN2/CLKO0 | same | GPIOC | port2 | gpio_function | Not Specified
6 | GPIOF8/RXD0/XB_OUT10/CMPD_O/PWM_2X | same | GPIOF | port8 | gpio_function | Not Specified
7 | GPIOC3/TA0/CMPA_O/RXD0/CLKIN1 | same | GPIOC | port3 | gpio_function | Not Specified
8 | GPIOC4/TA1/CMPB_O/XB_IN6/EWM_OUT_B | same | GPIOC | port4 | gpio_function | Not Specified
9 | GPIOA7/ANA7/CMPD_IN3 | same | GPIOA | port7 | gpio_function | Not Specified
10 | GPIOA6/ANA6/CMPD_IN2 | same | GPIOA | port6 | gpio_function | Not Specified
11 | GPIOA5/ANA5/CMPD_IN1 | same | GPIOA | port5 | gpio_function | Not Specified
12 | GPIOA4/ANA4/CMPD_IN0 | same | GPIOA | port4 | gpio_function | Not Specified
13 | GPIOA0/ANA0/CMPA_IN3/CMPC_O | same | GPIOA | port0 | gpio_function | Not Specified
14 | GPIOA1/ANA1/CMPA_IN0 | same | GPIOA | port1 | gpio_function | Not Specified
15 | GPIOA2/ANA2/VREFHA/CMPA_IN1 | same | GPIOA | port2 | gpio_function | Not Specified
16 | GPIOA3/ANA3/VREFLA/CMPA_IN2 | same | GPIOA | port3 | gpio_function | Not Specified
17 | GPIOB7/ANB7/CMPB_IN2 | same | GPIOB | port7 | gpio_function | Not Specified
18 | GPIOC5/DACA_O/XB_IN7 | same | GPIOC | port5 | gpio_function | Not Specified
19 | GPIOB6/ANB6/CMPB_IN1 | same | GPIOB | port6 | gpio_function | Not Specified
20 | GPIOB5/ANB5/CMPC_IN2 | same | GPIOB | port5 | gpio_function | Not Specified
21 | GPIOB4/ANB4/CMPC_IN1 | same | GPIOB | port4 | gpio_function | Not Specified
22 | VDDA | same | ADC | ADCvrefVREFHA | gpio_function | Input
ADC | ADCvrefVREFHB | gpio_function | Input
non-peripheral | VCC | gpio_function | Not Specified
23 | VSSA | same | ADC | ADCvrefVREFLA | gpio_function | Input
ADC | ADCvrefVREFLB | gpio_function | Input
non-peripheral | GND | gpio_function | Not Specified
24 | GPIOB0/ANB0/CMPB_IN3 | same | GPIOB | port0 | gpio_function | Not Specified
25 | GPIOB1/ANB1/CMPB_IN0/DACB_O | same | GPIOB | port1 | gpio_function | Not Specified
26 | VCAP_26 | same | non-peripheral | other | gpio_function | Not Specified
27 | GPIOB2/ANB2/VREFHB/CMPC_IN3 | same | GPIOB | port2 | gpio_function | Not Specified
28 | GPIOB3/ANB3/VREFLB/CMPC_IN0 | same | GPIOB | port3 | gpio_function | Not Specified
29 | VDD_29 | same | non-peripheral | VCC | gpio_function | Not Specified
30 | VSS_30 | same | non-peripheral | GND | gpio_function | Not Specified
31 | GPIOC6/TA2/XB_IN3/CMP_REF/SS0_B | same | GPIOC | port6 | gpio_function | Not Specified
32 | GPIOC7/SS0_B/TXD0/XB_IN8 | same | GPIOC | port7 | gpio_function | Not Specified
33 | GPIOC8/MISO0/RXD0/XB_IN9/XB_OUT6 | same | GPIOC | port8 | gpio_function | Not Specified
34 | GPIOC9/SCK0/XB_IN4/TXD0/XB_OUT8 | same | GPIOC | port9 | gpio_function | Not Specified
35 | GPIOC10/MOSI0/XB_IN5/MISO0/XB_OUT9 | same | GPIOC | port10 | gpio_function | Not Specified
36 | GPIOF0/XB_IN6/SCK1 | same | GPIOF | port0 | gpio_function | Not Specified
37 | GPIOC11/CANTX/SCL0/TXD1 | same | GPIOC | port11 | gpio_function | Not Specified
38 | GPIOC12/CANRX/SDA0/RXD1 | same | GPIOC | port12 | gpio_function | Not Specified
39 | GPIOF2/SCL0/XB_OUT6/MISO1 | same | GPIOF | port2 | gpio_function | Not Specified
40 | GPIOF3/SDA0/XB_OUT7/MOSI1 | same | GPIOF | port3 | gpio_function | Not Specified
41 | GPIOF4/TXD1/XB_OUT8/PWM_0X/PWM_FAULT6 | same | GPIOF | port4 | gpio_function | Not Specified
42 | GPIOF5/RXD1/XB_OUT9/PWM_1X/PWM_FAULT7 | same | GPIOF | port5 | gpio_function | Not Specified
43 | VSS_43 | same | non-peripheral | GND | gpio_function | Not Specified
44 | VDD_44 | same | non-peripheral | VCC | gpio_function | Not Specified
45 | GPIOE0/PWM_0B | same | GPIOE | port0 | gpio_function | Output
46 | GPIOE1/PWM_0A | same | GPIOE | port1 | gpio_function | Output
47 | GPIOE2/PWM_1B | same | GPIOE | port2 | gpio_function | Not Specified
48 | GPIOE3/PWM_1A | same | GPIOE | port3 | gpio_function | Not Specified
49 | GPIOC13/TA3/XB_IN6/EWM_OUT_B | same | GPIOC | port13 | gpio_function | Not Specified
50 | GPIOF1/CLKO1/XB_IN7/CMPD_O | same | GPIOF | port1 | gpio_function | Not Specified
51 | GPIOE4/PWM_2B/XB_IN2 | same | GPIOE | port4 | gpio_function | Not Specified
52 | GPIOE5/PWM_2A/XB_IN3 | same | GPIOE | port5 | gpio_function | Not Specified
53 | GPIOE6/PWM_3B/XB_IN4 | same | GPIOE | port6 | gpio_function | Not Specified
54 | GPIOE7/PWM_3A/XB_IN5 | same | GPIOE | port7 | gpio_function | Not Specified
55 | GPIOC14/SDA0/XB_OUT4/PWM_FAULT4 | same | GPIOC | port14 | gpio_function | Not Specified
56 | GPIOC15/SCL0/XB_OUT5/PWM_FAULT5 | same | GPIOC | port15 | gpio_function | Not Specified
57 | VCAP_57 | same | non-peripheral | other | gpio_function | Not Specified
58 | GPIOF6/PWM_3X/XB_IN2 | same | GPIOF | port6 | gpio_function | Not Specified
59 | GPIOF7/CMPC_O/SS1_B/XB_IN3 | same | GPIOF | port7 | gpio_function | Not Specified
60 | VDD_60 | same | non-peripheral | VCC | gpio_function | Not Specified
61 | VSS_61 | same | non-peripheral | GND | gpio_function | Not Specified
62 | TDO/GPIOD1 | same | EONCE | TDO | alt0 | Output
63 | TMS/GPIOD3 | same | EONCE | TMS | alt0 | Input
64 | TDI/GPIOD0 | same | EONCE | TDI | alt0 | Input

## Routable Pins

| alt0 | alt1 | alt2 | alt3 | gpio function
Package Pin # | Pin Name | User Assigned Signal Name | Peripheral | Function | Dir | Peripheral | Function | Dir | Peripheral | Function | Dir | Peripheral | Function | Dir | Peripheral | Function | Dir
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | TCK/GPIOD2 | same | EONCE | TCK | Input |  |  |  |  |  |  |  |  |  |  |  |
2 | RESETB/VPP/GPIOD4 | same | non-peripheral | RESET vpp |  |  |  |  |  |  |  |  |  |  |  |  |
3 | GPIOC0/EXTAL/CLKIN0 | same | OCCS | EXTAL | Input | OCCS | ClockInput | Input |  |  |  |  |  |  |  |  |
4 | GPIOC1/XTAL | same | OCCS | XTAL | Output |  |  |  |  |  |  |  |  |  |  |  |
5 | GPIOC2/TXD0/XB_OUT11/XB_IN2/CLKO0 | same | QSCI0 | sci_tx | Output | XBARA CMPA CMPB CMPC CMPD TMR TMR TMR TMR AOI AOI AOI AOI PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PIT0 PIT1 | xBarOut11 Output Output Output Output TMR_OUT_PIN0 TMR_OUT_PIN1 TMR_OUT_PIN2 TMR_OUT_PIN3 Output0 Output1 Output2 Output3 OutputTrigger00 OutputTrigger10 OutputTrigger01 OutputTrigger11 OutputTrigger02 OutputTrigger12 OutputTrigger03 OutputTrigger13 PIT_OUT_PIN PIT_OUT_PIN | Output | XBARA AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI DMA DMA DMA DMA ADC ADC DACB DACA CMPA CMPB CMPC CMPD PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA TMR TMR TMR TMR QSCI0 QSCI1 EWM | xBarIn2 InputA0 InputB0 InputC0 InputD0 InputA1 InputB1 InputC1 InputD1 InputA2 InputB2 InputC2 InputD2 InputA3 InputB3 InputC3 InputD3 DMAtrigger0 DMAtrigger1 DMAtrigger2 DMAtrigger3 ADCtriggerA ADCtriggerB DACtrigger DACtrigger WindowSample WindowSample WindowSample WindowSample ExternalControlA0 ExternalControlA1 ExternalControlA2 ExternalControlA3 ExternalSync0 ExternalSync1 ExternalSync2 ExternalSync3 EXT_CLK Fault0 Fault1 Fault2 Fault3 ExternalForce TMR_IN_PIN0 TMR_IN_PIN1 TMR_IN_PIN2 TMR_IN_PIN3 sci_rx sci_rx ewminput | Input | SIM | ClockOutput0 | Output |  |  |
6 | GPIOF8/RXD0/XB_OUT10/CMPD_O/PWM_2X | same | QSCI0 | sci_rx | Input | XBARA CMPA CMPB CMPC TMR TMR TMR TMR AOI AOI AOI AOI PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PIT0 PIT1 | xBarOut10 Output Output Output TMR_OUT_PIN0 TMR_OUT_PIN1 TMR_OUT_PIN2 TMR_OUT_PIN3 Output0 Output1 Output2 Output3 OutputTrigger00 OutputTrigger10 OutputTrigger01 OutputTrigger11 OutputTrigger02 OutputTrigger12 OutputTrigger03 OutputTrigger13 PIT_OUT_PIN PIT_OUT_PIN | Output | CMPD | Output | Output | PWMA | out_X2 | Input, Output |  |  |
7 | GPIOC3/TA0/CMPA_O/RXD0/CLKIN1 | same | TMR | TMR_IN_PIN0 TMR_OUT_PIN0 | Input, Output | CMPA | Output | Output | QSCI0 | sci_rx | Input | OCCS | ClockInput | Input |  |  |
8 | GPIOC4/TA1/CMPB_O/XB_IN6/EWM_OUT_B | same | TMR | TMR_IN_PIN1 TMR_OUT_PIN1 | Input, Output | CMPB | Output | Output | XBARA AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI DMA DMA DMA DMA ADC ADC DACB DACA CMPA CMPB CMPC CMPD PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA TMR TMR TMR QSCI0 QSCI1 EWM | xBarIn6 InputA0 InputB0 InputC0 InputD0 InputA1 InputB1 InputC1 InputD1 InputA2 InputB2 InputC2 InputD2 InputA3 InputB3 InputC3 InputD3 DMAtrigger0 DMAtrigger1 DMAtrigger2 DMAtrigger3 ADCtriggerA ADCtriggerB DACtrigger DACtrigger WindowSample WindowSample WindowSample WindowSample ExternalControlA0 ExternalControlA1 ExternalControlA2 ExternalControlA3 ExternalSync0 ExternalSync1 ExternalSync2 ExternalSync3 EXT_CLK Fault0 Fault1 Fault2 Fault3 ExternalForce TMR_IN_PIN0 TMR_IN_PIN2 TMR_IN_PIN3 sci_rx sci_rx ewminput | Input | EWM | ewmoutput | Output |  |  |
9 | GPIOA7/ANA7/CMPD_IN3 | same | ADC CMPD CMPD | ADC7 Positive3 Negative3 | Input |  |  |  |  |  |  |  |  |  |  |  |
10 | GPIOA6/ANA6/CMPD_IN2 | same | ADC CMPD CMPD | ADC6 Positive2 Negative2 | Input |  |  |  |  |  |  |  |  |  |  |  |
11 | GPIOA5/ANA5/CMPD_IN1 | same | ADC CMPD CMPD | ADC5 Positive1 Negative1 | Input |  |  |  |  |  |  |  |  |  |  |  |
12 | GPIOA4/ANA4/CMPD_IN0 | same | ADC CMPD CMPD | ADC4 Positive0 Negative0 | Input |  |  |  |  |  |  |  |  |  |  |  |
13 | GPIOA0/ANA0/CMPA_IN3/CMPC_O | same | ADC CMPA CMPA | ADC0 Positive3 Negative3 | Input | CMPC | Output | Output |  |  |  |  |  |  |  |  |
14 | GPIOA1/ANA1/CMPA_IN0 | same | ADC CMPA CMPA | ADC1 Positive0 Negative0 | Input |  |  |  |  |  |  |  |  |  |  |  |
15 | GPIOA2/ANA2/VREFHA/CMPA_IN1 | same | ADC ADC CMPA CMPA | ADC2 ADCvrefVREFHA Positive1 Negative1 | Input |  |  |  |  |  |  |  |  |  |  |  |
16 | GPIOA3/ANA3/VREFLA/CMPA_IN2 | same | ADC ADC CMPA CMPA | ADC3 ADCvrefVREFLA Positive2 Negative2 | Input |  |  |  |  |  |  |  |  |  |  |  |
17 | GPIOB7/ANB7/CMPB_IN2 | same | ADC CMPB CMPB | ADC15 Positive2 Negative2 | Input |  |  |  |  |  |  |  |  |  |  |  |
18 | GPIOC5/DACA_O/XB_IN7 | same | DACA | dacout | Output | XBARA AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI DMA DMA DMA DMA ADC ADC DACB DACA CMPA CMPB CMPC CMPD PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA TMR TMR TMR TMR QSCI0 QSCI1 EWM | xBarIn7 InputA0 InputB0 InputC0 InputD0 InputA1 InputB1 InputC1 InputD1 InputA2 InputB2 InputC2 InputD2 InputA3 InputB3 InputC3 InputD3 DMAtrigger0 DMAtrigger1 DMAtrigger2 DMAtrigger3 ADCtriggerA ADCtriggerB DACtrigger DACtrigger WindowSample WindowSample WindowSample WindowSample ExternalControlA0 ExternalControlA1 ExternalControlA2 ExternalControlA3 ExternalSync0 ExternalSync1 ExternalSync2 ExternalSync3 EXT_CLK Fault0 Fault1 Fault2 Fault3 ExternalForce TMR_IN_PIN0 TMR_IN_PIN1 TMR_IN_PIN2 TMR_IN_PIN3 sci_rx sci_rx ewminput | Input |  |  |  |  |  |  |  |  |
19 | GPIOB6/ANB6/CMPB_IN1 | same | ADC CMPB CMPB | ADC14 Positive1 Negative1 | Input |  |  |  |  |  |  |  |  |  |  |  |
20 | GPIOB5/ANB5/CMPC_IN2 | same | ADC CMPC CMPC | ADC13 Positive2 Negative2 | Input |  |  |  |  |  |  |  |  |  |  |  |
21 | GPIOB4/ANB4/CMPC_IN1 | same | ADC CMPC CMPC | ADC12 Positive1 Negative1 | Input |  |  |  |  |  |  |  |  |  |  |  |
22 | VDDA | same |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
23 | VSSA | same |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
24 | GPIOB0/ANB0/CMPB_IN3 | same | ADC CMPB CMPB | ADC8 Positive3 Negative3 | Input |  |  |  |  |  |  |  |  |  |  |  |
25 | GPIOB1/ANB1/CMPB_IN0/DACB_O | same | ADC CMPB CMPB | ADC9 Positive0 Negative0 | Input | DACB | dacout | Output |  |  |  |  |  |  |  |  |
26 | VCAP_26 | same |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
27 | GPIOB2/ANB2/VREFHB/CMPC_IN3 | same | ADC ADC CMPC CMPC | ADC10 ADCvrefVREFHB Positive3 Negative3 | Input |  |  |  |  |  |  |  |  |  |  |  |
28 | GPIOB3/ANB3/VREFLB/CMPC_IN0 | same | ADC ADC CMPC CMPC | ADC11 ADCvrefVREFLB Positive0 Negative0 | Input |  |  |  |  |  |  |  |  |  |  |  |
29 | VDD_29 | same |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
30 | VSS_30 | same |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
31 | GPIOC6/TA2/XB_IN3/CMP_REF/SS0_B | same | TMR | TMR_IN_PIN2 TMR_OUT_PIN2 | Input, Output | XBARA AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI DMA DMA DMA DMA ADC ADC DACB DACA CMPA CMPB CMPC CMPD PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA TMR TMR TMR QSCI0 QSCI1 EWM | xBarIn3 InputA0 InputB0 InputC0 InputD0 InputA1 InputB1 InputC1 InputD1 InputA2 InputB2 InputC2 InputD2 InputA3 InputB3 InputC3 InputD3 DMAtrigger0 DMAtrigger1 DMAtrigger2 DMAtrigger3 ADCtriggerA ADCtriggerB DACtrigger DACtrigger WindowSample WindowSample WindowSample WindowSample ExternalControlA0 ExternalControlA1 ExternalControlA2 ExternalControlA3 ExternalSync0 ExternalSync1 ExternalSync2 ExternalSync3 EXT_CLK Fault0 Fault1 Fault2 Fault3 ExternalForce TMR_IN_PIN0 TMR_IN_PIN1 TMR_IN_PIN3 sci_rx sci_rx ewminput | Input | CMPA CMPB CMPC CMPD CMPA CMPB CMPC CMPD | Positive5 Positive5 Positive5 Positive5 Negative5 Negative5 Negative5 Negative5 | Input | QSPI0 | spi_ss | Input, Output |  |  |
32 | GPIOC7/SS0_B/TXD0/XB_IN8 | same | QSPI0 | spi_ss | Input, Output | QSCI0 | sci_tx | Output | XBARA AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI DMA DMA DMA DMA ADC ADC DACB DACA CMPA CMPB CMPC CMPD PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA TMR TMR TMR TMR QSCI0 QSCI1 EWM | xBarIn8 InputA0 InputB0 InputC0 InputD0 InputA1 InputB1 InputC1 InputD1 InputA2 InputB2 InputC2 InputD2 InputA3 InputB3 InputC3 InputD3 DMAtrigger0 DMAtrigger1 DMAtrigger2 DMAtrigger3 ADCtriggerA ADCtriggerB DACtrigger DACtrigger WindowSample WindowSample WindowSample WindowSample ExternalControlA0 ExternalControlA1 ExternalControlA2 ExternalControlA3 ExternalSync0 ExternalSync1 ExternalSync2 ExternalSync3 EXT_CLK Fault0 Fault1 Fault2 Fault3 ExternalForce TMR_IN_PIN0 TMR_IN_PIN1 TMR_IN_PIN2 TMR_IN_PIN3 sci_rx sci_rx ewminput | Input |  |  |  |  |  |
33 | GPIOC8/MISO0/RXD0/XB_IN9/XB_OUT6 | same | QSPI0 | spi_miso | Input, Output | QSCI0 | sci_rx | Input | XBARA AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI DMA DMA DMA DMA ADC ADC DACB DACA CMPA CMPB CMPC CMPD PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA TMR TMR TMR TMR QSCI1 EWM | xBarIn9 InputA0 InputB0 InputC0 InputD0 InputA1 InputB1 InputC1 InputD1 InputA2 InputB2 InputC2 InputD2 InputA3 InputB3 InputC3 InputD3 DMAtrigger0 DMAtrigger1 DMAtrigger2 DMAtrigger3 ADCtriggerA ADCtriggerB DACtrigger DACtrigger WindowSample WindowSample WindowSample WindowSample ExternalControlA0 ExternalControlA1 ExternalControlA2 ExternalControlA3 ExternalSync0 ExternalSync1 ExternalSync2 ExternalSync3 EXT_CLK Fault0 Fault1 Fault2 Fault3 ExternalForce TMR_IN_PIN0 TMR_IN_PIN1 TMR_IN_PIN2 TMR_IN_PIN3 sci_rx ewminput | Input | XBARA CMPA CMPB CMPC CMPD TMR TMR TMR TMR AOI AOI AOI AOI PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PIT0 PIT1 | xBarOut6 Output Output Output Output TMR_OUT_PIN0 TMR_OUT_PIN1 TMR_OUT_PIN2 TMR_OUT_PIN3 Output0 Output1 Output2 Output3 OutputTrigger00 OutputTrigger10 OutputTrigger01 OutputTrigger11 OutputTrigger02 OutputTrigger12 OutputTrigger03 OutputTrigger13 PIT_OUT_PIN PIT_OUT_PIN | Output |  |  |
34 | GPIOC9/SCK0/XB_IN4/TXD0/XB_OUT8 | same | QSPI0 | spi_sck | Input, Output | XBARA AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI DMA DMA DMA DMA ADC ADC DACB DACA CMPA CMPB CMPC CMPD PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA TMR TMR TMR TMR QSCI0 QSCI1 EWM | xBarIn4 InputA0 InputB0 InputC0 InputD0 InputA1 InputB1 InputC1 InputD1 InputA2 InputB2 InputC2 InputD2 InputA3 InputB3 InputC3 InputD3 DMAtrigger0 DMAtrigger1 DMAtrigger2 DMAtrigger3 ADCtriggerA ADCtriggerB DACtrigger DACtrigger WindowSample WindowSample WindowSample WindowSample ExternalControlA0 ExternalControlA1 ExternalControlA2 ExternalControlA3 ExternalSync0 ExternalSync1 ExternalSync2 ExternalSync3 EXT_CLK Fault0 Fault1 Fault2 Fault3 ExternalForce TMR_IN_PIN0 TMR_IN_PIN1 TMR_IN_PIN2 TMR_IN_PIN3 sci_rx sci_rx ewminput | Input | QSCI0 | sci_tx | Output | XBARA CMPA CMPB CMPC CMPD TMR TMR TMR TMR AOI AOI AOI AOI PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PIT0 PIT1 | xBarOut8 Output Output Output Output TMR_OUT_PIN0 TMR_OUT_PIN1 TMR_OUT_PIN2 TMR_OUT_PIN3 Output0 Output1 Output2 Output3 OutputTrigger00 OutputTrigger10 OutputTrigger01 OutputTrigger11 OutputTrigger02 OutputTrigger12 OutputTrigger03 OutputTrigger13 PIT_OUT_PIN PIT_OUT_PIN | Output |  |  |
35 | GPIOC10/MOSI0/XB_IN5/MISO0/XB_OUT9 | same | QSPI0 | spi_mosi | Input, Output | XBARA AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI DMA DMA DMA DMA ADC ADC DACB DACA CMPA CMPB CMPC CMPD PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA TMR TMR TMR TMR QSCI0 QSCI1 EWM | xBarIn5 InputA0 InputB0 InputC0 InputD0 InputA1 InputB1 InputC1 InputD1 InputA2 InputB2 InputC2 InputD2 InputA3 InputB3 InputC3 InputD3 DMAtrigger0 DMAtrigger1 DMAtrigger2 DMAtrigger3 ADCtriggerA ADCtriggerB DACtrigger DACtrigger WindowSample WindowSample WindowSample WindowSample ExternalControlA0 ExternalControlA1 ExternalControlA2 ExternalControlA3 ExternalSync0 ExternalSync1 ExternalSync2 ExternalSync3 EXT_CLK Fault0 Fault1 Fault2 Fault3 ExternalForce TMR_IN_PIN0 TMR_IN_PIN1 TMR_IN_PIN2 TMR_IN_PIN3 sci_rx sci_rx ewminput | Input | QSPI0 | spi_miso | Input, Output | XBARA CMPA CMPB CMPC CMPD TMR TMR TMR TMR AOI AOI AOI AOI PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PIT0 PIT1 | xBarOut9 Output Output Output Output TMR_OUT_PIN0 TMR_OUT_PIN1 TMR_OUT_PIN2 TMR_OUT_PIN3 Output0 Output1 Output2 Output3 OutputTrigger00 OutputTrigger10 OutputTrigger01 OutputTrigger11 OutputTrigger02 OutputTrigger12 OutputTrigger03 OutputTrigger13 PIT_OUT_PIN PIT_OUT_PIN | Output |  |  |
36 | GPIOF0/XB_IN6/SCK1 | same | XBARA AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI DMA DMA DMA DMA ADC ADC DACB DACA CMPA CMPB CMPC CMPD PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA TMR TMR TMR TMR QSCI0 QSCI1 EWM | xBarIn6 InputA0 InputB0 InputC0 InputD0 InputA1 InputB1 InputC1 InputD1 InputA2 InputB2 InputC2 InputD2 InputA3 InputB3 InputC3 InputD3 DMAtrigger0 DMAtrigger1 DMAtrigger2 DMAtrigger3 ADCtriggerA ADCtriggerB DACtrigger DACtrigger WindowSample WindowSample WindowSample WindowSample ExternalControlA0 ExternalControlA1 ExternalControlA2 ExternalControlA3 ExternalSync0 ExternalSync1 ExternalSync2 ExternalSync3 EXT_CLK Fault0 Fault1 Fault2 Fault3 ExternalForce TMR_IN_PIN0 TMR_IN_PIN1 TMR_IN_PIN2 TMR_IN_PIN3 sci_rx sci_rx ewminput | Input |  |  |  | QSPI1 | spi_sck | Input, Output |  |  |  |  |  |
37 | GPIOC11/CANTX/SCL0/TXD1 | same | CAN | can_txd | Output | I2C | i2c_sclk | Input/Output | QSCI1 | sci_tx | Output |  |  |  |  |  |
38 | GPIOC12/CANRX/SDA0/RXD1 | same | CAN | can_rxd | Input | I2C | i2c_sda | Input/Output | QSCI1 | sci_rx | Input |  |  |  |  |  |
39 | GPIOF2/SCL0/XB_OUT6/MISO1 | same | I2C | i2c_sclk | Input/Output | XBARA CMPA CMPB CMPC CMPD TMR TMR TMR TMR AOI AOI AOI AOI PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PIT0 PIT1 | xBarOut6 Output Output Output Output TMR_OUT_PIN0 TMR_OUT_PIN1 TMR_OUT_PIN2 TMR_OUT_PIN3 Output0 Output1 Output2 Output3 OutputTrigger00 OutputTrigger10 OutputTrigger01 OutputTrigger11 OutputTrigger02 OutputTrigger12 OutputTrigger03 OutputTrigger13 PIT_OUT_PIN PIT_OUT_PIN | Output | QSPI1 | spi_miso | Input, Output |  |  |  |  |  |
40 | GPIOF3/SDA0/XB_OUT7/MOSI1 | same | I2C | i2c_sda | Input/Output | XBARA CMPA CMPB CMPC CMPD TMR TMR TMR TMR AOI AOI AOI AOI PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PIT0 PIT1 | xBarOut7 Output Output Output Output TMR_OUT_PIN0 TMR_OUT_PIN1 TMR_OUT_PIN2 TMR_OUT_PIN3 Output0 Output1 Output2 Output3 OutputTrigger00 OutputTrigger10 OutputTrigger01 OutputTrigger11 OutputTrigger02 OutputTrigger12 OutputTrigger03 OutputTrigger13 PIT_OUT_PIN PIT_OUT_PIN | Output | QSPI1 | spi_mosi | Input, Output |  |  |  |  |  |
41 | GPIOF4/TXD1/XB_OUT8/PWM_0X/PWM_FAULT6 | same | QSCI1 | sci_tx | Output | XBARA CMPA CMPB CMPC CMPD TMR TMR TMR TMR AOI AOI AOI AOI PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PIT0 PIT1 | xBarOut8 Output Output Output Output TMR_OUT_PIN0 TMR_OUT_PIN1 TMR_OUT_PIN2 TMR_OUT_PIN3 Output0 Output1 Output2 Output3 OutputTrigger00 OutputTrigger10 OutputTrigger01 OutputTrigger11 OutputTrigger02 OutputTrigger12 OutputTrigger03 OutputTrigger13 PIT_OUT_PIN PIT_OUT_PIN | Output | PWMA | out_X0 | Input, Output | PWMA | Fault6 | Input |  |  |
42 | GPIOF5/RXD1/XB_OUT9/PWM_1X/PWM_FAULT7 | same | QSCI1 | sci_rx | Input | XBARA CMPA CMPB CMPC CMPD TMR TMR TMR TMR AOI AOI AOI AOI PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PIT0 PIT1 | xBarOut9 Output Output Output Output TMR_OUT_PIN0 TMR_OUT_PIN1 TMR_OUT_PIN2 TMR_OUT_PIN3 Output0 Output1 Output2 Output3 OutputTrigger00 OutputTrigger10 OutputTrigger01 OutputTrigger11 OutputTrigger02 OutputTrigger12 OutputTrigger03 OutputTrigger13 PIT_OUT_PIN PIT_OUT_PIN | Output | PWMA | out_X1 | Input, Output | PWMA | Fault7 | Input |  |  |
43 | VSS_43 | same |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
44 | VDD_44 | same |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
45 | GPIOE0/PWM_0B | same | PWMA | out_B0 | Input, Output |  |  |  |  |  |  |  |  |  |  |  |
46 | GPIOE1/PWM_0A | same | PWMA | out_A0 | Input, Output |  |  |  |  |  |  |  |  |  |  |  |
47 | GPIOE2/PWM_1B | same | PWMA | out_B1 | Input, Output |  |  |  |  |  |  |  |  |  |  |  |
48 | GPIOE3/PWM_1A | same | PWMA | out_A1 | Input, Output |  |  |  |  |  |  |  |  |  |  |  |
49 | GPIOC13/TA3/XB_IN6/EWM_OUT_B | same | TMR | TMR_IN_PIN3 TMR_OUT_PIN3 | Input, Output | XBARA AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI DMA DMA DMA DMA ADC ADC DACB DACA CMPA CMPB CMPC CMPD PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA TMR TMR TMR QSCI0 QSCI1 EWM | xBarIn6 InputA0 InputB0 InputC0 InputD0 InputA1 InputB1 InputC1 InputD1 InputA2 InputB2 InputC2 InputD2 InputA3 InputB3 InputC3 InputD3 DMAtrigger0 DMAtrigger1 DMAtrigger2 DMAtrigger3 ADCtriggerA ADCtriggerB DACtrigger DACtrigger WindowSample WindowSample WindowSample WindowSample ExternalControlA0 ExternalControlA1 ExternalControlA2 ExternalControlA3 ExternalSync0 ExternalSync1 ExternalSync2 ExternalSync3 EXT_CLK Fault0 Fault1 Fault2 Fault3 ExternalForce TMR_IN_PIN0 TMR_IN_PIN1 TMR_IN_PIN2 sci_rx sci_rx ewminput | Input | EWM | ewmoutput | Output |  |  |  |  |  |
50 | GPIOF1/CLKO1/XB_IN7/CMPD_O | same | SIM | ClockOutput1 | Output | XBARA AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI DMA DMA DMA DMA ADC ADC DACB DACA CMPA CMPB CMPC CMPD PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA TMR TMR TMR TMR QSCI0 QSCI1 EWM | xBarIn7 InputA0 InputB0 InputC0 InputD0 InputA1 InputB1 InputC1 InputD1 InputA2 InputB2 InputC2 InputD2 InputA3 InputB3 InputC3 InputD3 DMAtrigger0 DMAtrigger1 DMAtrigger2 DMAtrigger3 ADCtriggerA ADCtriggerB DACtrigger DACtrigger WindowSample WindowSample WindowSample WindowSample ExternalControlA0 ExternalControlA1 ExternalControlA2 ExternalControlA3 ExternalSync0 ExternalSync1 ExternalSync2 ExternalSync3 EXT_CLK Fault0 Fault1 Fault2 Fault3 ExternalForce TMR_IN_PIN0 TMR_IN_PIN1 TMR_IN_PIN2 TMR_IN_PIN3 sci_rx sci_rx ewminput | Input | CMPD | Output | Output |  |  |  |  |  |
51 | GPIOE4/PWM_2B/XB_IN2 | same | PWMA | out_B2 | Input, Output | XBARA AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI DMA DMA DMA DMA ADC ADC DACB DACA CMPA CMPB CMPC CMPD PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA TMR TMR TMR TMR QSCI0 QSCI1 EWM | xBarIn2 InputA0 InputB0 InputC0 InputD0 InputA1 InputB1 InputC1 InputD1 InputA2 InputB2 InputC2 InputD2 InputA3 InputB3 InputC3 InputD3 DMAtrigger0 DMAtrigger1 DMAtrigger2 DMAtrigger3 ADCtriggerA ADCtriggerB DACtrigger DACtrigger WindowSample WindowSample WindowSample WindowSample ExternalControlA0 ExternalControlA1 ExternalControlA2 ExternalControlA3 ExternalSync0 ExternalSync1 ExternalSync2 ExternalSync3 EXT_CLK Fault0 Fault1 Fault2 Fault3 ExternalForce TMR_IN_PIN0 TMR_IN_PIN1 TMR_IN_PIN2 TMR_IN_PIN3 sci_rx sci_rx ewminput | Input |  |  |  |  |  |  |  |  |
52 | GPIOE5/PWM_2A/XB_IN3 | same | PWMA | out_A2 | Input, Output | XBARA AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI DMA DMA DMA DMA ADC ADC DACB DACA CMPA CMPB CMPC CMPD PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA TMR TMR TMR TMR QSCI0 QSCI1 EWM | xBarIn3 InputA0 InputB0 InputC0 InputD0 InputA1 InputB1 InputC1 InputD1 InputA2 InputB2 InputC2 InputD2 InputA3 InputB3 InputC3 InputD3 DMAtrigger0 DMAtrigger1 DMAtrigger2 DMAtrigger3 ADCtriggerA ADCtriggerB DACtrigger DACtrigger WindowSample WindowSample WindowSample WindowSample ExternalControlA0 ExternalControlA1 ExternalControlA2 ExternalControlA3 ExternalSync0 ExternalSync1 ExternalSync2 ExternalSync3 EXT_CLK Fault0 Fault1 Fault2 Fault3 ExternalForce TMR_IN_PIN0 TMR_IN_PIN1 TMR_IN_PIN2 TMR_IN_PIN3 sci_rx sci_rx ewminput | Input |  |  |  |  |  |  |  |  |
53 | GPIOE6/PWM_3B/XB_IN4 | same | PWMA | out_B3 | Input, Output | XBARA AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI DMA DMA DMA DMA ADC ADC DACB DACA CMPA CMPB CMPC CMPD PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA TMR TMR TMR TMR QSCI0 QSCI1 EWM | xBarIn4 InputA0 InputB0 InputC0 InputD0 InputA1 InputB1 InputC1 InputD1 InputA2 InputB2 InputC2 InputD2 InputA3 InputB3 InputC3 InputD3 DMAtrigger0 DMAtrigger1 DMAtrigger2 DMAtrigger3 ADCtriggerA ADCtriggerB DACtrigger DACtrigger WindowSample WindowSample WindowSample WindowSample ExternalControlA0 ExternalControlA1 ExternalControlA2 ExternalControlA3 ExternalSync0 ExternalSync1 ExternalSync2 ExternalSync3 EXT_CLK Fault0 Fault1 Fault2 Fault3 ExternalForce TMR_IN_PIN0 TMR_IN_PIN1 TMR_IN_PIN2 TMR_IN_PIN3 sci_rx sci_rx ewminput | Input |  |  |  |  |  |  |  |  |
54 | GPIOE7/PWM_3A/XB_IN5 | same | PWMA | out_A3 | Input, Output | XBARA AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI DMA DMA DMA DMA ADC ADC DACB DACA CMPA CMPB CMPC CMPD PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA TMR TMR TMR TMR QSCI0 QSCI1 EWM | xBarIn5 InputA0 InputB0 InputC0 InputD0 InputA1 InputB1 InputC1 InputD1 InputA2 InputB2 InputC2 InputD2 InputA3 InputB3 InputC3 InputD3 DMAtrigger0 DMAtrigger1 DMAtrigger2 DMAtrigger3 ADCtriggerA ADCtriggerB DACtrigger DACtrigger WindowSample WindowSample WindowSample WindowSample ExternalControlA0 ExternalControlA1 ExternalControlA2 ExternalControlA3 ExternalSync0 ExternalSync1 ExternalSync2 ExternalSync3 EXT_CLK Fault0 Fault1 Fault2 Fault3 ExternalForce TMR_IN_PIN0 TMR_IN_PIN1 TMR_IN_PIN2 TMR_IN_PIN3 sci_rx sci_rx ewminput | Input |  |  |  |  |  |  |  |  |
55 | GPIOC14/SDA0/XB_OUT4/PWM_FAULT4 | same | I2C | i2c_sda | Input/Output | XBARA CMPA CMPB CMPC CMPD TMR TMR TMR TMR AOI AOI AOI AOI PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PIT0 PIT1 | xBarOut4 Output Output Output Output TMR_OUT_PIN0 TMR_OUT_PIN1 TMR_OUT_PIN2 TMR_OUT_PIN3 Output0 Output1 Output2 Output3 OutputTrigger00 OutputTrigger10 OutputTrigger01 OutputTrigger11 OutputTrigger02 OutputTrigger12 OutputTrigger03 OutputTrigger13 PIT_OUT_PIN PIT_OUT_PIN | Output | PWMA | Fault4 | Input |  |  |  |  |  |
56 | GPIOC15/SCL0/XB_OUT5/PWM_FAULT5 | same | I2C | i2c_sclk | Input/Output | XBARA CMPA CMPB CMPC CMPD TMR TMR TMR TMR AOI AOI AOI AOI PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PIT0 PIT1 | xBarOut5 Output Output Output Output TMR_OUT_PIN0 TMR_OUT_PIN1 TMR_OUT_PIN2 TMR_OUT_PIN3 Output0 Output1 Output2 Output3 OutputTrigger00 OutputTrigger10 OutputTrigger01 OutputTrigger11 OutputTrigger02 OutputTrigger12 OutputTrigger03 OutputTrigger13 PIT_OUT_PIN PIT_OUT_PIN | Output | PWMA | Fault5 | Input |  |  |  |  |  |
57 | VCAP_57 | same |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
58 | GPIOF6/PWM_3X/XB_IN2 | same |  |  |  | PWMA | out_X3 | Input, Output |  |  |  | XBARA AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI DMA DMA DMA DMA ADC ADC DACB DACA CMPA CMPB CMPC CMPD PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA TMR TMR TMR TMR QSCI0 QSCI1 EWM | xBarIn2 InputA0 InputB0 InputC0 InputD0 InputA1 InputB1 InputC1 InputD1 InputA2 InputB2 InputC2 InputD2 InputA3 InputB3 InputC3 InputD3 DMAtrigger0 DMAtrigger1 DMAtrigger2 DMAtrigger3 ADCtriggerA ADCtriggerB DACtrigger DACtrigger WindowSample WindowSample WindowSample WindowSample ExternalControlA0 ExternalControlA1 ExternalControlA2 ExternalControlA3 ExternalSync0 ExternalSync1 ExternalSync2 ExternalSync3 EXT_CLK Fault0 Fault1 Fault2 Fault3 ExternalForce TMR_IN_PIN0 TMR_IN_PIN1 TMR_IN_PIN2 TMR_IN_PIN3 sci_rx sci_rx ewminput | Input |  |  |
59 | GPIOF7/CMPC_O/SS1_B/XB_IN3 | same |  |  |  | CMPC | Output | Output | QSPI1 | spi_ss | Input, Output | XBARA AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI AOI DMA DMA DMA DMA ADC ADC DACB DACA CMPA CMPB CMPC CMPD PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA PWMA TMR TMR TMR TMR QSCI0 QSCI1 EWM | xBarIn3 InputA0 InputB0 InputC0 InputD0 InputA1 InputB1 InputC1 InputD1 InputA2 InputB2 InputC2 InputD2 InputA3 InputB3 InputC3 InputD3 DMAtrigger0 DMAtrigger1 DMAtrigger2 DMAtrigger3 ADCtriggerA ADCtriggerB DACtrigger DACtrigger WindowSample WindowSample WindowSample WindowSample ExternalControlA0 ExternalControlA1 ExternalControlA2 ExternalControlA3 ExternalSync0 ExternalSync1 ExternalSync2 ExternalSync3 EXT_CLK Fault0 Fault1 Fault2 Fault3 ExternalForce TMR_IN_PIN0 TMR_IN_PIN1 TMR_IN_PIN2 TMR_IN_PIN3 sci_rx sci_rx ewminput | Input |  |  |
60 | VDD_60 | same |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
61 | VSS_61 | same |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
62 | TDO/GPIOD1 | same | EONCE | TDO | Output |  |  |  |  |  |  |  |  |  |  |  |
63 | TMS/GPIOD3 | same | EONCE | TMS | Input |  |  |  |  |  |  |  |  |  |  |  |
64 | TDI/GPIOD0 | same | EONCE | TDI | Input |  |  |  |  |  |  |  |  |  |  |  |