<?xml version="1.0" encoding="UTF-8"?>
<PE_PROJECT_SETTINGS_DOCUMENTATION>
  <PE_product_version v="version 10.3 for Freescale Microcontrollers" />
  <PE_core_version v="Processor Expert Version 0509" />
  <CPU_Bean name="Cpu" type="MC56F82748VLH">
    <Enabled v="Y" />
    <Properties>
      <Component_name v="Cpu" />
      <CPU_type v="MC56F82748VLH" />
      <list name="Clock settings (included)" v="1">
        <group name="Clock settings (OCCS)">
          <group name="Internal oscillator">
            <boolgroup name="Internal 200kHz relaxation oscillator (ROSC_200K)" v="Disabled" />
            <boolgroup name="Internal 8MHz relaxation oscillator (ROSC_8M)" v="Enabled">
              <Fast_internal_reference_clock__MHz_ v="8" />
              <boolgroup name="Initialize frequency trim" v="yes">
                <Frequency_trim_value_address v="58412" />
              </boolgroup>
              <boolgroup name="Initialize temperature trim" v="no" />
            </boolgroup>
          </group>
          <boolgroup name="External reference clock" v="Disabled" />
          <group name="Clock protection">
            <Frequency v="Off" />
            <Oscillator v="Off" />
            <Phase_locked_loop v="Off" />
          </group>
          <Dual_speed_clock v="Fast mode" />
          <list name="Clock configurations" v="1">
            <group name="Clock configuration 0">
              <Input_clock_source_ v="Internal oscillator 8MHz" />
              <Clock_output_divider__Postscaler_ v="Auto select" />
              <Bus_clock__IP_Bus___MHz_ v="50" />
              <Core_clock__MHz_ v="100" />
              <System_clock__MHz_ v="100" />
              <boolgroup name="PLL clock" v="Enabled">
                <PLL_multiplier v="Auto select" />
                <PLL_clock v="400" />
                <Enable_PLL_after_reset v="yes" />
                <Number_of_lock_checks v="1" />
                <group name="PWM clock source">
                  <PWM_nano_edge v="PLL" />
                  <PWM_nano_edge_clock__MHz_ v="400" />
                </group>
              </boolgroup>
              <group name="Peripheral clock rates">
                <QSCI0_clock_rate v="&amp;lt;Automatic&amp;gt;" />
                <QSCI1_clock_rate v="&amp;lt;Automatic&amp;gt;" />
                <TMR_clock_rate v="&amp;lt;Automatic&amp;gt;" />
                <PWM_clock_rate v="&amp;lt;Automatic&amp;gt;" />
                <I2C_filter_clock_rate v="&amp;lt;Automatic&amp;gt;" />
              </group>
            </group>
          </list>
        </group>
      </list>
      <list name="Common settings (included)" v="1">
        <group name="Common settings">
          <Initialization_priority v="minimal priority" />
          <Watchdog v="Disabled" />
          <Saturation_mode v="Disabled" />
          <Utilize_after_reset_values v="default" />
          <list name="Shared Reset settings" v="1">
            <boolgroup name="Reset pin" v="Enabled">
              <Reset_Pin v="RESETB/VPP/GPIOD4" />
            </boolgroup>
          </list>
          <list name="Shared JTAG pins setiings" v="1">
            <group name="JTAG pins">
              <boolgroup name="TDI" v="Enabled">
                <TDI_Pin v="TDI/GPIOD0" />
              </boolgroup>
              <boolgroup name="TDO" v="Enabled">
                <TDO_Pin v="TDO/GPIOD1" />
              </boolgroup>
              <boolgroup name="TCK" v="Enabled">
                <TCK_Pin v="TCK/GPIOD2" />
              </boolgroup>
              <boolgroup name="TMS" v="Enabled">
                <TMS_Pin v="TMS/GPIOD3" />
              </boolgroup>
            </group>
          </list>
          <list name="Initialize unused I/O pins (included)" v="1">
            <enumgroup name="Initialize unused I/O pins" v="No initialization">
              <Pull_resistor v="No initialization" />
              <Open_drain v="No initialization" />
              <Output_value v="No initialization" />
              <Include_Reset_pin v="no" />
              <Include_JTAG_pins v="no" />
            </enumgroup>
          </list>
          <list name="Initialize shadow registers (included)" v="1">
            <boolgroup name="Initialize shadow registers" v="yes">
              <R0 v="0" />
              <R1 v="0" />
              <R2 v="0" />
              <R3 v="0" />
              <R4 v="0" />
              <R5 v="0" />
              <N v="0" />
              <N3 v="65535" />
              <M01 v="65535" />
            </boolgroup>
          </list>
          <boolgroup name="Initialize bandgap trim value" v="yes">
            <Trim_value_address v="58413" />
          </boolgroup>
          <list name="Memory resource protection (include)" v="1">
            <enumgroup name="Memory resource protection" v="Disabled">
              <EmptySection_DummyValue />
            </enumgroup>
          </list>
          <list name="Flash config settings (included)" v="1">
            <boolgroup name="Flash configuration field" v="Disabled" />
          </list>
          <list name="Flash memory organization (included)" v="1">
            <group name="Flash memory organization">
              <list name="Shared FLASH settings" v="1">
                <EmptySection_DummyValue />
              </list>
              <list name="Flash blocks" v="1">
                <group name="Flash block 0">
                  <Address v="0" />
                  <Size v="32768" />
                  <Write_unit_size v="2" />
                  <Erase_unit_size v="512" />
                  <Protection_unit_size v="1024" />
                </group>
              </list>
            </group>
          </list>
        </group>
      </list>
      <group name="CPU interrupts">
        <boolgroup name="Interrupt SW0" v="Disabled" />
        <boolgroup name="Interrupt SW1" v="Disabled" />
        <boolgroup name="Interrupt SW2" v="Disabled" />
        <boolgroup name="Interrupt SW3" v="Disabled" />
        <boolgroup name="Interrupt LP" v="Disabled" />
        <boolgroup name="Interrupt PLL" v="Disabled" />
        <boolgroup name="Interrupt Illegal Instruction" v="Disabled" />
        <boolgroup name="Interrupt Misalign Access" v="Disabled" />
        <boolgroup name="Interrupt HW Stack Overflow" v="Disabled" />
      </group>
    </Properties>
    <Methods>
      <list name="CPUCond0" v="1">
        <SetClockConfiguration v="don&amp;apos;t generate code" />
        <GetClockConfiguration v="don&amp;apos;t generate code" />
        <SetOperationMode v="don&amp;apos;t generate code" />
        <EnableInt v="generate code" />
        <DisableInt v="generate code" />
        <GetResetSource v="don&amp;apos;t generate code" />
        <SetWaitMode v="generate code" />
        <SetStopMode v="generate code" />
        <GetBusFreqHz v="don&amp;apos;t generate code" />
        <OpenBackDoor v="don&amp;apos;t generate code" />
        <SetFlexRAMFunction v="don&amp;apos;t generate code" />
        <SetFlexNVMPartition v="don&amp;apos;t generate code" />
        <InitShadowRegs v="don&amp;apos;t generate code" />
        <Delay100US v="don&amp;apos;t generate code" />
        <EnablePLL v="don&amp;apos;t generate code" />
      </list>
    </Methods>
    <Events>
      <Event_module_name v="Events" />
      <list name="CPUCond" v="1">
        <event name="OnReset" v="don&amp;apos;t generate code" />
        <event name="OnSwINT0" v="don&amp;apos;t generate code" />
        <event name="OnSwINT1" v="don&amp;apos;t generate code" />
        <event name="OnSwINT2" v="don&amp;apos;t generate code" />
        <event name="OnSwINT3" v="don&amp;apos;t generate code" />
        <event name="OnSwINTLP" v="don&amp;apos;t generate code" />
        <event name="OnPLLError" v="don&amp;apos;t generate code" />
        <event name="OnIllegalOpcode" v="don&amp;apos;t generate code" />
        <event name="OnMisalignData" v="don&amp;apos;t generate code" />
        <event name="OnHWStackError" v="don&amp;apos;t generate code" />
      </list>
    </Events>
    <Compiler v="CodeWarrior DSP C Compiler" />
    <CompilerProperties>
      <Compiler v="CodeWarrior DSP C Compiler" />
      <Unhandled_interrupts v="One handler for all" />
      <boolgroup name="Generate debugger files" v="yes">
        <Generate_mem_file v="yes" />
      </boolgroup>
      <boolgroup name="Generate linker file" v="no" />
      <list name="System paths " v="0">
        <EmptySection_DummyValue />
      </list>
      <list name="User paths " v="0">
        <EmptySection_DummyValue />
      </list>
      <list name="Libraries" v="0">
        <EmptySection_DummyValue />
      </list>
      <list name="User directories" v="0">
        <EmptySection_DummyValue />
      </list>
    </CompilerProperties>
  </CPU_Bean>
  <CPU_Bean name="Cpu" type="MC56F82748VLH">
    <Enabled v="N" />
    <Properties>
      <Component_name v="Cpu" />
      <CPU_type v="MC56F82748VLH" />
      <list name="Clock settings (included)" v="1">
        <group name="Clock settings (OCCS)">
          <group name="Internal oscillator">
            <boolgroup name="Internal 200kHz relaxation oscillator (ROSC_200K)" v="Disabled" />
            <boolgroup name="Internal 8MHz relaxation oscillator (ROSC_8M)" v="Enabled">
              <Fast_internal_reference_clock__MHz_ v="8" />
              <boolgroup name="Initialize frequency trim" v="yes">
                <Frequency_trim_value_address v="58412" />
              </boolgroup>
              <boolgroup name="Initialize temperature trim" v="no" />
            </boolgroup>
          </group>
          <boolgroup name="External reference clock" v="Disabled" />
          <group name="Clock protection">
            <Frequency v="Off" />
            <Oscillator v="Off" />
            <Phase_locked_loop v="Off" />
          </group>
          <Dual_speed_clock v="Normal mode" />
          <list name="Clock configurations" v="1">
            <group name="Clock configuration 0">
              <Input_clock_source_ v="Internal oscillator 8MHz" />
              <Clock_output_divider__Postscaler_ v="Auto select" />
              <Bus_clock__IP_Bus___MHz_ v="50" />
              <Core_clock__MHz_ v="50" />
              <System_clock__MHz_ v="50" />
              <boolgroup name="PLL clock" v="Enabled">
                <PLL_multiplier v="Auto select" />
                <PLL_clock v="400" />
                <Enable_PLL_after_reset v="yes" />
                <Number_of_lock_checks v="1" />
              </boolgroup>
              <group name="Peripheral clock rates">
                <QSCI0_clock_rate v="Auto select" />
                <QSCI1_clock_rate v="Auto select" />
                <TMR_clock_rate v="Auto select" />
                <PWM_clock_rate v="Auto select" />
                <I2C_filter_clock_rate v="&amp;lt;Automatic&amp;gt;" />
              </group>
            </group>
          </list>
        </group>
      </list>
      <list name="Common settings (included)" v="1">
        <group name="Common settings">
          <Initialization_priority v="minimal priority" />
          <Watchdog v="No initialization" />
          <Saturation_mode v="Disabled" />
          <Utilize_after_reset_values v="default" />
          <list name="Shared Reset settings" v="1">
            <boolgroup name="Reset pin" v="Enabled">
              <Reset_Pin v="RESETB/VPP/GPIOD4" />
            </boolgroup>
          </list>
          <list name="Shared JTAG pins setiings" v="1">
            <group name="JTAG pins">
              <boolgroup name="TDI" v="Enabled">
                <TDI_Pin v="TDI/GPIOD0" />
              </boolgroup>
              <boolgroup name="TDO" v="Enabled">
                <TDO_Pin v="TDO/GPIOD1" />
              </boolgroup>
              <boolgroup name="TCK" v="Enabled">
                <TCK_Pin v="TCK/GPIOD2" />
              </boolgroup>
              <boolgroup name="TMS" v="Enabled">
                <TMS_Pin v="TMS/GPIOD3" />
              </boolgroup>
            </group>
          </list>
          <list name="Initialize unused I/O pins (included)" v="1">
            <enumgroup name="Initialize unused I/O pins" v="No initialization">
              <Pull_resistor v="No initialization" />
              <Open_drain v="No initialization" />
              <Output_value v="No initialization" />
              <Include_Reset_pin v="no" />
              <Include_JTAG_pins v="no" />
            </enumgroup>
          </list>
          <list name="Initialize shadow registers (included)" v="1">
            <boolgroup name="Initialize shadow registers" v="yes">
              <R0 v="0" />
              <R1 v="0" />
              <R2 v="0" />
              <R3 v="0" />
              <R4 v="0" />
              <R5 v="0" />
              <N v="0" />
              <N3 v="65535" />
              <M01 v="65535" />
            </boolgroup>
          </list>
          <boolgroup name="Initialize bandgap trim value" v="yes">
            <Trim_value_address v="58413" />
          </boolgroup>
          <list name="Memory resource protection (include)" v="1">
            <enumgroup name="Memory resource protection" v="Disabled">
              <EmptySection_DummyValue />
            </enumgroup>
          </list>
          <list name="Flash config settings (included)" v="1">
            <boolgroup name="Flash configuration field" v="Disabled" />
          </list>
          <list name="Flash memory organization (included)" v="1">
            <group name="Flash memory organization">
              <list name="Shared FLASH settings" v="1">
                <EmptySection_DummyValue />
              </list>
              <list name="Flash blocks" v="1">
                <group name="Flash block 0">
                  <Address v="0" />
                  <Size v="32768" />
                  <Write_unit_size v="2" />
                  <Erase_unit_size v="512" />
                  <Protection_unit_size v="1024" />
                </group>
              </list>
            </group>
          </list>
        </group>
      </list>
      <group name="CPU interrupts">
        <boolgroup name="Interrupt SW0" v="Disabled" />
        <boolgroup name="Interrupt SW1" v="Disabled" />
        <boolgroup name="Interrupt SW2" v="Disabled" />
        <boolgroup name="Interrupt SW3" v="Disabled" />
        <boolgroup name="Interrupt LP" v="Disabled" />
        <boolgroup name="Interrupt PLL" v="Disabled" />
        <boolgroup name="Interrupt Illegal Instruction" v="Disabled" />
        <boolgroup name="Interrupt Misalign Access" v="Disabled" />
        <boolgroup name="Interrupt HW Stack Overflow" v="Disabled" />
      </group>
    </Properties>
    <Methods>
      <list name="CPUCond0" v="1">
        <SetClockConfiguration v="don&amp;apos;t generate code" />
        <GetClockConfiguration v="don&amp;apos;t generate code" />
        <SetOperationMode v="don&amp;apos;t generate code" />
        <EnableInt v="generate code" />
        <DisableInt v="generate code" />
        <GetResetSource v="don&amp;apos;t generate code" />
        <SetWaitMode v="generate code" />
        <SetStopMode v="generate code" />
        <GetBusFreqHz v="don&amp;apos;t generate code" />
        <OpenBackDoor v="don&amp;apos;t generate code" />
        <SetFlexRAMFunction v="don&amp;apos;t generate code" />
        <SetFlexNVMPartition v="don&amp;apos;t generate code" />
        <InitShadowRegs v="don&amp;apos;t generate code" />
        <Delay100US v="don&amp;apos;t generate code" />
        <EnablePLL v="don&amp;apos;t generate code" />
      </list>
    </Methods>
    <Events>
      <Event_module_name v="Events" />
      <list name="CPUCond" v="1">
        <event name="OnReset" v="don&amp;apos;t generate code" />
        <event name="OnSwINT0" v="don&amp;apos;t generate code" />
        <event name="OnSwINT1" v="don&amp;apos;t generate code" />
        <event name="OnSwINT2" v="don&amp;apos;t generate code" />
        <event name="OnSwINT3" v="don&amp;apos;t generate code" />
        <event name="OnSwINTLP" v="don&amp;apos;t generate code" />
        <event name="OnPLLError" v="don&amp;apos;t generate code" />
        <event name="OnIllegalOpcode" v="don&amp;apos;t generate code" />
        <event name="OnMisalignData" v="don&amp;apos;t generate code" />
        <event name="OnHWStackError" v="don&amp;apos;t generate code" />
      </list>
    </Events>
    <Compiler v="CodeWarrior DSP C Compiler" />
    <CompilerProperties>
      <Compiler v="CodeWarrior DSP C Compiler" />
      <Unhandled_interrupts v="One handler for all" />
      <Unhandled_int_code>
        <StrgList><![CDATA[/* This code can be changed using the CPU bean property "Build Options / Unhandled int code" */
  asm(DEBUGHLT);                       /* Halt the core and placing it in the debug processing state. */
  /* Here should be two NOPs if DEBUGHLT is removed.
  asm(nop);
  asm(nop); */
]]></StrgList>
      </Unhandled_int_code>
      <boolgroup name="Generate debugger files" v="yes">
        <Generate_mem_file v="yes" />
      </boolgroup>
      <boolgroup name="Generate linker file" v="yes">
        <Constants_in_xROM v="no" />
        <xROM_xRAM_mode v="no" />
        <pROM_xRAM_mode v="yes" />
        <boolgroup name="Serial bootloader support" v="no" />
        <Stack_size v="512" />
        <Heap_size v="256" />
        <list name="ROM/RAM Areas" v="5">
          <group name="MemoryArea0">
            <boolgroup name="ROM/RAM Area" v="Enabled">
              <Name v=".p_Interrupts" />
              <Address v="0" />
              <Size v="222" />
              <Qualifier v="RWX" />
            </boolgroup>
          </group>
          <group name="MemoryArea1">
            <boolgroup name="ROM/RAM Area" v="Enabled">
              <Name v=".p_Code" />
              <Address v="520" />
              <Size v="32248" />
              <Qualifier v="RWX" />
            </boolgroup>
          </group>
          <group name="MemoryArea2">
            <boolgroup name="ROM/RAM Area" v="Enabled">
              <Name v=".x_Data" />
              <Address v="0" />
              <Size v="4096" />
              <Qualifier v="RW" />
            </boolgroup>
          </group>
          <group name="MemoryArea3">
            <boolgroup name="ROM/RAM Area" v="Enabled">
              <Name v=".p_reserved_FCF" />
              <Address v="512" />
              <Size v="8" />
              <Qualifier v="RWX" />
            </boolgroup>
          </group>
          <group name="MemoryArea4">
            <boolgroup name="ROM/RAM Area" v="Enabled">
              <Name v=".x_internal_ROM" />
              <Address v="16606" />
              <Size v="290" />
              <Qualifier v="RW" />
            </boolgroup>
          </group>
        </list>
      </boolgroup>
      <list name="System paths " v="0">
        <EmptySection_DummyValue />
      </list>
      <list name="User paths " v="0">
        <EmptySection_DummyValue />
      </list>
      <list name="Libraries" v="0">
        <EmptySection_DummyValue />
      </list>
      <list name="User directories" v="0">
        <EmptySection_DummyValue />
      </list>
    </CompilerProperties>
  </CPU_Bean>
  <Bean name="Pins1" type="PinSettings">
    <Enabled v="Y" />
    <Properties>
      <Component_name v="Pins1" />
      <PinSettings_IP_Block v="PinSettings" />
      <Processor v="MC56F82748VLH" />
      <list name="ProcessorSpecificItem" v="1">
        <group name="Pin settings">
          <group name="Routing">
            <group name="Peripheral Type ADC">
              <Custom_name v="ADC" />
              <ADC__ADC_Analog_Channel_A_input_0 v="&amp;lt;Automatic&amp;gt;" />
              <ADC__ADC_Analog_Channel_A_input_1 v="&amp;lt;Automatic&amp;gt;" />
              <ADC__ADC_Analog_Channel_A_input_2 v="&amp;lt;Automatic&amp;gt;" />
              <ADC__ADC_Analog_Channel_A_input_3 v="&amp;lt;Automatic&amp;gt;" />
              <ADC__ADC_Analog_Channel_A_input_4 v="&amp;lt;Automatic&amp;gt;" />
              <ADC__ADC_Analog_Channel_A_input_5 v="&amp;lt;Automatic&amp;gt;" />
              <ADC__ADC_Analog_Channel_A_input_6 v="&amp;lt;Automatic&amp;gt;" />
              <ADC__ADC_Analog_Channel_A_input_7 v="&amp;lt;Automatic&amp;gt;" />
              <ADC__ADC_Analog_Channel_B_input_0 v="&amp;lt;Automatic&amp;gt;" />
              <ADC__ADC_Analog_Channel_B_input_1 v="&amp;lt;Automatic&amp;gt;" />
              <ADC__ADC_Analog_Channel_B_input_2 v="&amp;lt;Automatic&amp;gt;" />
              <ADC__ADC_Analog_Channel_B_input_3 v="&amp;lt;Automatic&amp;gt;" />
              <ADC__ADC_Analog_Channel_B_input_4 v="&amp;lt;Automatic&amp;gt;" />
              <ADC__ADC_Analog_Channel_B_input_5 v="&amp;lt;Automatic&amp;gt;" />
              <ADC__ADC_Analog_Channel_B_input_6 v="&amp;lt;Automatic&amp;gt;" />
              <ADC__ADC_Analog_Channel_B_input_7 v="&amp;lt;Automatic&amp;gt;" />
              <ADC__ADC_Analog_Channel_A_input_8 v="&amp;lt;Automatic&amp;gt;" />
              <ADC__ADC_Analog_Channel_A_input_9 v="&amp;lt;Automatic&amp;gt;" />
              <ADC__ADC_Analog_Channel_B_input_8 v="&amp;lt;Automatic&amp;gt;" />
              <ADC__ADC_Analog_Channel_B_input_9 v="&amp;lt;Automatic&amp;gt;" />
              <ADC__ADC_trigger_A_input v="&amp;lt;Automatic&amp;gt;" />
              <ADC__ADC_trigger_B_input v="&amp;lt;Automatic&amp;gt;" />
              <ADC__ADC_Channel_A_Voltage_Reference_High v="&amp;lt;Automatic&amp;gt;" />
              <ADC__ADC_Channel_B_Voltage_Reference_High v="&amp;lt;Automatic&amp;gt;" />
              <ADC__ADC_Channel_A_Voltage_Reference_Low v="&amp;lt;Automatic&amp;gt;" />
              <ADC__ADC_Channel_B_Voltage_Reference_Low v="&amp;lt;Automatic&amp;gt;" />
            </group>
            <group name="Peripheral Type AOI">
              <Custom_name v="AOI" />
              <AOI__AOI_input_A0 v="&amp;lt;Automatic&amp;gt;" />
              <AOI__AOI_input_A1 v="&amp;lt;Automatic&amp;gt;" />
              <AOI__AOI_input_A2 v="&amp;lt;Automatic&amp;gt;" />
              <AOI__AOI_input_A3 v="&amp;lt;Automatic&amp;gt;" />
              <AOI__AOI_input_B0 v="&amp;lt;Automatic&amp;gt;" />
              <AOI__AOI_input_B1 v="&amp;lt;Automatic&amp;gt;" />
              <AOI__AOI_input_B2 v="&amp;lt;Automatic&amp;gt;" />
              <AOI__AOI_input_B3 v="&amp;lt;Automatic&amp;gt;" />
              <AOI__AOI_input_C0 v="&amp;lt;Automatic&amp;gt;" />
              <AOI__AOI_input_C1 v="&amp;lt;Automatic&amp;gt;" />
              <AOI__AOI_input_C2 v="&amp;lt;Automatic&amp;gt;" />
              <AOI__AOI_input_C3 v="&amp;lt;Automatic&amp;gt;" />
              <AOI__AOI_input_D0 v="&amp;lt;Automatic&amp;gt;" />
              <AOI__AOI_input_D1 v="&amp;lt;Automatic&amp;gt;" />
              <AOI__AOI_input_D2 v="&amp;lt;Automatic&amp;gt;" />
              <AOI__AOI_input_D3 v="&amp;lt;Automatic&amp;gt;" />
              <AOI__AOI_output_0 v="&amp;lt;Automatic&amp;gt;" />
              <AOI__AOI_output_1 v="&amp;lt;Automatic&amp;gt;" />
              <AOI__AOI_output_2 v="&amp;lt;Automatic&amp;gt;" />
              <AOI__AOI_output_3 v="&amp;lt;Automatic&amp;gt;" />
            </group>
            <group name="Peripheral Type CAN">
              <Custom_name v="CAN" />
              <CAN__CAN_Receiver_Input_Pin v="&amp;lt;Automatic&amp;gt;" />
              <CAN__CAN_Transmitter_Output_Pin v="&amp;lt;Automatic&amp;gt;" />
            </group>
            <group name="Peripheral Type CMP">
              <Custom_name v="CMPA" />
              <CMPA__Comparator_negative_input_0_ v="&amp;lt;Automatic&amp;gt;" />
              <CMPA__Comparator_negative_input_1_ v="&amp;lt;Automatic&amp;gt;" />
              <CMPA__Comparator_negative_input_2_ v="&amp;lt;Automatic&amp;gt;" />
              <CMPA__Comparator_negative_input_3_ v="&amp;lt;Automatic&amp;gt;" />
              <CMPA__Comparator_negative_input_4_ v="&amp;lt;Automatic&amp;gt;" />
              <CMPA__Comparator_negative_input_5 v="&amp;lt;Automatic&amp;gt;" />
              <CMPA__Comparator_negative_input_6_ v="&amp;lt;Automatic&amp;gt;" />
              <CMPA__Comparator_negative_input_7_ v="&amp;lt;Automatic&amp;gt;" />
              <CMPA__Comparator_output v="&amp;lt;Automatic&amp;gt;" />
              <CMPA__Comparator_positive_input_0 v="&amp;lt;Automatic&amp;gt;" />
              <CMPA__Comparator_positive_input_1 v="&amp;lt;Automatic&amp;gt;" />
              <CMPA__Comparator_positive_input_2 v="&amp;lt;Automatic&amp;gt;" />
              <CMPA__Comparator_positive_input_3 v="&amp;lt;Automatic&amp;gt;" />
              <CMPA__Comparator_positive_input_4_ v="&amp;lt;Automatic&amp;gt;" />
              <CMPA__Comparator_positive_input_5 v="&amp;lt;Automatic&amp;gt;" />
              <CMPA__Comparator_positive_input_6_ v="&amp;lt;Automatic&amp;gt;" />
              <CMPA__Comparator_positive_input_7_ v="&amp;lt;Automatic&amp;gt;" />
              <CMPA__Comparator_window_sample_input v="&amp;lt;Automatic&amp;gt;" />
              <Custom_name v="CMPB" />
              <CMPB__Comparator_negative_input_0_ v="&amp;lt;Automatic&amp;gt;" />
              <CMPB__Comparator_negative_input_1_ v="&amp;lt;Automatic&amp;gt;" />
              <CMPB__Comparator_negative_input_2_ v="&amp;lt;Automatic&amp;gt;" />
              <CMPB__Comparator_negative_input_3_ v="&amp;lt;Automatic&amp;gt;" />
              <CMPB__Comparator_negative_input_4_ v="&amp;lt;Automatic&amp;gt;" />
              <CMPB__Comparator_negative_input_5 v="&amp;lt;Automatic&amp;gt;" />
              <CMPB__Comparator_negative_input_6_ v="&amp;lt;Automatic&amp;gt;" />
              <CMPB__Comparator_negative_input_7_ v="&amp;lt;Automatic&amp;gt;" />
              <CMPB__Comparator_output v="&amp;lt;Automatic&amp;gt;" />
              <CMPB__Comparator_positive_input_0 v="&amp;lt;Automatic&amp;gt;" />
              <CMPB__Comparator_positive_input_1 v="&amp;lt;Automatic&amp;gt;" />
              <CMPB__Comparator_positive_input_2 v="&amp;lt;Automatic&amp;gt;" />
              <CMPB__Comparator_positive_input_3 v="&amp;lt;Automatic&amp;gt;" />
              <CMPB__Comparator_positive_input_4_ v="&amp;lt;Automatic&amp;gt;" />
              <CMPB__Comparator_positive_input_5 v="&amp;lt;Automatic&amp;gt;" />
              <CMPB__Comparator_positive_input_6_ v="&amp;lt;Automatic&amp;gt;" />
              <CMPB__Comparator_positive_input_7_ v="&amp;lt;Automatic&amp;gt;" />
              <CMPB__Comparator_window_sample_input v="&amp;lt;Automatic&amp;gt;" />
              <Custom_name v="CMPC" />
              <CMPC__Comparator_negative_input_0_ v="&amp;lt;Automatic&amp;gt;" />
              <CMPC__Comparator_negative_input_1_ v="&amp;lt;Automatic&amp;gt;" />
              <CMPC__Comparator_negative_input_2_ v="&amp;lt;Automatic&amp;gt;" />
              <CMPC__Comparator_negative_input_3_ v="&amp;lt;Automatic&amp;gt;" />
              <CMPC__Comparator_negative_input_4_ v="&amp;lt;Automatic&amp;gt;" />
              <CMPC__Comparator_negative_input_5 v="&amp;lt;Automatic&amp;gt;" />
              <CMPC__Comparator_negative_input_6_ v="&amp;lt;Automatic&amp;gt;" />
              <CMPC__Comparator_negative_input_7_ v="&amp;lt;Automatic&amp;gt;" />
              <CMPC__Comparator_output v="&amp;lt;Automatic&amp;gt;" />
              <CMPC__Comparator_positive_input_0 v="&amp;lt;Automatic&amp;gt;" />
              <CMPC__Comparator_positive_input_1 v="&amp;lt;Automatic&amp;gt;" />
              <CMPC__Comparator_positive_input_2 v="&amp;lt;Automatic&amp;gt;" />
              <CMPC__Comparator_positive_input_3 v="&amp;lt;Automatic&amp;gt;" />
              <CMPC__Comparator_positive_input_4_ v="&amp;lt;Automatic&amp;gt;" />
              <CMPC__Comparator_positive_input_5 v="&amp;lt;Automatic&amp;gt;" />
              <CMPC__Comparator_positive_input_6_ v="&amp;lt;Automatic&amp;gt;" />
              <CMPC__Comparator_positive_input_7_ v="&amp;lt;Automatic&amp;gt;" />
              <CMPC__Comparator_window_sample_input v="&amp;lt;Automatic&amp;gt;" />
              <Custom_name v="CMPD" />
              <CMPD__Comparator_negative_input_0_ v="&amp;lt;Automatic&amp;gt;" />
              <CMPD__Comparator_negative_input_1_ v="&amp;lt;Automatic&amp;gt;" />
              <CMPD__Comparator_negative_input_2_ v="&amp;lt;Automatic&amp;gt;" />
              <CMPD__Comparator_negative_input_3_ v="&amp;lt;Automatic&amp;gt;" />
              <CMPD__Comparator_negative_input_4_ v="&amp;lt;Automatic&amp;gt;" />
              <CMPD__Comparator_negative_input_5 v="&amp;lt;Automatic&amp;gt;" />
              <CMPD__Comparator_negative_input_6_ v="&amp;lt;Automatic&amp;gt;" />
              <CMPD__Comparator_negative_input_7_ v="&amp;lt;Automatic&amp;gt;" />
              <CMPD__Comparator_output v="&amp;lt;Automatic&amp;gt;" />
              <CMPD__Comparator_positive_input_0 v="&amp;lt;Automatic&amp;gt;" />
              <CMPD__Comparator_positive_input_1 v="&amp;lt;Automatic&amp;gt;" />
              <CMPD__Comparator_positive_input_2 v="&amp;lt;Automatic&amp;gt;" />
              <CMPD__Comparator_positive_input_3 v="&amp;lt;Automatic&amp;gt;" />
              <CMPD__Comparator_positive_input_4_ v="&amp;lt;Automatic&amp;gt;" />
              <CMPD__Comparator_positive_input_5 v="&amp;lt;Automatic&amp;gt;" />
              <CMPD__Comparator_positive_input_6_ v="&amp;lt;Automatic&amp;gt;" />
              <CMPD__Comparator_positive_input_7_ v="&amp;lt;Automatic&amp;gt;" />
              <CMPD__Comparator_window_sample_input v="&amp;lt;Automatic&amp;gt;" />
            </group>
            <group name="Peripheral Type COP">
              <Custom_name v="COP" />
            </group>
            <group name="Peripheral Type CRC">
              <Custom_name v="CRC" />
            </group>
            <group name="Peripheral Type DAC">
              <Custom_name v="DACA" />
              <DACA__DAC_trigger_input v="&amp;lt;Automatic&amp;gt;" />
              <DACA__DAC_output v="&amp;lt;Automatic&amp;gt;" />
              <Custom_name v="DACB" />
              <DACB__DAC_trigger_input v="&amp;lt;Automatic&amp;gt;" />
              <DACB__DAC_output v="&amp;lt;Automatic&amp;gt;" />
            </group>
            <group name="Peripheral Type DMA">
              <Custom_name v="DMA" />
              <DMA__DMA_channel_0_input v="&amp;lt;Automatic&amp;gt;" />
              <DMA__DMA_channel_1_input v="&amp;lt;Automatic&amp;gt;" />
              <DMA__DMA_channel_2_input v="&amp;lt;Automatic&amp;gt;" />
              <DMA__DMA_channel_3_input v="&amp;lt;Automatic&amp;gt;" />
            </group>
            <group name="Peripheral Type EONCE">
              <EONCE__JTAG_Clock v="&amp;lt;Automatic&amp;gt;" />
              <EONCE__JTAG_Data_Input v="&amp;lt;Automatic&amp;gt;" />
              <EONCE__JTAG_Data_Output v="&amp;lt;Automatic&amp;gt;" />
              <EONCE__JTAG_Mode_Selection v="&amp;lt;Automatic&amp;gt;" />
            </group>
            <group name="Peripheral Type EWM">
              <Custom_name v="EWM" />
              <EWM__EWM_safety_status_input v="&amp;lt;Automatic&amp;gt;" />
              <EWM__EWM_output v="&amp;lt;Automatic&amp;gt;" />
            </group>
            <group name="Peripheral Type FMC">
              <Custom_name v="FMC" />
            </group>
            <group name="Peripheral Type FTFA">
              <Custom_name v="FTFA" />
            </group>
            <group name="Peripheral Type GPIO">
              <Custom_name v="GPIOA" />
              <GPIOA__General_purpose_IO_pin_0 v="&amp;lt;Automatic&amp;gt;" />
              <Direction v="&amp;lt;Automatic&amp;gt;" />
              <GPIOA__General_purpose_IO_pin_1 v="&amp;lt;Automatic&amp;gt;" />
              <Direction v="&amp;lt;Automatic&amp;gt;" />
              <GPIOA__General_purpose_IO_pin_2 v="&amp;lt;Automatic&amp;gt;" />
              <Direction v="&amp;lt;Automatic&amp;gt;" />
              <GPIOA__General_purpose_IO_pin_3 v="&amp;lt;Automatic&amp;gt;" />
              <Direction v="&amp;lt;Automatic&amp;gt;" />
              <GPIOA__General_purpose_IO_pin_4 v="&amp;lt;Automatic&amp;gt;" />
              <Direction v="&amp;lt;Automatic&amp;gt;" />
              <GPIOA__General_purpose_IO_pin_5 v="&amp;lt;Automatic&amp;gt;" />
              <Direction v="&amp;lt;Automatic&amp;gt;" />
              <GPIOA__General_purpose_IO_pin_6 v="&amp;lt;Automatic&amp;gt;" />
              <Direction v="&amp;lt;Automatic&amp;gt;" />
              <GPIOA__General_purpose_IO_pin_7 v="&amp;lt;Automatic&amp;gt;" />
              <Direction v="&amp;lt;Automatic&amp;gt;" />
              <Custom_name v="GPIOB" />
              <GPIOB__General_purpose_IO_pin_0 v="&amp;lt;Automatic&amp;gt;" />
              <Direction v="&amp;lt;Automatic&amp;gt;" />
              <GPIOB__General_purpose_IO_pin_1 v="&amp;lt;Automatic&amp;gt;" />
              <Direction v="&amp;lt;Automatic&amp;gt;" />
              <GPIOB__General_purpose_IO_pin_2 v="&amp;lt;Automatic&amp;gt;" />
              <Direction v="&amp;lt;Automatic&amp;gt;" />
              <GPIOB__General_purpose_IO_pin_3 v="&amp;lt;Automatic&amp;gt;" />
              <Direction v="&amp;lt;Automatic&amp;gt;" />
              <GPIOB__General_purpose_IO_pin_4 v="&amp;lt;Automatic&amp;gt;" />
              <Direction v="&amp;lt;Automatic&amp;gt;" />
              <GPIOB__General_purpose_IO_pin_5 v="&amp;lt;Automatic&amp;gt;" />
              <Direction v="&amp;lt;Automatic&amp;gt;" />
              <GPIOB__General_purpose_IO_pin_6 v="&amp;lt;Automatic&amp;gt;" />
              <Direction v="&amp;lt;Automatic&amp;gt;" />
              <GPIOB__General_purpose_IO_pin_7 v="&amp;lt;Automatic&amp;gt;" />
              <Direction v="&amp;lt;Automatic&amp;gt;" />
              <Custom_name v="GPIOC" />
              <GPIOC__General_purpose_IO_pin_0 v="&amp;lt;Automatic&amp;gt;" />
              <Direction v="&amp;lt;Automatic&amp;gt;" />
              <GPIOC__General_purpose_IO_pin_1 v="&amp;lt;Automatic&amp;gt;" />
              <Direction v="&amp;lt;Automatic&amp;gt;" />
              <GPIOC__General_purpose_IO_pin_2 v="&amp;lt;Automatic&amp;gt;" />
              <Direction v="&amp;lt;Automatic&amp;gt;" />
              <GPIOC__General_purpose_IO_pin_3 v="&amp;lt;Automatic&amp;gt;" />
              <Direction v="&amp;lt;Automatic&amp;gt;" />
              <GPIOC__General_purpose_IO_pin_4 v="&amp;lt;Automatic&amp;gt;" />
              <Direction v="&amp;lt;Automatic&amp;gt;" />
              <GPIOC__General_purpose_IO_pin_5 v="&amp;lt;Automatic&amp;gt;" />
              <Direction v="&amp;lt;Automatic&amp;gt;" />
              <GPIOC__General_purpose_IO_pin_6 v="&amp;lt;Automatic&amp;gt;" />
              <Direction v="&amp;lt;Automatic&amp;gt;" />
              <GPIOC__General_purpose_IO_pin_7 v="&amp;lt;Automatic&amp;gt;" />
              <Direction v="&amp;lt;Automatic&amp;gt;" />
              <GPIOC__General_purpose_IO_pin_8 v="&amp;lt;Automatic&amp;gt;" />
              <Direction v="&amp;lt;Automatic&amp;gt;" />
              <GPIOC__General_purpose_IO_pin_9 v="&amp;lt;Automatic&amp;gt;" />
              <Direction v="&amp;lt;Automatic&amp;gt;" />
              <GPIOC__General_purpose_IO_pin_10 v="&amp;lt;Automatic&amp;gt;" />
              <Direction v="&amp;lt;Automatic&amp;gt;" />
              <GPIOC__General_purpose_IO_pin_11 v="&amp;lt;Automatic&amp;gt;" />
              <Direction v="&amp;lt;Automatic&amp;gt;" />
              <GPIOC__General_purpose_IO_pin_12 v="&amp;lt;Automatic&amp;gt;" />
              <Direction v="&amp;lt;Automatic&amp;gt;" />
              <GPIOC__General_purpose_IO_pin_13 v="&amp;lt;Automatic&amp;gt;" />
              <Direction v="&amp;lt;Automatic&amp;gt;" />
              <GPIOC__General_purpose_IO_pin_14 v="&amp;lt;Automatic&amp;gt;" />
              <Direction v="&amp;lt;Automatic&amp;gt;" />
              <GPIOC__General_purpose_IO_pin_15 v="&amp;lt;Automatic&amp;gt;" />
              <Direction v="&amp;lt;Automatic&amp;gt;" />
              <Custom_name v="GPIOD" />
              <GPIOD__General_purpose_IO_pin_0 v="&amp;lt;Automatic&amp;gt;" />
              <Direction v="&amp;lt;Automatic&amp;gt;" />
              <GPIOD__General_purpose_IO_pin_1 v="&amp;lt;Automatic&amp;gt;" />
              <Direction v="&amp;lt;Automatic&amp;gt;" />
              <GPIOD__General_purpose_IO_pin_2 v="&amp;lt;Automatic&amp;gt;" />
              <Direction v="&amp;lt;Automatic&amp;gt;" />
              <GPIOD__General_purpose_IO_pin_3 v="&amp;lt;Automatic&amp;gt;" />
              <Direction v="&amp;lt;Automatic&amp;gt;" />
              <GPIOD__General_purpose_IO_pin_4 v="&amp;lt;Automatic&amp;gt;" />
              <Direction v="&amp;lt;Automatic&amp;gt;" />
              <Custom_name v="GPIOE" />
              <GPIOE__General_purpose_IO_pin_0 v="&amp;lt;Automatic&amp;gt;" />
              <Direction v="&amp;lt;Automatic&amp;gt;" />
              <GPIOE__General_purpose_IO_pin_1 v="&amp;lt;Automatic&amp;gt;" />
              <Direction v="Output" />
              <GPIOE__General_purpose_IO_pin_2 v="&amp;lt;Automatic&amp;gt;" />
              <Direction v="&amp;lt;Automatic&amp;gt;" />
              <GPIOE__General_purpose_IO_pin_3 v="&amp;lt;Automatic&amp;gt;" />
              <Direction v="&amp;lt;Automatic&amp;gt;" />
              <GPIOE__General_purpose_IO_pin_4 v="&amp;lt;Automatic&amp;gt;" />
              <Direction v="&amp;lt;Automatic&amp;gt;" />
              <GPIOE__General_purpose_IO_pin_5 v="&amp;lt;Automatic&amp;gt;" />
              <Direction v="&amp;lt;Automatic&amp;gt;" />
              <GPIOE__General_purpose_IO_pin_6 v="&amp;lt;Automatic&amp;gt;" />
              <Direction v="&amp;lt;Automatic&amp;gt;" />
              <GPIOE__General_purpose_IO_pin_7 v="&amp;lt;Automatic&amp;gt;" />
              <Direction v="&amp;lt;Automatic&amp;gt;" />
              <Custom_name v="GPIOF" />
              <GPIOF__General_purpose_IO_pin_0 v="&amp;lt;Automatic&amp;gt;" />
              <Direction v="&amp;lt;Automatic&amp;gt;" />
              <GPIOF__General_purpose_IO_pin_1 v="&amp;lt;Automatic&amp;gt;" />
              <Direction v="&amp;lt;Automatic&amp;gt;" />
              <GPIOF__General_purpose_IO_pin_2 v="&amp;lt;Automatic&amp;gt;" />
              <Direction v="&amp;lt;Automatic&amp;gt;" />
              <GPIOF__General_purpose_IO_pin_3 v="&amp;lt;Automatic&amp;gt;" />
              <Direction v="&amp;lt;Automatic&amp;gt;" />
              <GPIOF__General_purpose_IO_pin_4 v="&amp;lt;Automatic&amp;gt;" />
              <Direction v="&amp;lt;Automatic&amp;gt;" />
              <GPIOF__General_purpose_IO_pin_5 v="&amp;lt;Automatic&amp;gt;" />
              <Direction v="&amp;lt;Automatic&amp;gt;" />
              <GPIOF__General_purpose_IO_pin_6 v="&amp;lt;Automatic&amp;gt;" />
              <Direction v="&amp;lt;Automatic&amp;gt;" />
              <GPIOF__General_purpose_IO_pin_7 v="&amp;lt;Automatic&amp;gt;" />
              <Direction v="&amp;lt;Automatic&amp;gt;" />
              <GPIOF__General_purpose_IO_pin_8 v="&amp;lt;Automatic&amp;gt;" />
              <Direction v="&amp;lt;Automatic&amp;gt;" />
            </group>
            <group name="Peripheral Type I2C">
              <Custom_name v="I2C" />
              <I2C__I2C_Serial_Clock_Line v="&amp;lt;Automatic&amp;gt;" />
              <I2C__I2C_Serial_Data_Line v="&amp;lt;Automatic&amp;gt;" />
            </group>
            <group name="Peripheral Type INTC">
              <Custom_name v="INTC" />
            </group>
            <group name="Peripheral Type MCM">
              <Custom_name v="MCM" />
            </group>
            <group name="Peripheral Type NV">
              <Custom_name v="FTFL_FlashConfig" />
            </group>
            <group name="Peripheral Type OCCS">
              <Custom_name v="OCCS" />
              <OCCS__OCCS_external_clock_input_0 v="&amp;lt;Automatic&amp;gt;" />
              <OCCS__Oscillator_input_pin v="&amp;lt;Automatic&amp;gt;" />
              <OCCS__Oscillator_output_pin v="&amp;lt;Automatic&amp;gt;" />
            </group>
            <group name="Peripheral Type PIT">
              <Custom_name v="PIT0" />
              <PIT0__PIT_output v="&amp;lt;Automatic&amp;gt;" />
              <Custom_name v="PIT1" />
              <PIT1__PIT_output v="&amp;lt;Automatic&amp;gt;" />
            </group>
            <group name="Peripheral Type PMC">
              <Custom_name v="PMC" />
            </group>
            <group name="Peripheral Type PWM">
              <Custom_name v="PWMA" />
              <PWMA__PWM_external_clock_input v="&amp;lt;Automatic&amp;gt;" />
              <PWMA__PWM_cannel_0_external_control_A_input v="&amp;lt;Automatic&amp;gt;" />
              <PWMA__PWM_cannel_1_external_control_A_input v="&amp;lt;Automatic&amp;gt;" />
              <PWMA__PWM_cannel_2_external_control_A_input v="&amp;lt;Automatic&amp;gt;" />
              <PWMA__PWM_cannel_3_external_control_A_input v="&amp;lt;Automatic&amp;gt;" />
              <PWMA__PWM_cannel_0_external_control_B_input v="&amp;lt;Automatic&amp;gt;" />
              <PWMA__PWM_cannel_1_external_control_B_input v="&amp;lt;Automatic&amp;gt;" />
              <PWMA__PWM_cannel_2_external_control_B_input v="&amp;lt;Automatic&amp;gt;" />
              <PWMA__PWM_cannel_3_external_control_B_input v="&amp;lt;Automatic&amp;gt;" />
              <PWMA__PWM_external_force_input v="&amp;lt;Automatic&amp;gt;" />
              <PWMA__PWM_cannel_0_external_synchronization_input v="&amp;lt;Automatic&amp;gt;" />
              <PWMA__PWM_cannel_1_external_synchronization_input v="&amp;lt;Automatic&amp;gt;" />
              <PWMA__PWM_cannel_2_external_synchronization_input v="&amp;lt;Automatic&amp;gt;" />
              <PWMA__PWM_cannel_3_external_synchronization_input v="&amp;lt;Automatic&amp;gt;" />
              <PWMA__PWM_Fault_input_0 v="&amp;lt;Automatic&amp;gt;" />
              <PWMA__PWM_Fault_input_1 v="&amp;lt;Automatic&amp;gt;" />
              <PWMA__PWM_Fault_input_2 v="&amp;lt;Automatic&amp;gt;" />
              <PWMA__PWM_Fault_input_3 v="&amp;lt;Automatic&amp;gt;" />
              <PWMA__PWM_fault_input_4 v="&amp;lt;Automatic&amp;gt;" />
              <PWMA__PWM_fault_input_5 v="&amp;lt;Automatic&amp;gt;" />
              <PWMA__PWM_fault_input_6 v="&amp;lt;Automatic&amp;gt;" />
              <PWMA__PWM_fault_input_7 v="&amp;lt;Automatic&amp;gt;" />
              <PWMA__PWM_channel_0_output_trigger_0 v="&amp;lt;Automatic&amp;gt;" />
              <PWMA__PWM_channel_1_output_trigger_0 v="&amp;lt;Automatic&amp;gt;" />
              <PWMA__PWM_channel_2_output_trigger_0 v="&amp;lt;Automatic&amp;gt;" />
              <PWMA__PWM_channel_3_output_trigger_0 v="&amp;lt;Automatic&amp;gt;" />
              <PWMA__PWM_channel_0_output_trigger_1 v="&amp;lt;Automatic&amp;gt;" />
              <PWMA__PWM_channel_1_output_trigger_1 v="&amp;lt;Automatic&amp;gt;" />
              <PWMA__PWM_channel_2_output_trigger_1 v="&amp;lt;Automatic&amp;gt;" />
              <PWMA__PWM_channel_3_output_trigger_1 v="&amp;lt;Automatic&amp;gt;" />
              <PWMA__PWM_output_A_channel_0 v="&amp;lt;Automatic&amp;gt;" />
              <Direction v="&amp;lt;Automatic&amp;gt;" />
              <PWMA__PWM_output_A_channel_1 v="&amp;lt;Automatic&amp;gt;" />
              <Direction v="&amp;lt;Automatic&amp;gt;" />
              <PWMA__PWM_output_A_channel_2 v="&amp;lt;Automatic&amp;gt;" />
              <Direction v="&amp;lt;Automatic&amp;gt;" />
              <PWMA__PWM_output_A_channel_3 v="&amp;lt;Automatic&amp;gt;" />
              <Direction v="&amp;lt;Automatic&amp;gt;" />
              <PWMA__PWM_output_B_channel_0 v="&amp;lt;Automatic&amp;gt;" />
              <Direction v="&amp;lt;Automatic&amp;gt;" />
              <PWMA__PWM_output_B_channel_1 v="&amp;lt;Automatic&amp;gt;" />
              <Direction v="&amp;lt;Automatic&amp;gt;" />
              <PWMA__PWM_output_B_channel_2 v="&amp;lt;Automatic&amp;gt;" />
              <Direction v="&amp;lt;Automatic&amp;gt;" />
              <PWMA__PWM_output_B_channel_3 v="&amp;lt;Automatic&amp;gt;" />
              <Direction v="&amp;lt;Automatic&amp;gt;" />
              <PWMA__PWM_output_X_channel_0 v="&amp;lt;Automatic&amp;gt;" />
              <Direction v="&amp;lt;Automatic&amp;gt;" />
              <PWMA__PWM_output_X_channel_1 v="&amp;lt;Automatic&amp;gt;" />
              <Direction v="&amp;lt;Automatic&amp;gt;" />
              <PWMA__PWM_output_X_channel_2 v="&amp;lt;Automatic&amp;gt;" />
              <Direction v="&amp;lt;Automatic&amp;gt;" />
              <PWMA__PWM_output_X_channel_3 v="&amp;lt;Automatic&amp;gt;" />
              <Direction v="&amp;lt;Automatic&amp;gt;" />
            </group>
            <group name="Peripheral Type QSCI">
              <Custom_name v="QSCI0" />
              <QSCI0__QSCI_receive_data v="&amp;lt;Automatic&amp;gt;" />
              <QSCI0__QSCI_transmit_data v="&amp;lt;Automatic&amp;gt;" />
              <Custom_name v="QSCI1" />
              <QSCI1__QSCI_receive_data v="&amp;lt;Automatic&amp;gt;" />
              <QSCI1__QSCI_transmit_data v="&amp;lt;Automatic&amp;gt;" />
            </group>
            <group name="Peripheral Type QSPI">
              <Custom_name v="QSPI0" />
              <QSPI0__SPI_Master_in_Slave_out v="&amp;lt;Automatic&amp;gt;" />
              <Direction v="&amp;lt;Automatic&amp;gt;" />
              <QSPI0__SPI_Master_out_Slave_in v="&amp;lt;Automatic&amp;gt;" />
              <Direction v="&amp;lt;Automatic&amp;gt;" />
              <QSPI0__SPI_Serial_Clock_Output v="&amp;lt;Automatic&amp;gt;" />
              <Direction v="&amp;lt;Automatic&amp;gt;" />
              <QSPI0__SPI_Slave_select v="&amp;lt;Automatic&amp;gt;" />
              <Direction v="&amp;lt;Automatic&amp;gt;" />
              <Custom_name v="QSPI1" />
              <QSPI1__SPI_Master_in_Slave_out v="&amp;lt;Automatic&amp;gt;" />
              <Direction v="&amp;lt;Automatic&amp;gt;" />
              <QSPI1__SPI_Master_out_Slave_in v="&amp;lt;Automatic&amp;gt;" />
              <Direction v="&amp;lt;Automatic&amp;gt;" />
              <QSPI1__SPI_Serial_Clock_Output v="&amp;lt;Automatic&amp;gt;" />
              <Direction v="&amp;lt;Automatic&amp;gt;" />
              <QSPI1__SPI_Slave_select v="&amp;lt;Automatic&amp;gt;" />
              <Direction v="&amp;lt;Automatic&amp;gt;" />
            </group>
            <group name="Peripheral Type SIM">
              <Custom_name v="SIM" />
              <SIM__Clock_generation_SIM_output_0 v="&amp;lt;Automatic&amp;gt;" />
              <SIM__Clock_generation_SIM_output_1 v="&amp;lt;Automatic&amp;gt;" />
            </group>
            <group name="Peripheral Type TMR">
              <Custom_name v="TMR" />
              <TMR__Quad_timer_input_0 v="&amp;lt;Automatic&amp;gt;" />
              <TMR__Quad_timer_input_1 v="&amp;lt;Automatic&amp;gt;" />
              <TMR__Quad_timer_input_2 v="&amp;lt;Automatic&amp;gt;" />
              <TMR__Quad_timer_input_3 v="&amp;lt;Automatic&amp;gt;" />
              <TMR__Quad_timer_output_0 v="&amp;lt;Automatic&amp;gt;" />
              <TMR__Quad_timer_output_1 v="&amp;lt;Automatic&amp;gt;" />
              <TMR__Quad_timer_output_2 v="&amp;lt;Automatic&amp;gt;" />
              <TMR__Quad_timer_output_3 v="&amp;lt;Automatic&amp;gt;" />
            </group>
            <group name="Peripheral Type XBARA">
              <Custom_name v="XBARA" />
              <XBARA__XBAR_input_0 v="&amp;lt;Automatic&amp;gt;" />
              <XBARA__XBAR_input_1 v="&amp;lt;Automatic&amp;gt;" />
              <XBARA__XBAR_input_2 v="&amp;lt;Automatic&amp;gt;" />
              <XBARA__XBAR_input_3 v="&amp;lt;Automatic&amp;gt;" />
              <XBARA__XBAR_input_4 v="&amp;lt;Automatic&amp;gt;" />
              <XBARA__XBAR_input_5 v="&amp;lt;Automatic&amp;gt;" />
              <XBARA__XBAR_input_6 v="&amp;lt;Automatic&amp;gt;" />
              <XBARA__XBAR_input_7 v="&amp;lt;Automatic&amp;gt;" />
              <XBARA__XBAR_input_8 v="&amp;lt;Automatic&amp;gt;" />
              <XBARA__XBAR_input_9 v="&amp;lt;Automatic&amp;gt;" />
              <XBARA__XBAR_input_10 v="&amp;lt;Automatic&amp;gt;" />
              <XBARA__XBAR_input_11 v="&amp;lt;Automatic&amp;gt;" />
              <XBARA__XBAR_input_12 v="&amp;lt;Automatic&amp;gt;" />
              <XBARA__XBAR_input_13 v="&amp;lt;Automatic&amp;gt;" />
              <XBARA__XBAR_input_14 v="&amp;lt;Automatic&amp;gt;" />
              <XBARA__XBAR_input_15 v="&amp;lt;Automatic&amp;gt;" />
              <XBARA__XBAR_input_16 v="&amp;lt;Automatic&amp;gt;" />
              <XBARA__XBAR_input_17 v="&amp;lt;Automatic&amp;gt;" />
              <XBARA__XBAR_input_18 v="&amp;lt;Automatic&amp;gt;" />
              <XBARA__XBAR_input_19 v="&amp;lt;Automatic&amp;gt;" />
              <XBARA__XBAR_input_20 v="&amp;lt;Automatic&amp;gt;" />
              <XBARA__XBAR_input_21 v="&amp;lt;Automatic&amp;gt;" />
              <XBARA__XBAR_input_22 v="&amp;lt;Automatic&amp;gt;" />
              <XBARA__XBAR_input_23 v="&amp;lt;Automatic&amp;gt;" />
              <XBARA__XBAR_input_24 v="&amp;lt;Automatic&amp;gt;" />
              <XBARA__XBAR_input_25 v="&amp;lt;Automatic&amp;gt;" />
              <XBARA__XBAR_input_26 v="&amp;lt;Automatic&amp;gt;" />
              <XBARA__XBAR_input_27 v="&amp;lt;Automatic&amp;gt;" />
              <XBARA__XBAR_input_28 v="&amp;lt;Automatic&amp;gt;" />
              <XBARA__XBAR_input_29 v="&amp;lt;Automatic&amp;gt;" />
              <XBARA__XBAR_input_30 v="&amp;lt;Automatic&amp;gt;" />
              <XBARA__XBAR_input_31 v="&amp;lt;Automatic&amp;gt;" />
              <XBARA__XBAR_output_4 v="&amp;lt;Automatic&amp;gt;" />
              <XBARA__XBAR_output_5 v="&amp;lt;Automatic&amp;gt;" />
              <XBARA__XBAR_output_6 v="&amp;lt;Automatic&amp;gt;" />
              <XBARA__XBAR_output_7 v="&amp;lt;Automatic&amp;gt;" />
              <XBARA__XBAR_output_8 v="&amp;lt;Automatic&amp;gt;" />
              <XBARA__XBAR_output_9 v="&amp;lt;Automatic&amp;gt;" />
              <XBARA__XBAR_output_10 v="&amp;lt;Automatic&amp;gt;" />
              <XBARA__XBAR_output_11 v="&amp;lt;Automatic&amp;gt;" />
            </group>
            <group name="Peripheral Type XBARB">
              <Custom_name v="XBARB" />
            </group>
            <group name="Non-peripheral pins">
              <RESET v="&amp;lt;Automatic&amp;gt;" />
              <vpp v="&amp;lt;Automatic&amp;gt;" />
              <VCC v="&amp;lt;Automatic&amp;gt;" />
              <GND v="&amp;lt;Automatic&amp;gt;" />
            </group>
          </group>
          <group name="Electrical properties">
            <group name="Pin 1: TCK/GPIOD2">
              <Custom_name__Signal_name v="TCK/GPIOD2" />
              <Slew_rate v="&amp;lt;Automatic&amp;gt;" />
              <Open_drain v="&amp;lt;Automatic&amp;gt;" />
              <Drive_strength v="&amp;lt;Automatic&amp;gt;" />
              <Pull_select v="&amp;lt;Automatic&amp;gt;" />
              <Pull_enable v="&amp;lt;Automatic&amp;gt;" />
            </group>
            <group name="Pin 2: RESETB/VPP/GPIOD4">
              <Custom_name__Signal_name v="RESETB/VPP/GPIOD4" />
              <Slew_rate v="&amp;lt;Automatic&amp;gt;" />
              <Open_drain v="&amp;lt;Automatic&amp;gt;" />
              <Drive_strength v="&amp;lt;Automatic&amp;gt;" />
              <Pull_select v="&amp;lt;Automatic&amp;gt;" />
              <Pull_enable v="&amp;lt;Automatic&amp;gt;" />
            </group>
            <group name="Pin 3: GPIOC0/EXTAL/CLKIN0">
              <Custom_name__Signal_name v="GPIOC0/EXTAL/CLKIN0" />
              <Slew_rate v="&amp;lt;Automatic&amp;gt;" />
              <Open_drain v="&amp;lt;Automatic&amp;gt;" />
              <Drive_strength v="&amp;lt;Automatic&amp;gt;" />
              <Pull_select v="&amp;lt;Automatic&amp;gt;" />
              <Pull_enable v="&amp;lt;Automatic&amp;gt;" />
            </group>
            <group name="Pin 4: GPIOC1/XTAL">
              <Custom_name__Signal_name v="GPIOC1/XTAL" />
              <Slew_rate v="&amp;lt;Automatic&amp;gt;" />
              <Open_drain v="&amp;lt;Automatic&amp;gt;" />
              <Drive_strength v="&amp;lt;Automatic&amp;gt;" />
              <Pull_select v="&amp;lt;Automatic&amp;gt;" />
              <Pull_enable v="&amp;lt;Automatic&amp;gt;" />
            </group>
            <group name="Pin 5: GPIOC2/TXD0/XB_OUT11/XB_IN2/CLKO0">
              <Custom_name__Signal_name v="GPIOC2/TXD0/XB_OUT11/XB_IN2/CLKO0" />
              <Slew_rate v="&amp;lt;Automatic&amp;gt;" />
              <Open_drain v="&amp;lt;Automatic&amp;gt;" />
              <Drive_strength v="&amp;lt;Automatic&amp;gt;" />
              <Pull_select v="&amp;lt;Automatic&amp;gt;" />
              <Pull_enable v="&amp;lt;Automatic&amp;gt;" />
            </group>
            <group name="Pin 6: GPIOF8/RXD0/XB_OUT10/CMPD_O/PWM_2X">
              <Custom_name__Signal_name v="GPIOF8/RXD0/XB_OUT10/CMPD_O/PWM_2X" />
              <Slew_rate v="&amp;lt;Automatic&amp;gt;" />
              <Open_drain v="&amp;lt;Automatic&amp;gt;" />
              <Drive_strength v="&amp;lt;Automatic&amp;gt;" />
              <Pull_select v="&amp;lt;Automatic&amp;gt;" />
              <Pull_enable v="&amp;lt;Automatic&amp;gt;" />
            </group>
            <group name="Pin 7: GPIOC3/TA0/CMPA_O/RXD0/CLKIN1">
              <Custom_name__Signal_name v="GPIOC3/TA0/CMPA_O/RXD0/CLKIN1" />
              <Slew_rate v="&amp;lt;Automatic&amp;gt;" />
              <Open_drain v="&amp;lt;Automatic&amp;gt;" />
              <Drive_strength v="&amp;lt;Automatic&amp;gt;" />
              <Pull_select v="&amp;lt;Automatic&amp;gt;" />
              <Pull_enable v="&amp;lt;Automatic&amp;gt;" />
            </group>
            <group name="Pin 8: GPIOC4/TA1/CMPB_O/XB_IN6/EWM_OUT_B">
              <Custom_name__Signal_name v="GPIOC4/TA1/CMPB_O/XB_IN6/EWM_OUT_B" />
              <Slew_rate v="&amp;lt;Automatic&amp;gt;" />
              <Open_drain v="&amp;lt;Automatic&amp;gt;" />
              <Drive_strength v="&amp;lt;Automatic&amp;gt;" />
              <Pull_select v="&amp;lt;Automatic&amp;gt;" />
              <Pull_enable v="&amp;lt;Automatic&amp;gt;" />
            </group>
            <group name="Pin 9: GPIOA7/ANA7/CMPD_IN3">
              <Custom_name__Signal_name v="GPIOA7/ANA7/CMPD_IN3" />
              <Slew_rate v="&amp;lt;Automatic&amp;gt;" />
              <Open_drain v="&amp;lt;Automatic&amp;gt;" />
              <Drive_strength v="&amp;lt;Automatic&amp;gt;" />
              <Pull_select v="&amp;lt;Automatic&amp;gt;" />
              <Pull_enable v="&amp;lt;Automatic&amp;gt;" />
            </group>
            <group name="Pin 10: GPIOA6/ANA6/CMPD_IN2">
              <Custom_name__Signal_name v="GPIOA6/ANA6/CMPD_IN2" />
              <Slew_rate v="&amp;lt;Automatic&amp;gt;" />
              <Open_drain v="&amp;lt;Automatic&amp;gt;" />
              <Drive_strength v="&amp;lt;Automatic&amp;gt;" />
              <Pull_select v="&amp;lt;Automatic&amp;gt;" />
              <Pull_enable v="&amp;lt;Automatic&amp;gt;" />
            </group>
            <group name="Pin 11: GPIOA5/ANA5/CMPD_IN1">
              <Custom_name__Signal_name v="GPIOA5/ANA5/CMPD_IN1" />
              <Slew_rate v="&amp;lt;Automatic&amp;gt;" />
              <Open_drain v="&amp;lt;Automatic&amp;gt;" />
              <Drive_strength v="&amp;lt;Automatic&amp;gt;" />
              <Pull_select v="&amp;lt;Automatic&amp;gt;" />
              <Pull_enable v="&amp;lt;Automatic&amp;gt;" />
            </group>
            <group name="Pin 12: GPIOA4/ANA4/CMPD_IN0">
              <Custom_name__Signal_name v="GPIOA4/ANA4/CMPD_IN0" />
              <Slew_rate v="&amp;lt;Automatic&amp;gt;" />
              <Open_drain v="&amp;lt;Automatic&amp;gt;" />
              <Drive_strength v="&amp;lt;Automatic&amp;gt;" />
              <Pull_select v="&amp;lt;Automatic&amp;gt;" />
              <Pull_enable v="&amp;lt;Automatic&amp;gt;" />
            </group>
            <group name="Pin 13: GPIOA0/ANA0/CMPA_IN3/CMPC_O">
              <Custom_name__Signal_name v="GPIOA0/ANA0/CMPA_IN3/CMPC_O" />
              <Slew_rate v="&amp;lt;Automatic&amp;gt;" />
              <Open_drain v="&amp;lt;Automatic&amp;gt;" />
              <Drive_strength v="&amp;lt;Automatic&amp;gt;" />
              <Pull_select v="&amp;lt;Automatic&amp;gt;" />
              <Pull_enable v="&amp;lt;Automatic&amp;gt;" />
            </group>
            <group name="Pin 14: GPIOA1/ANA1/CMPA_IN0">
              <Custom_name__Signal_name v="GPIOA1/ANA1/CMPA_IN0" />
              <Slew_rate v="&amp;lt;Automatic&amp;gt;" />
              <Open_drain v="&amp;lt;Automatic&amp;gt;" />
              <Drive_strength v="&amp;lt;Automatic&amp;gt;" />
              <Pull_select v="&amp;lt;Automatic&amp;gt;" />
              <Pull_enable v="&amp;lt;Automatic&amp;gt;" />
            </group>
            <group name="Pin 15: GPIOA2/ANA2/VREFHA/CMPA_IN1">
              <Custom_name__Signal_name v="GPIOA2/ANA2/VREFHA/CMPA_IN1" />
              <Slew_rate v="&amp;lt;Automatic&amp;gt;" />
              <Open_drain v="&amp;lt;Automatic&amp;gt;" />
              <Drive_strength v="&amp;lt;Automatic&amp;gt;" />
              <Pull_select v="&amp;lt;Automatic&amp;gt;" />
              <Pull_enable v="&amp;lt;Automatic&amp;gt;" />
            </group>
            <group name="Pin 16: GPIOA3/ANA3/VREFLA/CMPA_IN2">
              <Custom_name__Signal_name v="GPIOA3/ANA3/VREFLA/CMPA_IN2" />
              <Slew_rate v="&amp;lt;Automatic&amp;gt;" />
              <Open_drain v="&amp;lt;Automatic&amp;gt;" />
              <Drive_strength v="&amp;lt;Automatic&amp;gt;" />
              <Pull_select v="&amp;lt;Automatic&amp;gt;" />
              <Pull_enable v="&amp;lt;Automatic&amp;gt;" />
            </group>
            <group name="Pin 17: GPIOB7/ANB7/CMPB_IN2">
              <Custom_name__Signal_name v="GPIOB7/ANB7/CMPB_IN2" />
              <Slew_rate v="&amp;lt;Automatic&amp;gt;" />
              <Open_drain v="&amp;lt;Automatic&amp;gt;" />
              <Drive_strength v="&amp;lt;Automatic&amp;gt;" />
              <Pull_select v="&amp;lt;Automatic&amp;gt;" />
              <Pull_enable v="&amp;lt;Automatic&amp;gt;" />
            </group>
            <group name="Pin 18: GPIOC5/DACA_O/XB_IN7">
              <Custom_name__Signal_name v="GPIOC5/DACA_O/XB_IN7" />
              <Slew_rate v="&amp;lt;Automatic&amp;gt;" />
              <Open_drain v="&amp;lt;Automatic&amp;gt;" />
              <Drive_strength v="&amp;lt;Automatic&amp;gt;" />
              <Pull_select v="&amp;lt;Automatic&amp;gt;" />
              <Pull_enable v="&amp;lt;Automatic&amp;gt;" />
            </group>
            <group name="Pin 19: GPIOB6/ANB6/CMPB_IN1">
              <Custom_name__Signal_name v="GPIOB6/ANB6/CMPB_IN1" />
              <Slew_rate v="&amp;lt;Automatic&amp;gt;" />
              <Open_drain v="&amp;lt;Automatic&amp;gt;" />
              <Drive_strength v="&amp;lt;Automatic&amp;gt;" />
              <Pull_select v="&amp;lt;Automatic&amp;gt;" />
              <Pull_enable v="&amp;lt;Automatic&amp;gt;" />
            </group>
            <group name="Pin 20: GPIOB5/ANB5/CMPC_IN2">
              <Custom_name__Signal_name v="GPIOB5/ANB5/CMPC_IN2" />
              <Slew_rate v="&amp;lt;Automatic&amp;gt;" />
              <Open_drain v="&amp;lt;Automatic&amp;gt;" />
              <Drive_strength v="&amp;lt;Automatic&amp;gt;" />
              <Pull_select v="&amp;lt;Automatic&amp;gt;" />
              <Pull_enable v="&amp;lt;Automatic&amp;gt;" />
            </group>
            <group name="Pin 21: GPIOB4/ANB4/CMPC_IN1">
              <Custom_name__Signal_name v="GPIOB4/ANB4/CMPC_IN1" />
              <Slew_rate v="&amp;lt;Automatic&amp;gt;" />
              <Open_drain v="&amp;lt;Automatic&amp;gt;" />
              <Drive_strength v="&amp;lt;Automatic&amp;gt;" />
              <Pull_select v="&amp;lt;Automatic&amp;gt;" />
              <Pull_enable v="&amp;lt;Automatic&amp;gt;" />
            </group>
            <group name="Pin 22: VDDA">
              <Custom_name__Signal_name v="VDDA" />
            </group>
            <group name="Pin 23: VSSA">
              <Custom_name__Signal_name v="VSSA" />
            </group>
            <group name="Pin 24: GPIOB0/ANB0/CMPB_IN3">
              <Custom_name__Signal_name v="GPIOB0/ANB0/CMPB_IN3" />
              <Slew_rate v="&amp;lt;Automatic&amp;gt;" />
              <Open_drain v="&amp;lt;Automatic&amp;gt;" />
              <Drive_strength v="&amp;lt;Automatic&amp;gt;" />
              <Pull_select v="&amp;lt;Automatic&amp;gt;" />
              <Pull_enable v="&amp;lt;Automatic&amp;gt;" />
            </group>
            <group name="Pin 25: GPIOB1/ANB1/CMPB_IN0/DACB_O">
              <Custom_name__Signal_name v="GPIOB1/ANB1/CMPB_IN0/DACB_O" />
              <Slew_rate v="&amp;lt;Automatic&amp;gt;" />
              <Open_drain v="&amp;lt;Automatic&amp;gt;" />
              <Drive_strength v="&amp;lt;Automatic&amp;gt;" />
              <Pull_select v="&amp;lt;Automatic&amp;gt;" />
              <Pull_enable v="&amp;lt;Automatic&amp;gt;" />
            </group>
            <group name="Pin 26: VCAP_26">
              <Custom_name__Signal_name v="VCAP_26" />
            </group>
            <group name="Pin 27: GPIOB2/ANB2/VREFHB/CMPC_IN3">
              <Custom_name__Signal_name v="GPIOB2/ANB2/VREFHB/CMPC_IN3" />
              <Slew_rate v="&amp;lt;Automatic&amp;gt;" />
              <Open_drain v="&amp;lt;Automatic&amp;gt;" />
              <Drive_strength v="&amp;lt;Automatic&amp;gt;" />
              <Pull_select v="&amp;lt;Automatic&amp;gt;" />
              <Pull_enable v="&amp;lt;Automatic&amp;gt;" />
            </group>
            <group name="Pin 28: GPIOB3/ANB3/VREFLB/CMPC_IN0">
              <Custom_name__Signal_name v="GPIOB3/ANB3/VREFLB/CMPC_IN0" />
              <Slew_rate v="&amp;lt;Automatic&amp;gt;" />
              <Open_drain v="&amp;lt;Automatic&amp;gt;" />
              <Drive_strength v="&amp;lt;Automatic&amp;gt;" />
              <Pull_select v="&amp;lt;Automatic&amp;gt;" />
              <Pull_enable v="&amp;lt;Automatic&amp;gt;" />
            </group>
            <group name="Pin 29: VDD_29">
              <Custom_name__Signal_name v="VDD_29" />
            </group>
            <group name="Pin 30: VSS_30">
              <Custom_name__Signal_name v="VSS_30" />
            </group>
            <group name="Pin 31: GPIOC6/TA2/XB_IN3/CMP_REF/SS0_B">
              <Custom_name__Signal_name v="GPIOC6/TA2/XB_IN3/CMP_REF/SS0_B" />
              <Slew_rate v="&amp;lt;Automatic&amp;gt;" />
              <Open_drain v="&amp;lt;Automatic&amp;gt;" />
              <Drive_strength v="&amp;lt;Automatic&amp;gt;" />
              <Pull_select v="&amp;lt;Automatic&amp;gt;" />
              <Pull_enable v="&amp;lt;Automatic&amp;gt;" />
            </group>
            <group name="Pin 32: GPIOC7/SS0_B/TXD0/XB_IN8">
              <Custom_name__Signal_name v="GPIOC7/SS0_B/TXD0/XB_IN8" />
              <Slew_rate v="&amp;lt;Automatic&amp;gt;" />
              <Open_drain v="&amp;lt;Automatic&amp;gt;" />
              <Drive_strength v="&amp;lt;Automatic&amp;gt;" />
              <Pull_select v="&amp;lt;Automatic&amp;gt;" />
              <Pull_enable v="&amp;lt;Automatic&amp;gt;" />
            </group>
            <group name="Pin 33: GPIOC8/MISO0/RXD0/XB_IN9/XB_OUT6">
              <Custom_name__Signal_name v="GPIOC8/MISO0/RXD0/XB_IN9/XB_OUT6" />
              <Slew_rate v="&amp;lt;Automatic&amp;gt;" />
              <Open_drain v="&amp;lt;Automatic&amp;gt;" />
              <Drive_strength v="&amp;lt;Automatic&amp;gt;" />
              <Pull_select v="&amp;lt;Automatic&amp;gt;" />
              <Pull_enable v="&amp;lt;Automatic&amp;gt;" />
            </group>
            <group name="Pin 34: GPIOC9/SCK0/XB_IN4/TXD0/XB_OUT8">
              <Custom_name__Signal_name v="GPIOC9/SCK0/XB_IN4/TXD0/XB_OUT8" />
              <Slew_rate v="&amp;lt;Automatic&amp;gt;" />
              <Open_drain v="&amp;lt;Automatic&amp;gt;" />
              <Drive_strength v="&amp;lt;Automatic&amp;gt;" />
              <Pull_select v="&amp;lt;Automatic&amp;gt;" />
              <Pull_enable v="&amp;lt;Automatic&amp;gt;" />
            </group>
            <group name="Pin 35: GPIOC10/MOSI0/XB_IN5/MISO0/XB_OUT9">
              <Custom_name__Signal_name v="GPIOC10/MOSI0/XB_IN5/MISO0/XB_OUT9" />
              <Slew_rate v="&amp;lt;Automatic&amp;gt;" />
              <Open_drain v="&amp;lt;Automatic&amp;gt;" />
              <Drive_strength v="&amp;lt;Automatic&amp;gt;" />
              <Pull_select v="&amp;lt;Automatic&amp;gt;" />
              <Pull_enable v="&amp;lt;Automatic&amp;gt;" />
            </group>
            <group name="Pin 36: GPIOF0/XB_IN6/SCK1">
              <Custom_name__Signal_name v="GPIOF0/XB_IN6/SCK1" />
              <Slew_rate v="&amp;lt;Automatic&amp;gt;" />
              <Open_drain v="&amp;lt;Automatic&amp;gt;" />
              <Drive_strength v="&amp;lt;Automatic&amp;gt;" />
              <Pull_select v="&amp;lt;Automatic&amp;gt;" />
              <Pull_enable v="&amp;lt;Automatic&amp;gt;" />
            </group>
            <group name="Pin 37: GPIOC11/CANTX/SCL0/TXD1">
              <Custom_name__Signal_name v="GPIOC11/CANTX/SCL0/TXD1" />
              <Slew_rate v="&amp;lt;Automatic&amp;gt;" />
              <Open_drain v="&amp;lt;Automatic&amp;gt;" />
              <Drive_strength v="&amp;lt;Automatic&amp;gt;" />
              <Pull_select v="&amp;lt;Automatic&amp;gt;" />
              <Pull_enable v="&amp;lt;Automatic&amp;gt;" />
            </group>
            <group name="Pin 38: GPIOC12/CANRX/SDA0/RXD1">
              <Custom_name__Signal_name v="GPIOC12/CANRX/SDA0/RXD1" />
              <Slew_rate v="&amp;lt;Automatic&amp;gt;" />
              <Open_drain v="&amp;lt;Automatic&amp;gt;" />
              <Drive_strength v="&amp;lt;Automatic&amp;gt;" />
              <Pull_select v="&amp;lt;Automatic&amp;gt;" />
              <Pull_enable v="&amp;lt;Automatic&amp;gt;" />
            </group>
            <group name="Pin 39: GPIOF2/SCL0/XB_OUT6/MISO1">
              <Custom_name__Signal_name v="GPIOF2/SCL0/XB_OUT6/MISO1" />
              <Slew_rate v="&amp;lt;Automatic&amp;gt;" />
              <Open_drain v="&amp;lt;Automatic&amp;gt;" />
              <Drive_strength v="&amp;lt;Automatic&amp;gt;" />
              <Pull_select v="&amp;lt;Automatic&amp;gt;" />
              <Pull_enable v="&amp;lt;Automatic&amp;gt;" />
            </group>
            <group name="Pin 40: GPIOF3/SDA0/XB_OUT7/MOSI1">
              <Custom_name__Signal_name v="GPIOF3/SDA0/XB_OUT7/MOSI1" />
              <Slew_rate v="&amp;lt;Automatic&amp;gt;" />
              <Open_drain v="&amp;lt;Automatic&amp;gt;" />
              <Drive_strength v="&amp;lt;Automatic&amp;gt;" />
              <Pull_select v="&amp;lt;Automatic&amp;gt;" />
              <Pull_enable v="&amp;lt;Automatic&amp;gt;" />
            </group>
            <group name="Pin 41: GPIOF4/TXD1/XB_OUT8/PWM_0X/PWM_FAULT6">
              <Custom_name__Signal_name v="GPIOF4/TXD1/XB_OUT8/PWM_0X/PWM_FAULT6" />
              <Slew_rate v="&amp;lt;Automatic&amp;gt;" />
              <Open_drain v="&amp;lt;Automatic&amp;gt;" />
              <Drive_strength v="&amp;lt;Automatic&amp;gt;" />
              <Pull_select v="&amp;lt;Automatic&amp;gt;" />
              <Pull_enable v="&amp;lt;Automatic&amp;gt;" />
            </group>
            <group name="Pin 42: GPIOF5/RXD1/XB_OUT9/PWM_1X/PWM_FAULT7">
              <Custom_name__Signal_name v="GPIOF5/RXD1/XB_OUT9/PWM_1X/PWM_FAULT7" />
              <Slew_rate v="&amp;lt;Automatic&amp;gt;" />
              <Open_drain v="&amp;lt;Automatic&amp;gt;" />
              <Drive_strength v="&amp;lt;Automatic&amp;gt;" />
              <Pull_select v="&amp;lt;Automatic&amp;gt;" />
              <Pull_enable v="&amp;lt;Automatic&amp;gt;" />
            </group>
            <group name="Pin 43: VSS_43">
              <Custom_name__Signal_name v="VSS_43" />
            </group>
            <group name="Pin 44: VDD_44">
              <Custom_name__Signal_name v="VDD_44" />
            </group>
            <group name="Pin 45: GPIOE0/PWM_0B">
              <Custom_name__Signal_name v="GPIOE0/PWM_0B" />
              <Slew_rate v="&amp;lt;Automatic&amp;gt;" />
              <Open_drain v="&amp;lt;Automatic&amp;gt;" />
              <Drive_strength v="&amp;lt;Automatic&amp;gt;" />
              <Pull_select v="&amp;lt;Automatic&amp;gt;" />
              <Pull_enable v="&amp;lt;Automatic&amp;gt;" />
            </group>
            <group name="Pin 46: GPIOE1/PWM_0A">
              <Custom_name__Signal_name v="GPIOE1/PWM_0A" />
              <Slew_rate v="&amp;lt;Automatic&amp;gt;" />
              <Open_drain v="&amp;lt;Automatic&amp;gt;" />
              <Drive_strength v="&amp;lt;Automatic&amp;gt;" />
              <Pull_select v="&amp;lt;Automatic&amp;gt;" />
              <Pull_enable v="&amp;lt;Automatic&amp;gt;" />
            </group>
            <group name="Pin 47: GPIOE2/PWM_1B">
              <Custom_name__Signal_name v="GPIOE2/PWM_1B" />
              <Slew_rate v="&amp;lt;Automatic&amp;gt;" />
              <Open_drain v="&amp;lt;Automatic&amp;gt;" />
              <Drive_strength v="&amp;lt;Automatic&amp;gt;" />
              <Pull_select v="&amp;lt;Automatic&amp;gt;" />
              <Pull_enable v="&amp;lt;Automatic&amp;gt;" />
            </group>
            <group name="Pin 48: GPIOE3/PWM_1A">
              <Custom_name__Signal_name v="GPIOE3/PWM_1A" />
              <Slew_rate v="&amp;lt;Automatic&amp;gt;" />
              <Open_drain v="&amp;lt;Automatic&amp;gt;" />
              <Drive_strength v="&amp;lt;Automatic&amp;gt;" />
              <Pull_select v="&amp;lt;Automatic&amp;gt;" />
              <Pull_enable v="&amp;lt;Automatic&amp;gt;" />
            </group>
            <group name="Pin 49: GPIOC13/TA3/XB_IN6/EWM_OUT_B">
              <Custom_name__Signal_name v="GPIOC13/TA3/XB_IN6/EWM_OUT_B" />
              <Slew_rate v="&amp;lt;Automatic&amp;gt;" />
              <Open_drain v="&amp;lt;Automatic&amp;gt;" />
              <Drive_strength v="&amp;lt;Automatic&amp;gt;" />
              <Pull_select v="&amp;lt;Automatic&amp;gt;" />
              <Pull_enable v="&amp;lt;Automatic&amp;gt;" />
            </group>
            <group name="Pin 50: GPIOF1/CLKO1/XB_IN7/CMPD_O">
              <Custom_name__Signal_name v="GPIOF1/CLKO1/XB_IN7/CMPD_O" />
              <Slew_rate v="&amp;lt;Automatic&amp;gt;" />
              <Open_drain v="&amp;lt;Automatic&amp;gt;" />
              <Drive_strength v="&amp;lt;Automatic&amp;gt;" />
              <Pull_select v="&amp;lt;Automatic&amp;gt;" />
              <Pull_enable v="&amp;lt;Automatic&amp;gt;" />
            </group>
            <group name="Pin 51: GPIOE4/PWM_2B/XB_IN2">
              <Custom_name__Signal_name v="GPIOE4/PWM_2B/XB_IN2" />
              <Slew_rate v="&amp;lt;Automatic&amp;gt;" />
              <Open_drain v="&amp;lt;Automatic&amp;gt;" />
              <Drive_strength v="&amp;lt;Automatic&amp;gt;" />
              <Pull_select v="&amp;lt;Automatic&amp;gt;" />
              <Pull_enable v="&amp;lt;Automatic&amp;gt;" />
            </group>
            <group name="Pin 52: GPIOE5/PWM_2A/XB_IN3">
              <Custom_name__Signal_name v="GPIOE5/PWM_2A/XB_IN3" />
              <Slew_rate v="&amp;lt;Automatic&amp;gt;" />
              <Open_drain v="&amp;lt;Automatic&amp;gt;" />
              <Drive_strength v="&amp;lt;Automatic&amp;gt;" />
              <Pull_select v="&amp;lt;Automatic&amp;gt;" />
              <Pull_enable v="&amp;lt;Automatic&amp;gt;" />
            </group>
            <group name="Pin 53: GPIOE6/PWM_3B/XB_IN4">
              <Custom_name__Signal_name v="GPIOE6/PWM_3B/XB_IN4" />
              <Slew_rate v="&amp;lt;Automatic&amp;gt;" />
              <Open_drain v="&amp;lt;Automatic&amp;gt;" />
              <Drive_strength v="&amp;lt;Automatic&amp;gt;" />
              <Pull_select v="&amp;lt;Automatic&amp;gt;" />
              <Pull_enable v="&amp;lt;Automatic&amp;gt;" />
            </group>
            <group name="Pin 54: GPIOE7/PWM_3A/XB_IN5">
              <Custom_name__Signal_name v="GPIOE7/PWM_3A/XB_IN5" />
              <Slew_rate v="&amp;lt;Automatic&amp;gt;" />
              <Open_drain v="&amp;lt;Automatic&amp;gt;" />
              <Drive_strength v="&amp;lt;Automatic&amp;gt;" />
              <Pull_select v="&amp;lt;Automatic&amp;gt;" />
              <Pull_enable v="&amp;lt;Automatic&amp;gt;" />
            </group>
            <group name="Pin 55: GPIOC14/SDA0/XB_OUT4/PWM_FAULT4">
              <Custom_name__Signal_name v="GPIOC14/SDA0/XB_OUT4/PWM_FAULT4" />
              <Slew_rate v="&amp;lt;Automatic&amp;gt;" />
              <Open_drain v="&amp;lt;Automatic&amp;gt;" />
              <Drive_strength v="&amp;lt;Automatic&amp;gt;" />
              <Pull_select v="&amp;lt;Automatic&amp;gt;" />
              <Pull_enable v="&amp;lt;Automatic&amp;gt;" />
            </group>
            <group name="Pin 56: GPIOC15/SCL0/XB_OUT5/PWM_FAULT5">
              <Custom_name__Signal_name v="GPIOC15/SCL0/XB_OUT5/PWM_FAULT5" />
              <Slew_rate v="&amp;lt;Automatic&amp;gt;" />
              <Open_drain v="&amp;lt;Automatic&amp;gt;" />
              <Drive_strength v="&amp;lt;Automatic&amp;gt;" />
              <Pull_select v="&amp;lt;Automatic&amp;gt;" />
              <Pull_enable v="&amp;lt;Automatic&amp;gt;" />
            </group>
            <group name="Pin 57: VCAP_57">
              <Custom_name__Signal_name v="VCAP_57" />
            </group>
            <group name="Pin 58: GPIOF6/PWM_3X/XB_IN2">
              <Custom_name__Signal_name v="GPIOF6/PWM_3X/XB_IN2" />
              <Slew_rate v="&amp;lt;Automatic&amp;gt;" />
              <Open_drain v="&amp;lt;Automatic&amp;gt;" />
              <Drive_strength v="&amp;lt;Automatic&amp;gt;" />
              <Pull_select v="&amp;lt;Automatic&amp;gt;" />
              <Pull_enable v="&amp;lt;Automatic&amp;gt;" />
            </group>
            <group name="Pin 59: GPIOF7/CMPC_O/SS1_B/XB_IN3">
              <Custom_name__Signal_name v="GPIOF7/CMPC_O/SS1_B/XB_IN3" />
              <Slew_rate v="&amp;lt;Automatic&amp;gt;" />
              <Open_drain v="&amp;lt;Automatic&amp;gt;" />
              <Drive_strength v="&amp;lt;Automatic&amp;gt;" />
              <Pull_select v="&amp;lt;Automatic&amp;gt;" />
              <Pull_enable v="&amp;lt;Automatic&amp;gt;" />
            </group>
            <group name="Pin 60: VDD_60">
              <Custom_name__Signal_name v="VDD_60" />
            </group>
            <group name="Pin 61: VSS_61">
              <Custom_name__Signal_name v="VSS_61" />
            </group>
            <group name="Pin 62: TDO/GPIOD1">
              <Custom_name__Signal_name v="TDO/GPIOD1" />
              <Slew_rate v="&amp;lt;Automatic&amp;gt;" />
              <Open_drain v="&amp;lt;Automatic&amp;gt;" />
              <Drive_strength v="&amp;lt;Automatic&amp;gt;" />
              <Pull_select v="&amp;lt;Automatic&amp;gt;" />
              <Pull_enable v="&amp;lt;Automatic&amp;gt;" />
            </group>
            <group name="Pin 63: TMS/GPIOD3">
              <Custom_name__Signal_name v="TMS/GPIOD3" />
              <Slew_rate v="&amp;lt;Automatic&amp;gt;" />
              <Open_drain v="&amp;lt;Automatic&amp;gt;" />
              <Drive_strength v="&amp;lt;Automatic&amp;gt;" />
              <Pull_select v="&amp;lt;Automatic&amp;gt;" />
              <Pull_enable v="&amp;lt;Automatic&amp;gt;" />
            </group>
            <group name="Pin 64: TDI/GPIOD0">
              <Custom_name__Signal_name v="TDI/GPIOD0" />
              <Slew_rate v="&amp;lt;Automatic&amp;gt;" />
              <Open_drain v="&amp;lt;Automatic&amp;gt;" />
              <Drive_strength v="&amp;lt;Automatic&amp;gt;" />
              <Pull_select v="&amp;lt;Automatic&amp;gt;" />
              <Pull_enable v="&amp;lt;Automatic&amp;gt;" />
            </group>
          </group>
        </group>
      </list>
    </Properties>
    <Methods>
      <list name="ProcessorSpecificMethods" v="1">
        <Init v="don&amp;apos;t generate code" />
      </list>
    </Methods>
    <Events>
      <EmptySection_DummyValue />
    </Events>
  </Bean>
  <Bean name="GPIOE0" type="BitIO">
    <Enabled v="Y" />
    <Properties>
      <Component_name v="GPIOE0" />
      <Pin_for_I_O v="GPIOE0/PWM_0B" />
      <inhrbean type="BitIO_LDD">
        <Enabled v="Y" />
        <Template v="BitIO_LDD" />
        <Properties>
          <Component_name v="BitIoLdd1" />
          <Pin_for_I_O v="GPIOE0/PWM_0B" />
          <Direction v="Output" />
          <group name="Initialization">
            <Init__direction v="Output" />
            <Init__value v="0" />
            <Auto_initialization v="yes" />
          </group>
          <Safe_mode v="yes" />
          <Optimization_for v="speed" />
        </Properties>
        <Methods>
          <Init v="generate code" />
          <Deinit v="don&amp;apos;t generate code" />
          <GetDir v="don&amp;apos;t generate code" />
          <SetDir v="don&amp;apos;t generate code" />
          <SetInput v="don&amp;apos;t generate code" />
          <SetOutput v="don&amp;apos;t generate code" />
          <GetVal v="generate code" />
          <PutVal v="generate code" />
          <ClrVal v="generate code" />
          <SetVal v="generate code" />
          <NegVal v="don&amp;apos;t generate code" />
          <ConnectPin v="don&amp;apos;t generate code" />
          <GetRawVal v="don&amp;apos;t generate code" />
        </Methods>
        <Events>
          <EmptySection_DummyValue />
        </Events>
      </inhrbean>
      <Direction v="Output" />
      <group name="Initialization">
        <Init__direction v="Output" />
        <Init__value v="0" />
      </group>
      <Safe_mode v="yes" />
      <Optimization_for v="speed" />
    </Properties>
    <Methods>
      <GetDir v="don&amp;apos;t generate code" />
      <SetDir v="don&amp;apos;t generate code" />
      <SetInput v="don&amp;apos;t generate code" />
      <SetOutput v="don&amp;apos;t generate code" />
      <GetVal v="generate code" />
      <PutVal v="generate code" />
      <ClrVal v="generate code" />
      <SetVal v="generate code" />
      <NegVal v="don&amp;apos;t generate code" />
      <ConnectPin v="don&amp;apos;t generate code" />
      <GetRawVal v="don&amp;apos;t generate code" />
    </Methods>
    <Events>
      <EmptySection_DummyValue />
    </Events>
  </Bean>
  <Bean name="TU1" type="TimerUnit_LDD">
    <Enabled v="Y" />
    <Properties>
      <Component_name v="TU1" />
      <Module_name v="PIT0" />
      <Counter v="PIT0_CNTR" />
      <Counter_direction v="Up" />
      <Counter_width v="16 bits" />
      <Value_type v="Optimal" />
      <enumgroup name="Input clock source" v="Internal">
        <Counter_frequency v="Auto select" />
      </enumgroup>
      <enumgroup name="Counter restart" v="On-match">
        <Period_device v="PIT0_MOD" />
        <Period v="100 kHz" />
        <boolgroup name="Interrupt" v="Disabled" />
      </enumgroup>
      <list name="Channel list" v="0">
        <EmptySection_DummyValue />
      </list>
      <group name="Initialization">
        <Enabled_in_init__code v="yes" />
        <list name="Auto Initialization" v="1">
          <Auto_initialization v="no" />
        </list>
        <group name="Event mask">
          <OnCounterRestart v="Disabled" />
          <OnChannel0 v="Disabled" />
          <OnChannel1 v="Disabled" />
          <OnChannel2 v="Disabled" />
          <OnChannel3 v="Disabled" />
          <OnChannel4 v="Disabled" />
          <OnChannel5 v="Disabled" />
          <OnChannel6 v="Disabled" />
          <OnChannel7 v="Disabled" />
        </group>
      </group>
      <list name="CPU clock/configuration selection (included)" v="1">
        <group name="CPU clock/configuration selection">
          <Clock_configuration_0 v="This component enabled" />
          <Clock_configuration_1 v="This component disabled" />
          <Clock_configuration_2 v="This component disabled" />
          <Clock_configuration_3 v="This component disabled" />
          <Clock_configuration_4 v="This component disabled" />
          <Clock_configuration_5 v="This component disabled" />
          <Clock_configuration_6 v="This component disabled" />
          <Clock_configuration_7 v="This component disabled" />
        </group>
      </list>
    </Properties>
    <Methods>
      <Init v="generate code" />
      <Deinit v="don&amp;apos;t generate code" />
      <Enable v="don&amp;apos;t generate code" />
      <Disable v="don&amp;apos;t generate code" />
      <SetEventMask v="don&amp;apos;t generate code" />
      <GetEventMask v="don&amp;apos;t generate code" />
      <GetEventStatus v="don&amp;apos;t generate code" />
      <SelectInputFrequency v="don&amp;apos;t generate code" />
      <GetInputFrequencyReal v="don&amp;apos;t generate code" />
      <GetInputFrequency v="don&amp;apos;t generate code" />
      <SetPeriodTicks v="don&amp;apos;t generate code" />
      <GetPeriodTicks v="don&amp;apos;t generate code" />
      <ResetCounter v="don&amp;apos;t generate code" />
      <GetCounterValue v="don&amp;apos;t generate code" />
      <SetOffsetTicks v="don&amp;apos;t generate code" />
      <GetOffsetTicks v="don&amp;apos;t generate code" />
      <GetCaptureValue v="don&amp;apos;t generate code" />
      <SelectOutputAction v="don&amp;apos;t generate code" />
      <SelectCaptureEdge v="don&amp;apos;t generate code" />
      <ConnectPin v="don&amp;apos;t generate code" />
      <SetOperationMode v="don&amp;apos;t generate code" />
      <GetDriverState v="don&amp;apos;t generate code" />
    </Methods>
    <Events>
      <Event_module_name v="Events" />
      <event name="OnCounterRestart" v="don&amp;apos;t generate code" />
      <event name="OnChannel0" v="don&amp;apos;t generate code" />
      <event name="OnChannel1" v="don&amp;apos;t generate code" />
      <event name="OnChannel2" v="don&amp;apos;t generate code" />
      <event name="OnChannel3" v="don&amp;apos;t generate code" />
      <event name="OnChannel4" v="don&amp;apos;t generate code" />
      <event name="OnChannel5" v="don&amp;apos;t generate code" />
      <event name="OnChannel6" v="don&amp;apos;t generate code" />
      <event name="OnChannel7" v="don&amp;apos;t generate code" />
    </Events>
  </Bean>
  <Bean name="PWMA" type="Init_eFlexPWM">
    <Enabled v="Y" />
    <Properties>
      <Component_name v="PWMA" />
      <Device v="PWMA" />
      <group name="Settings">
        <boolgroup name="Submodule 0" v="Enabled">
          <group name="Clock setting">
            <PWM_clock_source v="IP Bus clock" />
            <PWM_generator_clock v="Enabled" />
            <PWM_prescaler v="1" />
            <Module_clock v="100 MHz" />
            <Init_counter_value v="1" />
            <PWM_value_0___half_cycle_point v="0" />
            <PWM_value_1___counter_modulo v="1000" />
            <Fractional_circuit_power_up v="Disabled" />
            <Fractional_value_1_circuit v="Disabled" />
            <Fractional_value_1 v="0" />
            <Dead_time_value_0 v="0" />
            <Dead_time_value_1 v="0" />
            <PWM_frequency v="100.0000 kHz" />
            <PWM_period v="10.0000 us" />
            <PWM_dead_time_0 v="0" />
            <PWM_dead_time_1 v="0" />
          </group>
          <Enabled_in_Wait_mode v="no" />
          <Enabled_in_Debug_mode v="no" />
          <group name="Channel settings">
            <Mode_of_PWM_ch_A_and_B v="Complementary" />
            <Complementary_PWM_source v="PWM23" />
            <Double_switching v="Disabled" />
            <Split_DBLPWM_to_channel_A_and_B v="Disabled" />
            <group name="Channel A (PWM23)">
              <group name="PWM function">
                <PWM_value_2 v="500" />
                <Fractional_value_2_and_3_circuit v="Disabled" />
                <Fractional_value_2 v="0" />
                <PWM_value_3 v="1000" />
                <Fractional_value_3 v="0" />
                <SW_output v="Logic 0" />
                <Deadtime_source v="Generated PWM" />
                <Output_fault_state v="Forced to 0 prior to output polarity" />
                <Output_polarity v="Not inverted" />
                <Channel_masked v="no" />
                <Channel_output v="Enabled" />
                <group name="Fault channel 0">
                  <Disable_by_fault_0 v="no" />
                  <Disable_by_fault_1 v="no" />
                  <Disable_by_fault_2 v="no" />
                  <Disable_by_fault_3 v="no" />
                </group>
                <group name="Fault channel 1">
                  <Disable_by_fault_0 v="no" />
                  <Disable_by_fault_1 v="no" />
                  <Disable_by_fault_2 v="no" />
                  <Disable_by_fault_3 v="no" />
                </group>
              </group>
              <group name="E-capture function">
                <FIFOs_water_mark_level v="0" />
                <Edge_counter v="Disabled" />
                <Edge_compare v="0" />
                <Input_select_A v="Raw PWMA input signal" />
                <Capture_0_circuitry v="Disabled" />
                <Capture_1_circuitry v="Disabled" />
                <Capture_circuitry_mode v="Free running" />
                <Input_capture_process v="Disabled" />
              </group>
            </group>
            <group name="Channel B (PWM45)">
              <group name="PWM function">
                <PWM_value_4 v="0" />
                <Fractional_value_4_and_5_circuit v="Disabled" />
                <Fractional_value_4 v="0" />
                <PWM_value_5 v="0" />
                <Fractional_value_5 v="0" />
                <SW_output v="Logic 0" />
                <Deadtime_source v="Generated PWM" />
                <Output_fault_state v="Forced to 0 prior to output polarity" />
                <Output_polarity v="Not inverted" />
                <Channel_masked v="no" />
                <Channel_output v="Disabled" />
                <group name="Fault channel 0">
                  <Disable_by_fault_0 v="yes" />
                  <Disable_by_fault_1 v="yes" />
                  <Disable_by_fault_2 v="yes" />
                  <Disable_by_fault_3 v="yes" />
                </group>
                <group name="Fault channel 1">
                  <Disable_by_fault_0 v="yes" />
                  <Disable_by_fault_1 v="yes" />
                  <Disable_by_fault_2 v="yes" />
                  <Disable_by_fault_3 v="yes" />
                </group>
              </group>
              <group name="E-capture function">
                <FIFOs_water_mark_level v="0" />
                <Edge_counter v="Disabled" />
                <Edge_compare v="0" />
                <Input_select_B v="Raw PWMB input signal" />
                <Capture_0_circuitry v="Disabled" />
                <Capture_1_circuitry v="Disabled" />
                <Capture_circuitry_mode v="Free running" />
                <Input_capture_process v="Disabled" />
              </group>
            </group>
            <group name="Channel X (PWM01)">
              <group name="PWM function">
                <Output_fault_state v="Forced to 0 prior to output polarity" />
                <Output_polarity v="Not inverted" />
                <Channel_masked v="no" />
                <X_Double_switching v="Disabled" />
                <Channel_output v="Disabled" />
                <group name="Fault channel 0">
                  <Disable_by_fault_0 v="yes" />
                  <Disable_by_fault_1 v="yes" />
                  <Disable_by_fault_2 v="yes" />
                  <Disable_by_fault_3 v="yes" />
                </group>
                <group name="Fault channel 1">
                  <Disable_by_fault_0 v="yes" />
                  <Disable_by_fault_1 v="yes" />
                  <Disable_by_fault_2 v="yes" />
                  <Disable_by_fault_3 v="yes" />
                </group>
              </group>
              <group name="E-capture function">
                <FIFOs_water_mark_level v="0" />
                <Edge_counter v="Disabled" />
                <Edge_compare v="0" />
                <Input_select_X v="Raw PWMX input signal" />
                <Capture_0_circuitry v="Disabled" />
                <Capture_1_circuitry v="Disabled" />
                <Capture_circuitry_mode v="Free running" />
                <Input_capture_process v="Disabled" />
              </group>
            </group>
          </group>
          <group name="Output trigger settings">
            <Output_trigger_0_source_select v="OUT_TRIG0 signal" />
            <Output_trigger_1_source_select v="OUT_TRIG1 signal" />
            <group name="OUT_TRIG0 signal settings">
              <Output_trigger_for_Val_0 v="Disabled" />
              <Output_trigger_for_Val_2 v="Disabled" />
              <Output_trigger_for_Val_4 v="Disabled" />
            </group>
            <group name="OUT_TRIG1 signal settings">
              <Output_trigger_for_Val_1 v="Disabled" />
              <Output_trigger_for_Val_3 v="Disabled" />
              <Output_trigger_for_Val_5 v="Disabled" />
            </group>
          </group>
          <group name="Reload settings">
            <Reload_source v="Local reload signal" />
            <Reload_frequency v="1" />
            <Half_cycle_reload v="Disabled" />
            <Full_cycle_reload v="Enabled" />
            <Load_mode v="Load at next PWM reload if LDOK is set" />
          </group>
          <group name="Force and initialization settings">
            <Initialization_source v="Local sync signal" />
            <Force_initialization v="Disabled" />
            <Force_source v="Local force signal" />
            <Init_value_ch_A v="Low" />
            <Init_value_ch_B v="Low" />
            <Init_value_ch_X v="Low" />
          </group>
        </boolgroup>
        <boolgroup name="Submodule 1" v="Disabled" />
        <boolgroup name="Submodule 2" v="Disabled" />
        <boolgroup name="Submodule 3" v="Disabled" />
        <group name="Fault channel 0 protection settings">
          <group name="Common fault settings">
            <boolgroup name="Input filter" v="Disabled" />
            <Fault_Glitch_Stretch v="Disabled" />
          </group>
          <group name="Fault 0">
            <Fault_active_level v="Logic 0" />
            <Fault_clearing_mode v="Manual" />
            <Fault_safety_mode v="Normal" />
            <Half_cycle_recovery v="no" />
            <Full_cycle_recovery v="no" />
          </group>
          <group name="Fault 1">
            <Fault_active_level v="Logic 0" />
            <Fault_clearing_mode v="Manual" />
            <Fault_safety_mode v="Normal" />
            <Half_cycle_recovery v="no" />
            <Full_cycle_recovery v="no" />
          </group>
          <group name="Fault 2">
            <Fault_active_level v="Logic 0" />
            <Fault_clearing_mode v="Manual" />
            <Fault_safety_mode v="Normal" />
            <Half_cycle_recovery v="no" />
            <Full_cycle_recovery v="no" />
          </group>
          <group name="Fault 3">
            <Fault_active_level v="Logic 0" />
            <Fault_clearing_mode v="Manual" />
            <Fault_safety_mode v="Normal" />
            <Half_cycle_recovery v="no" />
            <Full_cycle_recovery v="no" />
          </group>
        </group>
        <group name="Fault channel 1 protection settings">
          <group name="Common fault settings">
            <boolgroup name="Input filter" v="Disabled" />
            <Fault_Glitch_Stretch v="Disabled" />
          </group>
          <group name="Fault 0">
            <Fault_active_level v="Logic 0" />
            <Fault_clearing_mode v="Manual" />
            <Fault_safety_mode v="Normal" />
            <Half_cycle_recovery v="no" />
            <Full_cycle_recovery v="no" />
          </group>
          <group name="Fault 1">
            <Fault_active_level v="Logic 0" />
            <Fault_clearing_mode v="Manual" />
            <Fault_safety_mode v="Normal" />
            <Half_cycle_recovery v="no" />
            <Full_cycle_recovery v="no" />
          </group>
          <group name="Fault 2">
            <Fault_active_level v="Logic 0" />
            <Fault_clearing_mode v="Manual" />
            <Fault_safety_mode v="Normal" />
            <Half_cycle_recovery v="no" />
            <Full_cycle_recovery v="no" />
          </group>
          <group name="Fault 3">
            <Fault_active_level v="Logic 0" />
            <Fault_clearing_mode v="Manual" />
            <Fault_safety_mode v="Normal" />
            <Half_cycle_recovery v="no" />
            <Full_cycle_recovery v="no" />
          </group>
        </group>
      </group>
      <group name="Pins">
        <boolgroup name="SM0 pins" v="Disabled" />
        <boolgroup name="SM1 pins" v="Disabled" />
        <boolgroup name="SM2 pins" v="Disabled" />
        <boolgroup name="SM3 pins" v="Disabled" />
        <group name="PWM Faults">
          <group name="Fault channel 0">
            <boolgroup name="Fault 0" v="Disabled" />
            <boolgroup name="Fault 1" v="Disabled" />
            <boolgroup name="Fault 2" v="Disabled" />
            <boolgroup name="Fault 3" v="Disabled" />
          </group>
          <group name="Fault channel 1">
            <boolgroup name="Fault 4" v="Disabled" />
            <boolgroup name="Fault 5" v="Disabled" />
            <boolgroup name="Fault 6" v="Disabled" />
            <boolgroup name="Fault 7" v="Disabled" />
          </group>
        </group>
        <group name="External clock">
          <boolgroup name="External clock" v="Disabled" />
          <External_clock_frequency v="1" />
        </group>
        <boolgroup name="External force" v="Disabled" />
      </group>
      <group name="Interrupts/DMA">
        <boolgroup name="SM0 Interrupts/DMA" v="Enabled">
          <group name="Compare interrupt">
            <Interrupt v="INT_eFlexPWMA_CMP0" />
            <Interrupt_priority v="&amp;lt;Automatic&amp;gt;" />
            <ISR_Name v="" />
            <Compare_interrupt_0 v="Disabled" />
            <Compare_interrupt_1 v="Disabled" />
            <Compare_interrupt_2 v="Disabled" />
            <Compare_interrupt_3 v="Disabled" />
            <Compare_interrupt_4 v="Disabled" />
            <Compare_interrupt_5 v="Disabled" />
          </group>
          <group name="Capture interrupt">
            <Interrupt v="INT_eFlexPWMA_CAP" />
            <Interrupt_priority v="&amp;lt;Automatic&amp;gt;" />
            <ISR_Name v="" />
            <Capture_A_0_interrupt v="Disabled" />
            <Capture_A_1_interrupt v="Disabled" />
            <Capture_B_0_interrupt v="Disabled" />
            <Capture_B_1_interrupt v="Disabled" />
            <Capture_X_0_interrupt v="Disabled" />
            <Capture_X_1_interrupt v="Disabled" />
          </group>
          <group name="Reload interrupt">
            <Interrupt v="INT_eFlexPWMA_RELOAD0" />
            <Interrupt_priority v="1" />
            <ISR_Name v="PIT_100k_OnInterrupt" />
            <Reload_interrupt v="Enabled" />
          </group>
          <group name="Reload error interrupt">
            <Interrupt v="INT_eFlexPWMA_RERR" />
            <Interrupt_priority v="&amp;lt;Automatic&amp;gt;" />
            <ISR_Name v="" />
            <SM0_reload_error_interrupt v="Disabled" />
          </group>
          <group name="DMA settings">
            <DMA_for_value_registers v="Disabled" />
            <Selected_capture_FIFO_watermarks v="OR&amp;apos;ed together" />
            <Capture_FIFO_read_DMA_request v="Disabled" />
            <Capture_A_0_FIFO_DMA v="Disabled" />
            <Capture_A_1_FIFO_DMA v="Disabled" />
            <Capture_B_0_FIFO_DMA v="Disabled" />
            <Capture_B_1_FIFO_DMA v="Disabled" />
            <Capture_X_0_FIFO_DMA v="Disabled" />
            <Capture_X_1_FIFO_DMA v="Disabled" />
          </group>
        </boolgroup>
        <boolgroup name="SM1 Interrupts/DMA" v="Disabled" />
        <boolgroup name="SM2 Interrupts/DMA" v="Disabled" />
        <boolgroup name="SM3 Interrupts/DMA" v="Disabled" />
        <group name="Fault interrupt">
          <Interrupt v="INT_eFlexPWMA_FAULT" />
          <Interrupt_priority v="&amp;lt;Automatic&amp;gt;" />
          <ISR_Name v="" />
          <Channel_0_fault_0_interrupt v="Disabled" />
          <Channel_0_fault_1_interrupt v="Disabled" />
          <Channel_0_fault_2_interrupt v="Disabled" />
          <Channel_0_fault_3_interrupt v="Disabled" />
          <Channel_1_Fault_0_interrupt v="Disabled" />
          <Channel_1_Fault_1_interrupt v="Disabled" />
          <Channel_1_Fault_2_interrupt v="Disabled" />
          <Channel_1_Fault_3_interrupt v="Disabled" />
        </group>
      </group>
      <group name="Initialization">
        <Load_values_after_init_into_SM0 v="yes" />
        <Load_values_after_init_into_SM1 v="no" />
        <Load_values_after_init_into_SM2 v="no" />
        <Load_values_after_init_into_SM3 v="no" />
        <Update_mask_SM0_immediately v="no" />
        <Update_mask_SM1_immediately v="no" />
        <Update_mask_SM2_immediately v="no" />
        <Update_mask_SM3_immediately v="no" />
        <PWM_clock_rate v="&amp;lt;Automatic&amp;gt;" />
        <PLL_output_divided v="&amp;lt;Automatic&amp;gt;" />
        <Enable_peripheral_clock_for_SM0 v="yes" />
        <Enable_peripheral_clock_for_SM1 v="&amp;lt;Automatic&amp;gt;" />
        <Enable_peripheral_clock_for_SM2 v="&amp;lt;Automatic&amp;gt;" />
        <Enable_peripheral_clock_for_SM3 v="&amp;lt;Automatic&amp;gt;" />
        <Fault_channel_0_test v="No simulated fault" />
        <Fault_channel_1_test v="No simulated fault" />
        <group name="Fault flag clearing">
          <Fault_channel_0_flag_0 v="Clear" />
          <Fault_channel_0_flag_1 v="Clear" />
          <Fault_channel_0_flag_2 v="Clear" />
          <Fault_channel_0_flag_3 v="Clear" />
          <Fault_channel_1_flag_0 v="Clear" />
          <Fault_channel_1_flag_1 v="Clear" />
          <Fault_channel_1_flag_2 v="Clear" />
          <Fault_channel_1_flag_3 v="Clear" />
        </group>
        <Monitor_PLL_mode v="Do not monitor PLL" />
        <Call_Init_method v="yes" />
        <Utilize_after_reset_values v="default" />
      </group>
    </Properties>
    <Methods>
      <Init v="generate code" />
    </Methods>
    <Events>
      <EmptySection_DummyValue />
    </Events>
  </Bean>
</PE_PROJECT_SETTINGS_DOCUMENTATION>

