ANALOG
Ch 1 Scale 2.00V/, Pos -4.00000V, Coup DC, BW Limit Off, Inv Off, Imp 1M Ohm
     Probe 10.000000 : 1, Skew 0.0s
Ch 2 Scale 2.00V/, Pos 0.0V, Coup DC, BW Limit Off, Inv Off, Imp 1M Ohm
     Probe 10.000000 : 1, Skew 0.0s

TRIGGER
Sweep Mode Auto, Coup DC, Noise Rej Off, HF Rej Off, Holdoff 40.0ns
Mode Edge, Source Ch 1, Slope Rising, Level 1.85000V

HORIZONTAL
Mode Normal, Ref Left, Main Scale 200.0ns/, Main Delay 0.0s

ACQUISITION
Mode Normal, Realtime On, Vectors On, Persistence Off

MEASUREMENTS
+ Width(1), Cur 1.3220us, Mean 1.3218us, Min 1.3205us, Max 1.3230us, Std Dev 400ps, Count 5.397k
+ Width(2), Cur Low signal, Mean , Min , Max , Std Dev , Count 0

SEARCH
Mode Edge

