Errata OM13026 DALI slave board
-------------------------------

Issue
-----
Backward DALI frames from the OM13026 DALI board are not correctly transmitted when using a DALI bus power supply with low current capability (~60mA).
When using a 200mA DALI bus power supply the issue does not occur.


Solution
---------
Change resistor R2 to 1k Ohm.
Boards with the text MV20110211 in silk are mounted with the resistor R2 of 10k.

NXP Semiconductors
March 2012

