# Static Call Graph for image .\Flash_M4\Gpio_LedBlinky.axf

#<CALLGRAPH># ARM Linker, 5.02 [Build 28]: Last Updated: Mon Apr 01 11:03:16 2013

### Maximum Stack Usage = 32 bytes + Unknown(Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

main ⇒ c_entry ⇒ GPIO_OutputValue ⇒ GPIO_ClearValue

### Mutually Recursive functions

- NMI_Handler ⇒ NMI_Handler
- HardFault_Handler ⇒ HardFault_Handler
- MemManage_Handler ⇒ MemManage_Handler
- BusFault_Handler ⇒ BusFault_Handler
- UsageFault_Handler ⇒ UsageFault_Handler
- SVC_Handler ⇒ SVC_Handler
- DebugMon_Handler ⇒ DebugMon_Handler
- PendSV_Handler ⇒ PendSV_Handler
- ADC_IRQHandler ⇒ ADC_IRQHandler

  ### Function Pointers

  - ADC_IRQHandler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - BOD_IRQHandler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - BusFault_Handler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - CANActivity_IRQHandler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - CAN_IRQHandler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - DMA_IRQHandler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - DebugMon_Handler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - EEPROM_IRQHandler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - EINT0_IRQHandler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - EINT1_IRQHandler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - EINT2_IRQHandler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - EINT3_IRQHandler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - ENET_IRQHandler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - GPIO_IRQHandler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - HardFault_Handler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - I2C0_IRQHandler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - I2C1_IRQHandler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - I2C2_IRQHandler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - I2S_IRQHandler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - LCD_IRQHandler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - MCI_IRQHandler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - MCPWM_IRQHandler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - MemManage_Handler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - NMI_Handler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - PLL0_IRQHandler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - PLL1_IRQHandler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - PWM0_IRQHandler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - PWM1_IRQHandler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - PendSV_Handler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - QEI_IRQHandler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - RTC_IRQHandler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - Reset_Handler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - SSP0_IRQHandler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - SSP1_IRQHandler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - SSP2_IRQHandler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - SVC_Handler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - SysTick_Handler from gpio_ledblinky.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - SystemInit from system_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(.text)
  - TIMER0_IRQHandler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - TIMER1_IRQHandler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - TIMER2_IRQHandler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - TIMER3_IRQHandler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - UART0_IRQHandler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - UART1_IRQHandler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - UART2_IRQHandler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - UART3_IRQHandler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - UART4_IRQHandler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - USBActivity_IRQHandler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - USB_IRQHandler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - UsageFault_Handler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - WDT_IRQHandler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - __main from entry.o(.ARM.Collect$$$$00000000) referenced from startup_lpc407x_8x_177x_8x.o(.text)
  - main from gpio_ledblinky.o(.text) referenced from entry8.o(.ARM.Collect$$$$00000009)

  ### Global Symbols

  __main (Thumb, 0 bytes, Stack size unknown bytes, entry.o(.ARM.Collect$$$$00000000))
  [Address Reference Count : 1]

  - startup_lpc407x_8x_177x_8x.o(.text)

  _main_stk (Thumb, 0 bytes, Stack size unknown bytes, entry2.o(.ARM.Collect$$$$00000001))

  _main_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Calls]

  - >> __scatterload

  __main_after_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Called By]

  - >> __scatterload

  _main_clock (Thumb, 0 bytes, Stack size unknown bytes, entry7b.o(.ARM.Collect$$$$00000008))

  _main_init (Thumb, 0 bytes, Stack size unknown bytes, entry8.o(.ARM.Collect$$$$00000009))

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Address Reference Count : 1]

  - startup_lpc407x_8x_177x_8x.o(RESET)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Calls]

  - >> NMI_Handler
  [Called By]
  - >> NMI_Handler
  [Address Reference Count : 1]
  - startup_lpc407x_8x_177x_8x.o(RESET)

  HardFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Calls]

  - >> HardFault_Handler
  [Called By]
  - >> HardFault_Handler
  [Address Reference Count : 1]
  - startup_lpc407x_8x_177x_8x.o(RESET)

  MemManage_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Calls]

  - >> MemManage_Handler
  [Called By]
  - >> MemManage_Handler
  [Address Reference Count : 1]
  - startup_lpc407x_8x_177x_8x.o(RESET)

  BusFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Calls]

  - >> BusFault_Handler
  [Called By]
  - >> BusFault_Handler
  [Address Reference Count : 1]
  - startup_lpc407x_8x_177x_8x.o(RESET)

  UsageFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Calls]

  - >> UsageFault_Handler
  [Called By]
  - >> UsageFault_Handler
  [Address Reference Count : 1]
  - startup_lpc407x_8x_177x_8x.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Calls]

  - >> SVC_Handler
  [Called By]
  - >> SVC_Handler
  [Address Reference Count : 1]
  - startup_lpc407x_8x_177x_8x.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Calls]

  - >> DebugMon_Handler
  [Called By]
  - >> DebugMon_Handler
  [Address Reference Count : 1]
  - startup_lpc407x_8x_177x_8x.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Calls]

  - >> PendSV_Handler
  [Called By]
  - >> PendSV_Handler
  [Address Reference Count : 1]
  - startup_lpc407x_8x_177x_8x.o(RESET)

  ADC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Calls]

  - >> ADC_IRQHandler
  [Called By]
  - >> ADC_IRQHandler
  [Address Reference Count : 1]
  - startup_lpc407x_8x_177x_8x.o(RESET)

  BOD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Address Reference Count : 1]

  - startup_lpc407x_8x_177x_8x.o(RESET)

  CANActivity_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Address Reference Count : 1]

  - startup_lpc407x_8x_177x_8x.o(RESET)

  CAN_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Address Reference Count : 1]

  - startup_lpc407x_8x_177x_8x.o(RESET)

  DMA_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Address Reference Count : 1]

  - startup_lpc407x_8x_177x_8x.o(RESET)

  EEPROM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Address Reference Count : 1]

  - startup_lpc407x_8x_177x_8x.o(RESET)

  EINT0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Address Reference Count : 1]

  - startup_lpc407x_8x_177x_8x.o(RESET)

  EINT1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Address Reference Count : 1]

  - startup_lpc407x_8x_177x_8x.o(RESET)

  EINT2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Address Reference Count : 1]

  - startup_lpc407x_8x_177x_8x.o(RESET)

  EINT3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Address Reference Count : 1]

  - startup_lpc407x_8x_177x_8x.o(RESET)

  ENET_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Address Reference Count : 1]

  - startup_lpc407x_8x_177x_8x.o(RESET)

  GPIO_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Address Reference Count : 1]

  - startup_lpc407x_8x_177x_8x.o(RESET)

  I2C0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Address Reference Count : 1]

  - startup_lpc407x_8x_177x_8x.o(RESET)

  I2C1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Address Reference Count : 1]

  - startup_lpc407x_8x_177x_8x.o(RESET)

  I2C2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Address Reference Count : 1]

  - startup_lpc407x_8x_177x_8x.o(RESET)

  I2S_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Address Reference Count : 1]

  - startup_lpc407x_8x_177x_8x.o(RESET)

  LCD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Address Reference Count : 1]

  - startup_lpc407x_8x_177x_8x.o(RESET)

  MCI_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Address Reference Count : 1]

  - startup_lpc407x_8x_177x_8x.o(RESET)

  MCPWM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Address Reference Count : 1]

  - startup_lpc407x_8x_177x_8x.o(RESET)

  PLL0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Address Reference Count : 1]

  - startup_lpc407x_8x_177x_8x.o(RESET)

  PLL1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Address Reference Count : 1]

  - startup_lpc407x_8x_177x_8x.o(RESET)

  PWM0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Address Reference Count : 1]

  - startup_lpc407x_8x_177x_8x.o(RESET)

  PWM1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Address Reference Count : 1]

  - startup_lpc407x_8x_177x_8x.o(RESET)

  QEI_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Address Reference Count : 1]

  - startup_lpc407x_8x_177x_8x.o(RESET)

  RTC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Address Reference Count : 1]

  - startup_lpc407x_8x_177x_8x.o(RESET)

  SSP0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Address Reference Count : 1]

  - startup_lpc407x_8x_177x_8x.o(RESET)

  SSP1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Address Reference Count : 1]

  - startup_lpc407x_8x_177x_8x.o(RESET)

  SSP2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Address Reference Count : 1]

  - startup_lpc407x_8x_177x_8x.o(RESET)

  TIMER0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Address Reference Count : 1]

  - startup_lpc407x_8x_177x_8x.o(RESET)

  TIMER1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Address Reference Count : 1]

  - startup_lpc407x_8x_177x_8x.o(RESET)

  TIMER2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Address Reference Count : 1]

  - startup_lpc407x_8x_177x_8x.o(RESET)

  TIMER3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Address Reference Count : 1]

  - startup_lpc407x_8x_177x_8x.o(RESET)

  UART0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Address Reference Count : 1]

  - startup_lpc407x_8x_177x_8x.o(RESET)

  UART1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Address Reference Count : 1]

  - startup_lpc407x_8x_177x_8x.o(RESET)

  UART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Address Reference Count : 1]

  - startup_lpc407x_8x_177x_8x.o(RESET)

  UART3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Address Reference Count : 1]

  - startup_lpc407x_8x_177x_8x.o(RESET)

  UART4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Address Reference Count : 1]

  - startup_lpc407x_8x_177x_8x.o(RESET)

  USBActivity_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Address Reference Count : 1]

  - startup_lpc407x_8x_177x_8x.o(RESET)

  USB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Address Reference Count : 1]

  - startup_lpc407x_8x_177x_8x.o(RESET)

  WDT_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Address Reference Count : 1]

  - startup_lpc407x_8x_177x_8x.o(RESET)

  CLKPWR_SetCLKDiv (Thumb, 154 bytes, Stack size 16 bytes, lpc_clkpwr.o(.text), UNUSED)
  [Calls]

  - >> SystemCoreClockUpdate

  CLKPWR_GetCLK (Thumb, 46 bytes, Stack size 0 bytes, lpc_clkpwr.o(.text))
  [Called By]

  - >> c_entry

  CLKPWR_ConfigPPWR (Thumb, 38 bytes, Stack size 0 bytes, lpc_clkpwr.o(.text))
  [Called By]

  - >> GPIO_Deinit
  - >> GPIO_Init

  CLKPWR_Sleep (Thumb, 10 bytes, Stack size 0 bytes, lpc_clkpwr.o(.text), UNUSED)

  CLKPWR_DeepSleep (Thumb, 16 bytes, Stack size 0 bytes, lpc_clkpwr.o(.text), UNUSED)

  CLKPWR_PowerDown (Thumb, 16 bytes, Stack size 0 bytes, lpc_clkpwr.o(.text), UNUSED)

  CLKPWR_DeepPowerDown (Thumb, 16 bytes, Stack size 0 bytes, lpc_clkpwr.o(.text), UNUSED)

  __scatterload (Thumb, 28 bytes, Stack size 0 bytes, init.o(.text))
  [Calls]

  - >> __main_after_scatterload
  [Called By]
  - >> _main_scatterload

  __scatterload_rt2 (Thumb, 0 bytes, Stack size 0 bytes, init.o(.text), UNUSED)

  __scatterload_copy (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_copy), UNUSED)

  __scatterload_null (Thumb, 2 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_null), UNUSED)

  __scatterload_zeroinit (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_zeroinit), UNUSED)

  SystemCoreClockUpdate (Thumb, 664 bytes, Stack size 12 bytes, system_lpc407x_8x_177x_8x.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = SystemCoreClockUpdate
  [Called By]
  - >> CLKPWR_SetCLKDiv
  - >> SystemInit

  fpu_init (Thumb, 48 bytes, Stack size 20 bytes, system_lpc407x_8x_177x_8x.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = fpu_init
  [Called By]
  - >> SystemInit

  SystemInit (Thumb, 210 bytes, Stack size 4 bytes, system_lpc407x_8x_177x_8x.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = SystemInit ⇒ fpu_init
  [Calls]
  - >> fpu_init
  - >> SystemCoreClockUpdate
  [Address Reference Count : 1]
  - startup_lpc407x_8x_177x_8x.o(.text)

  GPIO_Init (Thumb, 12 bytes, Stack size 8 bytes, lpc_gpio.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = GPIO_Init
  [Calls]
  - >> CLKPWR_ConfigPPWR
  [Called By]
  - >> c_entry

  GPIO_Deinit (Thumb, 14 bytes, Stack size 8 bytes, lpc_gpio.o(.text), UNUSED)
  [Calls]

  - >> CLKPWR_ConfigPPWR

  GPIO_SetDir (Thumb, 40 bytes, Stack size 24 bytes, lpc_gpio.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = GPIO_SetDir
  [Calls]
  - >> GPIO_GetPointer
  [Called By]
  - >> c_entry
  - >> FIO_SetDir

  GPIO_SetValue (Thumb, 20 bytes, Stack size 16 bytes, lpc_gpio.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = GPIO_SetValue
  [Calls]
  - >> GPIO_GetPointer
  [Called By]
  - >> FIO_SetValue
  - >> GPIO_OutputValue

  GPIO_ClearValue (Thumb, 20 bytes, Stack size 16 bytes, lpc_gpio.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = GPIO_ClearValue
  [Calls]
  - >> GPIO_GetPointer
  [Called By]
  - >> FIO_ClearValue
  - >> GPIO_OutputValue

  GPIO_OutputValue (Thumb, 30 bytes, Stack size 16 bytes, lpc_gpio.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = GPIO_OutputValue ⇒ GPIO_ClearValue
  [Calls]
  - >> GPIO_ClearValue
  - >> GPIO_SetValue
  [Called By]
  - >> c_entry

  GPIO_ReadValue (Thumb, 22 bytes, Stack size 16 bytes, lpc_gpio.o(.text), UNUSED)
  [Calls]

  - >> GPIO_GetPointer
  [Called By]
  - >> FIO_ReadValue

  GPIO_IntCmd (Thumb, 54 bytes, Stack size 0 bytes, lpc_gpio.o(.text), UNUSED)
  [Called By]

  - >> FIO_IntCmd

  GPIO_GetIntStatus (Thumb, 86 bytes, Stack size 0 bytes, lpc_gpio.o(.text), UNUSED)
  [Called By]

  - >> FIO_GetIntStatus

  GPIO_ClearInt (Thumb, 24 bytes, Stack size 0 bytes, lpc_gpio.o(.text), UNUSED)
  [Called By]

  - >> FIO_ClearInt

  FIO_SetDir (Thumb, 20 bytes, Stack size 16 bytes, lpc_gpio.o(.text), UNUSED)
  [Calls]

  - >> GPIO_SetDir

  FIO_SetValue (Thumb, 16 bytes, Stack size 16 bytes, lpc_gpio.o(.text), UNUSED)
  [Calls]

  - >> GPIO_SetValue

  FIO_ClearValue (Thumb, 16 bytes, Stack size 16 bytes, lpc_gpio.o(.text), UNUSED)
  [Calls]

  - >> GPIO_ClearValue

  FIO_ReadValue (Thumb, 12 bytes, Stack size 8 bytes, lpc_gpio.o(.text), UNUSED)
  [Calls]

  - >> GPIO_ReadValue

  FIO_IntCmd (Thumb, 20 bytes, Stack size 16 bytes, lpc_gpio.o(.text), UNUSED)
  [Calls]

  - >> GPIO_IntCmd

  FIO_GetIntStatus (Thumb, 20 bytes, Stack size 16 bytes, lpc_gpio.o(.text), UNUSED)
  [Calls]

  - >> GPIO_GetIntStatus

  FIO_ClearInt (Thumb, 16 bytes, Stack size 8 bytes, lpc_gpio.o(.text), UNUSED)
  [Calls]

  - >> GPIO_ClearInt

  FIO_SetMask (Thumb, 40 bytes, Stack size 24 bytes, lpc_gpio.o(.text), UNUSED)
  [Calls]

  - >> GPIO_GetPointer

  FIO_HalfWordSetDir (Thumb, 62 bytes, Stack size 24 bytes, lpc_gpio.o(.text), UNUSED)
  [Calls]

  - >> FIO_HalfWordGetPointer

  FIO_HalfWordSetMask (Thumb, 62 bytes, Stack size 24 bytes, lpc_gpio.o(.text), UNUSED)
  [Calls]

  - >> FIO_HalfWordGetPointer

  FIO_HalfWordSetValue (Thumb, 32 bytes, Stack size 24 bytes, lpc_gpio.o(.text), UNUSED)
  [Calls]

  - >> FIO_HalfWordGetPointer

  FIO_HalfWordClearValue (Thumb, 32 bytes, Stack size 24 bytes, lpc_gpio.o(.text), UNUSED)
  [Calls]

  - >> FIO_HalfWordGetPointer

  FIO_HalfWordReadValue (Thumb, 30 bytes, Stack size 16 bytes, lpc_gpio.o(.text), UNUSED)
  [Calls]

  - >> FIO_HalfWordGetPointer

  FIO_ByteSetDir (Thumb, 50 bytes, Stack size 24 bytes, lpc_gpio.o(.text), UNUSED)
  [Calls]

  - >> FIO_ByteGetPointer

  FIO_ByteSetMask (Thumb, 66 bytes, Stack size 24 bytes, lpc_gpio.o(.text), UNUSED)
  [Calls]

  - >> FIO_ByteGetPointer

  FIO_ByteSetValue (Thumb, 78 bytes, Stack size 24 bytes, lpc_gpio.o(.text), UNUSED)
  [Calls]

  - >> FIO_ByteGetPointer

  FIO_ByteClearValue (Thumb, 34 bytes, Stack size 24 bytes, lpc_gpio.o(.text), UNUSED)
  [Calls]

  - >> FIO_ByteGetPointer

  FIO_ByteReadValue (Thumb, 32 bytes, Stack size 16 bytes, lpc_gpio.o(.text), UNUSED)
  [Calls]

  - >> FIO_ByteGetPointer

  SysTick_Handler (Thumb, 12 bytes, Stack size 0 bytes, gpio_ledblinky.o(.text))
  [Address Reference Count : 1]

  - startup_lpc407x_8x_177x_8x.o(RESET)

  Delay (Thumb, 18 bytes, Stack size 0 bytes, gpio_ledblinky.o(.text))
  [Called By]

  - >> c_entry

  c_entry (Thumb, 136 bytes, Stack size 0 bytes, gpio_ledblinky.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = c_entry ⇒ GPIO_OutputValue ⇒ GPIO_ClearValue
  [Calls]
  - >> Delay
  - >> CLKPWR_GetCLK
  - >> GPIO_OutputValue
  - >> GPIO_SetDir
  - >> GPIO_Init
  [Called By]
  - >> main

  main (Thumb, 4 bytes, Stack size 0 bytes, gpio_ledblinky.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = main ⇒ c_entry ⇒ GPIO_OutputValue ⇒ GPIO_ClearValue
  [Calls]
  - >> c_entry
  [Address Reference Count : 1]
  - entry8.o(.ARM.Collect$$$$00000009)

  ### Local Symbols

  GPIO_GetPointer (Thumb, 58 bytes, Stack size 0 bytes, lpc_gpio.o(.text))
  [Called By]

  - >> FIO_SetMask
  - >> GPIO_ReadValue
  - >> GPIO_ClearValue
  - >> GPIO_SetValue
  - >> GPIO_SetDir

  FIO_HalfWordGetPointer (Thumb, 58 bytes, Stack size 0 bytes, lpc_gpio.o(.text), UNUSED)
  [Called By]

  - >> FIO_HalfWordReadValue
  - >> FIO_HalfWordClearValue
  - >> FIO_HalfWordSetValue
  - >> FIO_HalfWordSetMask
  - >> FIO_HalfWordSetDir

  FIO_ByteGetPointer (Thumb, 58 bytes, Stack size 0 bytes, lpc_gpio.o(.text), UNUSED)
  [Called By]

  - >> FIO_ByteReadValue
  - >> FIO_ByteClearValue
  - >> FIO_ByteSetValue
  - >> FIO_ByteSetMask
  - >> FIO_ByteSetDir

  ### Undefined Global Symbols