# Static Call Graph for image .\SPIFI\Blinky.axf

#<CALLGRAPH># ARM Linker, 5.03 [Build 69]: Last Updated: Sat Sep 07 23:33:05 2013

### Maximum Stack Usage = 116 bytes + Unknown(Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

mxic ⇒ setDev ⇒ write_stat ⇒ wait_busy ⇒ read04 ⇒ cmd

### Mutually Recursive functions

- NMI_Handler ⇒ NMI_Handler
- HardFault_Handler ⇒ HardFault_Handler
- MemManage_Handler ⇒ MemManage_Handler
- BusFault_Handler ⇒ BusFault_Handler
- UsageFault_Handler ⇒ UsageFault_Handler
- SVC_Handler ⇒ SVC_Handler
- DebugMon_Handler ⇒ DebugMon_Handler
- PendSV_Handler ⇒ PendSV_Handler
- BOD_IRQHandler ⇒ BOD_IRQHandler

  ### Function Pointers

  - ADC_IRQHandler from adc.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - BOD_IRQHandler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - BusFault_Handler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - CANActivity_IRQHandler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - CAN_IRQHandler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - DMA_IRQHandler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - DebugMon_Handler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - EEPROM_IRQHandler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - EINT0_IRQHandler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - EINT1_IRQHandler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - EINT2_IRQHandler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - EINT3_IRQHandler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - ENET_IRQHandler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - GPIO_IRQHandler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - HardFault_Handler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - I2C0_IRQHandler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - I2C1_IRQHandler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - I2C2_IRQHandler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - I2S_IRQHandler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - LCD_IRQHandler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - MCI_IRQHandler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - MCPWM_IRQHandler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - MemManage_Handler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - NMI_Handler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - PLL0_IRQHandler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - PLL1_IRQHandler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - PWM0_IRQHandler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - PWM1_IRQHandler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - PendSV_Handler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - QEI_IRQHandler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - RTC_IRQHandler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - Reset_Handler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - SSP0_IRQHandler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - SSP1_IRQHandler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - SSP2_IRQHandler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - SVC_Handler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - SysTick_Handler from irq.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - SystemInit from system_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(.text)
  - TIMER0_IRQHandler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - TIMER1_IRQHandler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - TIMER2_IRQHandler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - TIMER3_IRQHandler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - UART0_IRQHandler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - UART1_IRQHandler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - UART2_IRQHandler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - UART3_IRQHandler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - UART4_IRQHandler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - USBActivity_IRQHandler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - USB_IRQHandler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - UsageFault_Handler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - WDT_IRQHandler from startup_lpc407x_8x_177x_8x.o(.text) referenced from startup_lpc407x_8x_177x_8x.o(RESET)
  - __main from entry.o(.ARM.Collect$$$$00000000) referenced from startup_lpc407x_8x_177x_8x.o(.text)
  - _sputc from printf8.o(i._sputc) referenced from printf8.o(i.__0sprintf$8)
  - amic from amic.o(.text) referenced from spifi_rom_api.o(.text)
  - atm from atmel.o(.text) referenced from spifi_rom_api.o(.text)
  - chi from chi.o(.text) referenced from spifi_rom_api.o(.text)
  - eon from eon.o(.text) referenced from spifi_rom_api.o(.text)
  - esmt from esmt.o(.text) referenced from spifi_rom_api.o(.text)
  - fputc from retarget.o(.text) referenced from printf8.o(i.__0printf$8)
  - giga from giga.o(.text) referenced from spifi_rom_api.o(.text)
  - main from blinky.o(.text) referenced from entry9a.o(.ARM.Collect$$$$0000000B)
  - mxic from macronix.o(.text) referenced from spifi_rom_api.o(.text)
  - numo from numonyx.o(.text) referenced from spifi_rom_api.o(.text)
  - span from spansion.o(.text) referenced from spifi_rom_api.o(.text)
  - sst from sst.o(.text) referenced from spifi_rom_api.o(.text)
  - wbd from winbond.o(.text) referenced from spifi_rom_api.o(.text)

  ### Global Symbols

  __main (Thumb, 0 bytes, Stack size unknown bytes, entry.o(.ARM.Collect$$$$00000000))
  [Address Reference Count : 1]

  - startup_lpc407x_8x_177x_8x.o(.text)

  _main_stk (Thumb, 0 bytes, Stack size unknown bytes, entry2.o(.ARM.Collect$$$$00000001))

  _main_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Calls]

  - >> __scatterload

  __main_after_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Called By]

  - >> __scatterload

  _main_clock (Thumb, 0 bytes, Stack size unknown bytes, entry7b.o(.ARM.Collect$$$$00000008))

  _main_cpp_init (Thumb, 0 bytes, Stack size unknown bytes, entry8b.o(.ARM.Collect$$$$0000000A))

  _main_init (Thumb, 0 bytes, Stack size unknown bytes, entry9a.o(.ARM.Collect$$$$0000000B))

  __rt_final_cpp (Thumb, 0 bytes, Stack size unknown bytes, entry10a.o(.ARM.Collect$$$$0000000D))

  __rt_final_exit (Thumb, 0 bytes, Stack size unknown bytes, entry11a.o(.ARM.Collect$$$$0000000F))

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Address Reference Count : 1]

  - startup_lpc407x_8x_177x_8x.o(RESET)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Calls]

  - >> NMI_Handler
  [Called By]
  - >> NMI_Handler
  [Address Reference Count : 1]
  - startup_lpc407x_8x_177x_8x.o(RESET)

  HardFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Calls]

  - >> HardFault_Handler
  [Called By]
  - >> HardFault_Handler
  [Address Reference Count : 1]
  - startup_lpc407x_8x_177x_8x.o(RESET)

  MemManage_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Calls]

  - >> MemManage_Handler
  [Called By]
  - >> MemManage_Handler
  [Address Reference Count : 1]
  - startup_lpc407x_8x_177x_8x.o(RESET)

  BusFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Calls]

  - >> BusFault_Handler
  [Called By]
  - >> BusFault_Handler
  [Address Reference Count : 1]
  - startup_lpc407x_8x_177x_8x.o(RESET)

  UsageFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Calls]

  - >> UsageFault_Handler
  [Called By]
  - >> UsageFault_Handler
  [Address Reference Count : 1]
  - startup_lpc407x_8x_177x_8x.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Calls]

  - >> SVC_Handler
  [Called By]
  - >> SVC_Handler
  [Address Reference Count : 1]
  - startup_lpc407x_8x_177x_8x.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Calls]

  - >> DebugMon_Handler
  [Called By]
  - >> DebugMon_Handler
  [Address Reference Count : 1]
  - startup_lpc407x_8x_177x_8x.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Calls]

  - >> PendSV_Handler
  [Called By]
  - >> PendSV_Handler
  [Address Reference Count : 1]
  - startup_lpc407x_8x_177x_8x.o(RESET)

  BOD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Calls]

  - >> BOD_IRQHandler
  [Called By]
  - >> BOD_IRQHandler
  [Address Reference Count : 1]
  - startup_lpc407x_8x_177x_8x.o(RESET)

  CANActivity_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Address Reference Count : 1]

  - startup_lpc407x_8x_177x_8x.o(RESET)

  CAN_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Address Reference Count : 1]

  - startup_lpc407x_8x_177x_8x.o(RESET)

  DMA_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Address Reference Count : 1]

  - startup_lpc407x_8x_177x_8x.o(RESET)

  EEPROM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Address Reference Count : 1]

  - startup_lpc407x_8x_177x_8x.o(RESET)

  EINT0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Address Reference Count : 1]

  - startup_lpc407x_8x_177x_8x.o(RESET)

  EINT1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Address Reference Count : 1]

  - startup_lpc407x_8x_177x_8x.o(RESET)

  EINT2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Address Reference Count : 1]

  - startup_lpc407x_8x_177x_8x.o(RESET)

  EINT3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Address Reference Count : 1]

  - startup_lpc407x_8x_177x_8x.o(RESET)

  ENET_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Address Reference Count : 1]

  - startup_lpc407x_8x_177x_8x.o(RESET)

  GPIO_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Address Reference Count : 1]

  - startup_lpc407x_8x_177x_8x.o(RESET)

  I2C0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Address Reference Count : 1]

  - startup_lpc407x_8x_177x_8x.o(RESET)

  I2C1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Address Reference Count : 1]

  - startup_lpc407x_8x_177x_8x.o(RESET)

  I2C2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Address Reference Count : 1]

  - startup_lpc407x_8x_177x_8x.o(RESET)

  I2S_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Address Reference Count : 1]

  - startup_lpc407x_8x_177x_8x.o(RESET)

  LCD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Address Reference Count : 1]

  - startup_lpc407x_8x_177x_8x.o(RESET)

  MCI_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Address Reference Count : 1]

  - startup_lpc407x_8x_177x_8x.o(RESET)

  MCPWM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Address Reference Count : 1]

  - startup_lpc407x_8x_177x_8x.o(RESET)

  PLL0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Address Reference Count : 1]

  - startup_lpc407x_8x_177x_8x.o(RESET)

  PLL1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Address Reference Count : 1]

  - startup_lpc407x_8x_177x_8x.o(RESET)

  PWM0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Address Reference Count : 1]

  - startup_lpc407x_8x_177x_8x.o(RESET)

  PWM1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Address Reference Count : 1]

  - startup_lpc407x_8x_177x_8x.o(RESET)

  QEI_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Address Reference Count : 1]

  - startup_lpc407x_8x_177x_8x.o(RESET)

  RTC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Address Reference Count : 1]

  - startup_lpc407x_8x_177x_8x.o(RESET)

  SSP0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Address Reference Count : 1]

  - startup_lpc407x_8x_177x_8x.o(RESET)

  SSP1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Address Reference Count : 1]

  - startup_lpc407x_8x_177x_8x.o(RESET)

  SSP2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Address Reference Count : 1]

  - startup_lpc407x_8x_177x_8x.o(RESET)

  TIMER0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Address Reference Count : 1]

  - startup_lpc407x_8x_177x_8x.o(RESET)

  TIMER1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Address Reference Count : 1]

  - startup_lpc407x_8x_177x_8x.o(RESET)

  TIMER2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Address Reference Count : 1]

  - startup_lpc407x_8x_177x_8x.o(RESET)

  TIMER3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Address Reference Count : 1]

  - startup_lpc407x_8x_177x_8x.o(RESET)

  UART0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Address Reference Count : 1]

  - startup_lpc407x_8x_177x_8x.o(RESET)

  UART1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Address Reference Count : 1]

  - startup_lpc407x_8x_177x_8x.o(RESET)

  UART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Address Reference Count : 1]

  - startup_lpc407x_8x_177x_8x.o(RESET)

  UART3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Address Reference Count : 1]

  - startup_lpc407x_8x_177x_8x.o(RESET)

  UART4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Address Reference Count : 1]

  - startup_lpc407x_8x_177x_8x.o(RESET)

  USBActivity_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Address Reference Count : 1]

  - startup_lpc407x_8x_177x_8x.o(RESET)

  USB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Address Reference Count : 1]

  - startup_lpc407x_8x_177x_8x.o(RESET)

  WDT_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc407x_8x_177x_8x.o(.text))
  [Address Reference Count : 1]

  - startup_lpc407x_8x_177x_8x.o(RESET)

  fputc (Thumb, 14 bytes, Stack size 16 bytes, retarget.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = fputc
  [Calls]
  - >> SER_PutChar
  [Address Reference Count : 1]
  - printf8.o(i.__0printf$8)

  fgetc (Thumb, 10 bytes, Stack size 8 bytes, retarget.o(.text), UNUSED)
  [Calls]

  - >> SER_GetChar

  ferror (Thumb, 8 bytes, Stack size 0 bytes, retarget.o(.text), UNUSED)

  _ttywrch (Thumb, 12 bytes, Stack size 8 bytes, retarget.o(.text), UNUSED)
  [Calls]

  - >> SER_PutChar

  _sys_exit (Thumb, 4 bytes, Stack size 0 bytes, retarget.o(.text), UNUSED)

  SER_Init (Thumb, 80 bytes, Stack size 0 bytes, serial.o(.text))
  [Called By]

  - >> main

  SER_PutChar (Thumb, 18 bytes, Stack size 0 bytes, serial.o(.text))
  [Called By]

  - >> _ttywrch
  - >> fputc

  SER_GetChar (Thumb, 22 bytes, Stack size 0 bytes, serial.o(.text), UNUSED)
  [Called By]

  - >> fgetc

  ADC_Init (Thumb, 66 bytes, Stack size 0 bytes, adc.o(.text))
  [Called By]

  - >> main

  ADC_StartCnv (Thumb, 24 bytes, Stack size 0 bytes, adc.o(.text))
  [Called By]

  - >> SysTick_Handler

  ADC_GetCnv (Thumb, 6 bytes, Stack size 0 bytes, adc.o(.text), UNUSED)

  ADC_IRQHandler (Thumb, 28 bytes, Stack size 8 bytes, adc.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = ADC_IRQHandler
  [Address Reference Count : 1]
  - startup_lpc407x_8x_177x_8x.o(RESET)

  SysTick_Handler (Thumb, 94 bytes, Stack size 8 bytes, irq.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = SysTick_Handler ⇒ LED_Out
  [Calls]
  - >> LED_Out (via Veneer)
  - >> ADC_StartCnv
  [Address Reference Count : 1]
  - startup_lpc407x_8x_177x_8x.o(RESET)

  __scatterload_null (Thumb, 2 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_null), UNUSED)

  __scatterload_copy (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_copy), UNUSED)

  SystemCoreClockUpdate (Thumb, 664 bytes, Stack size 12 bytes, system_lpc407x_8x_177x_8x.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = SystemCoreClockUpdate
  [Called By]
  - >> main
  - >> SystemInit

  fpu_init (Thumb, 64 bytes, Stack size 24 bytes, system_lpc407x_8x_177x_8x.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = fpu_init
  [Called By]
  - >> SystemInit

  SystemInit (Thumb, 214 bytes, Stack size 4 bytes, system_lpc407x_8x_177x_8x.o(.text))
  [Stack]

  - Max Depth = 28
  - Call Chain = SystemInit ⇒ fpu_init
  [Calls]
  - >> fpu_init
  - >> SystemCoreClockUpdate
  [Address Reference Count : 1]
  - startup_lpc407x_8x_177x_8x.o(.text)

  main (Thumb, 186 bytes, Stack size 0 bytes, blinky.o(.text))
  [Stack]

  - Max Depth = 92
  - Call Chain = main ⇒ SPIFI_Init ⇒ spifi_init ⇒ set_mem_mode ⇒ wren_send04 ⇒ send04 ⇒ cmd
  [Calls]
  - >> SPIFI_Init
  - >> LED_Init (via Veneer)
  - >> ADC_Init
  - >> SER_Init
  - >> SystemCoreClockUpdate
  - >> __2sprintf
  - >> __2printf
  [Address Reference Count : 1]
  - entry9a.o(.ARM.Collect$$$$0000000B)

  SPIFI_Init (Thumb, 172 bytes, Stack size 8 bytes, spifi.o(.text))
  [Stack]

  - Max Depth = 92
  - Call Chain = SPIFI_Init ⇒ spifi_init ⇒ set_mem_mode ⇒ wren_send04 ⇒ send04 ⇒ cmd
  [Calls]
  - >> spifi_init
  [Called By]
  - >> main

  read_flash (Thumb, 50 bytes, Stack size 0 bytes, spifi_rom_api.o(.text))
  [Called By]

  - >> readAd
  - >> read04
  - >> spifi_init

  cmd (Thumb, 22 bytes, Stack size 8 bytes, spifi_rom_api.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = cmd
  [Called By]
  - >> setProt
  - >> write_stat
  - >> send04
  - >> read04
  - >> spifi_init

  all_quad (Thumb, 16 bytes, Stack size 0 bytes, spifi_rom_api.o(.text))
  [Called By]

  - >> send_erase_cmd
  - >> setProt
  - >> readProt
  - >> wait_busy
  - >> wren_sendAd
  - >> send04
  - >> readAd
  - >> read04

  read04 (Thumb, 32 bytes, Stack size 8 bytes, spifi_rom_api.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = read04 ⇒ cmd
  [Calls]
  - >> all_quad
  - >> cmd
  - >> read_flash
  [Called By]
  - >> moreId
  - >> mxic
  - >> atm
  - >> setProt
  - >> setDev
  - >> setWPSEL
  - >> set_mem_mode
  - >> wait_busy
  - >> wren
  - >> spifi_init

  readAd (Thumb, 18 bytes, Stack size 4 bytes, spifi_rom_api.o(.text))
  [Stack]

  - Max Depth = 4
  - Call Chain = readAd
  [Calls]
  - >> all_quad
  - >> read_flash
  [Called By]
  - >> setProt
  - >> spifi_init

  send04 (Thumb, 40 bytes, Stack size 12 bytes, spifi_rom_api.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = send04 ⇒ cmd
  [Calls]
  - >> all_quad
  - >> cmd
  [Called By]
  - >> setDev
  - >> set_mem_mode
  - >> wren_send04

  wren (Thumb, 6 bytes, Stack size 0 bytes, spifi_rom_api.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = wren ⇒ read04 ⇒ cmd
  [Calls]
  - >> read04
  [Called By]
  - >> send_prog_cmd
  - >> send_erase_cmd
  - >> setProt
  - >> wren_sendAd
  - >> wren_send04

  wren_send04 (Thumb, 28 bytes, Stack size 20 bytes, spifi_rom_api.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = wren_send04 ⇒ send04 ⇒ cmd
  [Calls]
  - >> wren
  - >> send04
  [Called By]
  - >> spifi_erase
  - >> setProt
  - >> setDev
  - >> set_mem_mode
  - >> spifi_init

  wren_sendAd (Thumb, 74 bytes, Stack size 20 bytes, spifi_rom_api.o(.text))
  [Stack]

  - Max Depth = 36
  - Call Chain = wren_sendAd ⇒ wren ⇒ read04 ⇒ cmd
  [Calls]
  - >> wren
  - >> all_quad
  [Called By]
  - >> setProt
  - >> write_stat

  cancel_mem_mode (Thumb, 64 bytes, Stack size 0 bytes, spifi_rom_api.o(.text))
  [Called By]

  - >> spifi_erase
  - >> spifi_program
  - >> send_erase_cmd
  - >> setProt
  - >> wait_busy
  - >> spifi_init

  wait_busy (Thumb, 218 bytes, Stack size 24 bytes, spifi_rom_api.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = wait_busy ⇒ read04 ⇒ cmd
  [Calls]
  - >> cancel_mem_mode
  - >> read04
  - >> all_quad
  [Called By]
  - >> spifi_erase
  - >> prog_block
  - >> send_erase_cmd
  - >> write_stat

  write_stat (Thumb, 50 bytes, Stack size 12 bytes, spifi_rom_api.o(.text))
  [Stack]

  - Max Depth = 52
  - Call Chain = write_stat ⇒ wait_busy ⇒ read04 ⇒ cmd
  [Calls]
  - >> wait_busy
  - >> wren_sendAd
  - >> cmd
  [Called By]
  - >> mxic
  - >> setProt
  - >> setDev

  set_mem_mode (Thumb, 142 bytes, Stack size 20 bytes, spifi_rom_api.o(.text))
  [Stack]

  - Max Depth = 60
  - Call Chain = set_mem_mode ⇒ wren_send04 ⇒ send04 ⇒ cmd
  [Calls]
  - >> wren_send04
  - >> send04
  - >> read04
  [Called By]
  - >> spifi_erase
  - >> spifi_program
  - >> setProt
  - >> spifi_init

  setWPSEL (Thumb, 48 bytes, Stack size 8 bytes, spifi_rom_api.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = setWPSEL ⇒ read04 ⇒ cmd
  [Calls]
  - >> read04
  [Called By]
  - >> setProt
  - >> setDev

  setProtEnts (Thumb, 60 bytes, Stack size 12 bytes, spifi_rom_api.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = setProtEnts
  [Called By]
  - >> sst
  - >> mxic
  - >> atm

  getProtBytes (Thumb, 28 bytes, Stack size 0 bytes, spifi_rom_api.o(.text))
  [Called By]

  - >> setProt
  - >> readProt

  readProt (Thumb, 84 bytes, Stack size 8 bytes, spifi_rom_api.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = readProt
  [Calls]
  - >> getProtBytes
  - >> all_quad
  [Called By]
  - >> setProt
  - >> spifi_init

  setSize (Thumb, 52 bytes, Stack size 0 bytes, spifi_rom_api.o(.text))
  [Called By]

  - >> moreId
  - >> wbd
  - >> sst
  - >> span
  - >> numo
  - >> mxic
  - >> giga
  - >> esmt
  - >> eon
  - >> chi
  - >> atm
  - >> amic

  setDev (Thumb, 412 bytes, Stack size 24 bytes, spifi_rom_api.o(.text))
  [Stack]

  - Max Depth = 76
  - Call Chain = setDev ⇒ write_stat ⇒ wait_busy ⇒ read04 ⇒ cmd
  [Calls]
  - >> setWPSEL
  - >> write_stat
  - >> wren_send04
  - >> send04
  - >> read04
  [Called By]
  - >> wbd
  - >> sst
  - >> span
  - >> numo
  - >> mxic
  - >> giga
  - >> esmt
  - >> eon
  - >> chi
  - >> atm
  - >> amic

  spifi_init (Thumb, 462 bytes, Stack size 24 bytes, spifi_rom_api.o(.text))
  [Stack]

  - Max Depth = 84
  - Call Chain = spifi_init ⇒ set_mem_mode ⇒ wren_send04 ⇒ send04 ⇒ cmd
  [Calls]
  - >> __aeabi_memclr4
  - >> pullMISO
  - >> readProt
  - >> set_mem_mode
  - >> cancel_mem_mode
  - >> wren_send04
  - >> readAd
  - >> read04
  - >> cmd
  - >> read_flash
  [Called By]
  - >> SPIFI_Init

  setProt (Thumb, 1060 bytes, Stack size 88 bytes, spifi_rom_api.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memcpy
  - >> readProt
  - >> getProtBytes
  - >> setWPSEL
  - >> set_mem_mode
  - >> write_stat
  - >> cancel_mem_mode
  - >> wren_sendAd
  - >> wren_send04
  - >> wren
  - >> readAd
  - >> read04
  - >> all_quad
  - >> cmd
  [Called By]
  - >> spifi_erase
  - >> spifi_program

  checkAd (Thumb, 72 bytes, Stack size 16 bytes, spifi_rom_api.o(.text), UNUSED)
  [Called By]

  - >> spifi_erase
  - >> spifi_program

  send_erase_cmd (Thumb, 66 bytes, Stack size 16 bytes, spifi_rom_api.o(.text), UNUSED)
  [Calls]

  - >> wait_busy
  - >> cancel_mem_mode
  - >> wren
  - >> all_quad
  [Called By]
  - >> spifi_erase
  - >> spifi_program

  send_prog_cmd (Thumb, 24 bytes, Stack size 16 bytes, spifi_rom_api.o(.text), UNUSED)
  [Calls]

  - >> wren
  [Called By]
  - >> prog_block

  prog_block (Thumb, 246 bytes, Stack size 32 bytes, spifi_rom_api.o(.text), UNUSED)
  [Calls]

  - >> send_prog_cmd
  - >> wait_busy
  [Called By]
  - >> spifi_erase
  - >> spifi_program

  ck_erase (Thumb, 24 bytes, Stack size 0 bytes, spifi_rom_api.o(.text), UNUSED)
  [Called By]

  - >> spifi_erase
  - >> spifi_program

  ck_setup (Thumb, 22 bytes, Stack size 0 bytes, spifi_rom_api.o(.text), UNUSED)
  [Called By]

  - >> check_block
  - >> ck_prog

  ck_prog (Thumb, 98 bytes, Stack size 28 bytes, spifi_rom_api.o(.text), UNUSED)
  [Calls]

  - >> ck_setup
  [Called By]
  - >> spifi_erase
  - >> spifi_program

  check_block (Thumb, 128 bytes, Stack size 24 bytes, spifi_rom_api.o(.text), UNUSED)
  [Calls]

  - >> ck_setup
  [Called By]
  - >> spifi_program

  spifi_program (Thumb, 584 bytes, Stack size 160 bytes, spifi_rom_api.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memcpy4
  - >> __aeabi_memcpy
  - >> check_block
  - >> ck_prog
  - >> ck_erase
  - >> prog_block
  - >> send_erase_cmd
  - >> checkAd
  - >> setProt
  - >> set_mem_mode
  - >> cancel_mem_mode

  spifi_erase (Thumb, 496 bytes, Stack size 160 bytes, spifi_rom_api.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memcpy4
  - >> __aeabi_memcpy
  - >> ck_prog
  - >> ck_erase
  - >> prog_block
  - >> send_erase_cmd
  - >> checkAd
  - >> setProt
  - >> set_mem_mode
  - >> wait_busy
  - >> cancel_mem_mode
  - >> wren_send04

  amic (Thumb, 134 bytes, Stack size 24 bytes, amic.o(.text))
  [Stack]

  - Max Depth = 100
  - Call Chain = amic ⇒ setDev ⇒ write_stat ⇒ wait_busy ⇒ read04 ⇒ cmd
  [Calls]
  - >> setDev
  - >> setSize
  [Address Reference Count : 1]
  - spifi_rom_api.o(.text)

  atm (Thumb, 252 bytes, Stack size 24 bytes, atmel.o(.text))
  [Stack]

  - Max Depth = 100
  - Call Chain = atm ⇒ setDev ⇒ write_stat ⇒ wait_busy ⇒ read04 ⇒ cmd
  [Calls]
  - >> setDev
  - >> setSize
  - >> setProtEnts
  - >> read04
  [Address Reference Count : 1]
  - spifi_rom_api.o(.text)

  chi (Thumb, 194 bytes, Stack size 16 bytes, chi.o(.text))
  [Stack]

  - Max Depth = 92
  - Call Chain = chi ⇒ setDev ⇒ write_stat ⇒ wait_busy ⇒ read04 ⇒ cmd
  [Calls]
  - >> setDev
  - >> setSize
  [Address Reference Count : 1]
  - spifi_rom_api.o(.text)

  eon (Thumb, 174 bytes, Stack size 24 bytes, eon.o(.text))
  [Stack]

  - Max Depth = 100
  - Call Chain = eon ⇒ setDev ⇒ write_stat ⇒ wait_busy ⇒ read04 ⇒ cmd
  [Calls]
  - >> setDev
  - >> setSize
  [Address Reference Count : 1]
  - spifi_rom_api.o(.text)

  esmt (Thumb, 164 bytes, Stack size 24 bytes, esmt.o(.text))
  [Stack]

  - Max Depth = 100
  - Call Chain = esmt ⇒ setDev ⇒ write_stat ⇒ wait_busy ⇒ read04 ⇒ cmd
  [Calls]
  - >> setDev
  - >> setSize
  [Address Reference Count : 1]
  - spifi_rom_api.o(.text)

  giga (Thumb, 156 bytes, Stack size 24 bytes, giga.o(.text))
  [Stack]

  - Max Depth = 100
  - Call Chain = giga ⇒ setDev ⇒ write_stat ⇒ wait_busy ⇒ read04 ⇒ cmd
  [Calls]
  - >> setDev
  - >> setSize
  [Address Reference Count : 1]
  - spifi_rom_api.o(.text)

  mxic (Thumb, 382 bytes, Stack size 40 bytes, macronix.o(.text))
  [Stack]

  - Max Depth = 116
  - Call Chain = mxic ⇒ setDev ⇒ write_stat ⇒ wait_busy ⇒ read04 ⇒ cmd
  [Calls]
  - >> setDev
  - >> setSize
  - >> setProtEnts
  - >> write_stat
  - >> read04
  [Address Reference Count : 1]
  - spifi_rom_api.o(.text)

  numo_dummies (Thumb, 50 bytes, Stack size 12 bytes, numonyx.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = numo_dummies
  [Called By]
  - >> numo

  numo (Thumb, 290 bytes, Stack size 32 bytes, numonyx.o(.text))
  [Stack]

  - Max Depth = 108
  - Call Chain = numo ⇒ setDev ⇒ write_stat ⇒ wait_busy ⇒ read04 ⇒ cmd
  [Calls]
  - >> numo_dummies
  - >> setDev
  - >> setSize
  [Address Reference Count : 1]
  - spifi_rom_api.o(.text)

  moreId (Thumb, 66 bytes, Stack size 8 bytes, spansion.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = moreId ⇒ read04 ⇒ cmd
  [Calls]
  - >> setSize
  - >> read04
  [Called By]
  - >> span

  span (Thumb, 146 bytes, Stack size 16 bytes, spansion.o(.text))
  [Stack]

  - Max Depth = 92
  - Call Chain = span ⇒ setDev ⇒ write_stat ⇒ wait_busy ⇒ read04 ⇒ cmd
  [Calls]
  - >> moreId
  - >> setDev
  - >> setSize
  [Address Reference Count : 1]
  - spifi_rom_api.o(.text)

  sst (Thumb, 158 bytes, Stack size 16 bytes, sst.o(.text))
  [Stack]

  - Max Depth = 92
  - Call Chain = sst ⇒ setDev ⇒ write_stat ⇒ wait_busy ⇒ read04 ⇒ cmd
  [Calls]
  - >> setDev
  - >> setSize
  - >> setProtEnts
  [Address Reference Count : 1]
  - spifi_rom_api.o(.text)

  wbd_dummies (Thumb, 30 bytes, Stack size 8 bytes, winbond.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = wbd_dummies
  [Called By]
  - >> wbd

  wbd (Thumb, 202 bytes, Stack size 24 bytes, winbond.o(.text))
  [Stack]

  - Max Depth = 100
  - Call Chain = wbd ⇒ setDev ⇒ write_stat ⇒ wait_busy ⇒ read04 ⇒ cmd
  [Calls]
  - >> wbd_dummies
  - >> setDev
  - >> setSize
  [Address Reference Count : 1]
  - spifi_rom_api.o(.text)

  set_uart (Thumb, 42 bytes, Stack size 0 bytes, neo_details.o(.text), UNUSED)
  [Called By]

  - >> set_spifi_clk

  set_spifi_clk (Thumb, 254 bytes, Stack size 20 bytes, neo_details.o(.text), UNUSED)
  [Calls]

  - >> set_uart

  set_spifi_io (Thumb, 34 bytes, Stack size 0 bytes, neo_details.o(.text), UNUSED)

  pullMISO (Thumb, 26 bytes, Stack size 0 bytes, neo_details.o(.text))
  [Called By]

  - >> spifi_init

  __aeabi_memcpy (Thumb, 36 bytes, Stack size 0 bytes, memcpya.o(.text), UNUSED)
  [Called By]

  - >> spifi_erase
  - >> spifi_program
  - >> setProt

  __aeabi_memcpy4 (Thumb, 0 bytes, Stack size 0 bytes, memcpya.o(.text), UNUSED)
  [Called By]

  - >> spifi_erase
  - >> spifi_program

  __aeabi_memcpy8 (Thumb, 0 bytes, Stack size 0 bytes, memcpya.o(.text), UNUSED)

  __aeabi_memset (Thumb, 14 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)
  [Called By]

  - >> _memset$wrapper
  - >> __aeabi_memclr

  __aeabi_memset4 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  __aeabi_memset8 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  __aeabi_memclr (Thumb, 4 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memset

  __aeabi_memclr4 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text))
  [Called By]

  - >> spifi_init

  __aeabi_memclr8 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  _memset$wrapper (Thumb, 18 bytes, Stack size 8 bytes, memseta.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memset

  __aeabi_uldivmod (Thumb, 98 bytes, Stack size 40 bytes, uldiv.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_llsr
  - >> __aeabi_llsl
  [Called By]
  - >> _printf_core

  __scatterload (Thumb, 28 bytes, Stack size 0 bytes, init.o(.text))
  [Calls]

  - >> __main_after_scatterload
  [Called By]
  - >> _main_scatterload

  __scatterload_rt2 (Thumb, 0 bytes, Stack size 0 bytes, init.o(.text), UNUSED)

  __aeabi_llsl (Thumb, 30 bytes, Stack size 0 bytes, llshl.o(.text), UNUSED)
  [Called By]

  - >> __aeabi_uldivmod

  _ll_shift_l (Thumb, 0 bytes, Stack size 0 bytes, llshl.o(.text), UNUSED)

  __aeabi_llsr (Thumb, 32 bytes, Stack size 0 bytes, llushr.o(.text), UNUSED)
  [Called By]

  - >> __aeabi_uldivmod

  _ll_ushift_r (Thumb, 0 bytes, Stack size 0 bytes, llushr.o(.text), UNUSED)

  __0printf$8 (Thumb, 22 bytes, Stack size 24 bytes, printf8.o(i.__0printf$8), UNUSED)
  [Calls]

  - >> _printf_core

  __1printf$8 (Thumb, 0 bytes, Stack size 24 bytes, printf8.o(i.__0printf$8), UNUSED)

  __2printf (Thumb, 0 bytes, Stack size 24 bytes, printf8.o(i.__0printf$8))
  [Stack]

  - Max Depth = 24
  - Call Chain = __2printf
  [Called By]
  - >> main

  __0sprintf$8 (Thumb, 34 bytes, Stack size 24 bytes, printf8.o(i.__0sprintf$8), UNUSED)
  [Calls]

  - >> _sputc
  - >> _printf_core

  __1sprintf$8 (Thumb, 0 bytes, Stack size 24 bytes, printf8.o(i.__0sprintf$8), UNUSED)

  __2sprintf (Thumb, 0 bytes, Stack size 24 bytes, printf8.o(i.__0sprintf$8))
  [Stack]

  - Max Depth = 24
  - Call Chain = __2sprintf
  [Called By]
  - >> main

  __scatterload_zeroinit (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_zeroinit), UNUSED)

  LED_Init (Thumb, 32 bytes, Stack size 0 bytes, led.o(.text))
  [Called By]

  - >> main (via Veneer)

  LED_On (Thumb, 12 bytes, Stack size 0 bytes, led.o(.text))
  [Called By]

  - >> LED_Out

  LED_Off (Thumb, 12 bytes, Stack size 0 bytes, led.o(.text))
  [Called By]

  - >> LED_Out

  LED_Out (Thumb, 38 bytes, Stack size 8 bytes, led.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = LED_Out
  [Calls]
  - >> LED_Off
  - >> LED_On
  [Called By]
  - >> SysTick_Handler (via Veneer)

  ### Local Symbols

  _printf_core (Thumb, 988 bytes, Stack size 104 bytes, printf8.o(i._printf_core), UNUSED)
  [Calls]

  - >> __aeabi_uldivmod
  - >> _printf_pre_padding
  - >> _printf_post_padding
  [Called By]
  - >> __0sprintf$8
  - >> __0printf$8

  _printf_post_padding (Thumb, 38 bytes, Stack size 24 bytes, printf8.o(i._printf_post_padding), UNUSED)
  [Called By]

  - >> _printf_core

  _printf_pre_padding (Thumb, 48 bytes, Stack size 24 bytes, printf8.o(i._printf_pre_padding), UNUSED)
  [Called By]

  - >> _printf_core

  _sputc (Thumb, 10 bytes, Stack size 0 bytes, printf8.o(i._sputc))
  [Called By]

  - >> __0sprintf$8
  [Address Reference Count : 1]
  - printf8.o(i.__0sprintf$8)

  ### Undefined Global Symbols