| Linux NFC User Mode Stack

- Main Page
- Classes
- Files

- Class List
- Class Index
- Class Members

- All
- Variables

- a
- b
- c
- d
- h
- i
- k
- m
- n
- o
- p
- s
- t
- u
- w

### - a -

- address : nfc_btoob_pairing_t

### - b -

- bluetooth : nfc_handover_request_t , nfc_handover_select_t

### - c -

- current_ndef_length : ndef_info_t

### - d -

- device_name : nfc_btoob_pairing_t
- device_name_length : nfc_btoob_pairing_t

### - h -

- handle : nfc_tag_info_t
- has_wifi : nfc_wifi_request_t

### - i -

- is_ndef : ndef_info_t
- is_writable : ndef_info_t

### - k -

- key : nfc_wifi_pairing_t
- key_length : nfc_wifi_pairing_t

### - m -

- max_ndef_length : ndef_info_t

### - n -

- ndef : nfc_btoob_pairing_t , nfc_wifi_pairing_t , nfc_wifi_request_t
- ndef_length : nfc_btoob_pairing_t , nfc_wifi_pairing_t , nfc_wifi_request_t

### - o -

- onDataReceived : nfcHostCardEmulationCallback_t
- onDeviceArrival : nfcSnepClientCallback_t , nfcSnepServerCallback_t
- onDeviceDeparture : nfcSnepClientCallback_t , nfcSnepServerCallback_t
- onHandoverRequestReceived : nfcHandoverCallback_t
- onHandoverSelectReceived : nfcHandoverCallback_t
- onHostCardEmulationActivated : nfcHostCardEmulationCallback_t
- onHostCardEmulationDeactivated : nfcHostCardEmulationCallback_t
- onMessageReceived : nfcSnepServerCallback_t
- onTagArrival : nfcTagCallback_t
- onTagDeparture : nfcTagCallback_t

### - p -

- power_state : nfc_btoob_pairing_t , nfc_wifi_pairing_t
- protocol : nfc_tag_info_t

### - s -

- ssid : nfc_wifi_pairing_t
- ssid_length : nfc_wifi_pairing_t

### - t -

- technology : nfc_tag_info_t
- type : nfc_btoob_pairing_t

### - u -

- uid : nfc_tag_info_t
- uid_length : nfc_tag_info_t

### - w -

- wAgcDifferentialWithOpen1 : nfcFactory_Antenna_St_Resp_t
- wAgcDifferentialWithOpen2 : nfcFactory_Antenna_St_Resp_t
- wAgcDifferentialWithOpenTolerance1 : nfcFactory_Antenna_St_Resp_t
- wAgcDifferentialWithOpenTolerance2 : nfcFactory_Antenna_St_Resp_t
- wAgcValue : nfcFactory_Antenna_St_Resp_t
- wAgcValueTolerance : nfcFactory_Antenna_St_Resp_t
- wAgcValuewithfixedNFCLD : nfcFactory_Antenna_St_Resp_t
- wAgcValuewithfixedNFCLDTolerance : nfcFactory_Antenna_St_Resp_t
- wifi : nfc_handover_request_t , nfc_handover_select_t
- wTxdoMeasuredRangeMax : nfcFactory_Antenna_St_Resp_t
- wTxdoMeasuredRangeMin : nfcFactory_Antenna_St_Resp_t
- wTxdoMeasuredTolerance : nfcFactory_Antenna_St_Resp_t
- wTxdoRawValue : nfcFactory_Antenna_St_Resp_t