V5.33
---------------------------------------------------
- Iot on OpenWRT on Raspberry-Pi
- "One Gateway"
- NTAG layout V11
- PN7120 NFC Reader support
- Mobile and System webpages
- With Jennic flasher for JN5168 and JN5169 dongles
- Uses neighbour table to handle missed announce messages
- More distinct audio feedback during NFC transactions
- Fixed IP addresses in System webpage
- Save timezone name in /etc/config/system
- With latest ZCB from trunk
- Fixed error in system webpage
- Fixed error in flasher
- Added re-install anyway button
- Internet support via wifi dongle (requires V5.33 SD-card image)

wo okt  7 15:17:45 CEST 2015
