| USBD ROM Stack 1.0 ROM based USB device stack

mw_iap.h
1 /*
2 %
3 % Copyright 2012 NXP Semiconductors,
4 % 411 E Plumeria Dr San Jose CA USA
5 % All rights are reserved. Reproduction in whole or in part is prohibited
6 % without the prior written consent of the copyright owner.
7 %
8 */
9
10 /*
11 +++ IDENTIFICATION
12
13 PACKAGE :
14 COMPONENT :
15 INTERFACE :
16 TEMPLATE VERSION : 3
17 */
18 #ifndef __MW_IAP_H__
19 #define __MW_IAP_H__
20 #include "param_check.h"
21
22 #define READ_OP 0
23 #define WRITE_OP 1
24
25 #define NO_OF_IAP_PARAMS 5
26 #define IAP_CMD_CODE 0
27 #define IAP_PARAM_0 1
28 #define IAP_PARAM_1 2
29 #define IAP_PARAM_2 3
30 #define IAP_PARAM_3 4
31 #define IAP_STAT_CODE 0
32 #define IAP_RESULT_0 1
33 #define IAP_RESULT_1 2
34 #define IAP_RESULT_2 3
35 #define IAP_RESULT_3 4
36
37 /*********************
38 * EXPORTED TYPEDEFS *
39 **********************/
40
41 typedef enum
42 {
43 PREPARE_SECTOR_FOR_WRITE=50,
44 COPY_RAM_TO_FLASH=51,
45 ERASE_SECTOR=52,
46 BLANK_CHECK_SECTOR=53,
47 READ_PART_ID=54,
48 READ_BOOT_VER=55,
49 COMPARE=56,
50 REINVOKE_ISP=57,
51 READ_UID=58,
52 ERASE_PAGE=59,
53 READ_MISR=70,
54 READ_MISR_EX=73,
55 READ_PAGE_FAIM=80,
56 WRITE_PAGE_FAIM=81
57 }IAP_Command_Code;
58
59 void exec_iap_cmd(const PLATFORM_TypeDef * info, uint32_t param_tab[], uint32_t result_tab[]);
60
61 #endif /* __MW_IAP_H__ */