| USBD ROM Stack 1.0 ROM based USB device stack

Data Fields
USB_OTHER_SPEED_CONFIGURATION Struct Reference
USB Core Layer

`#include <mw_usbd/mw_usbd.h>`

## Data Fields
uint8_t | bLength
uint8_t | bDescriptorType
uint16_t | wTotalLength
uint8_t | bNumInterfaces
uint8_t | bConfigurationValue
uint8_t | IConfiguration
uint8_t | bmAttributes
uint8_t | bMaxPower

## Detailed Description

USB Other Speed Configuration

## Field Documentation

## ◆ bLength

uint8_t USB_OTHER_SPEED_CONFIGURATION::bLength

Size of descriptor

## ◆ bDescriptorType

uint8_t USB_OTHER_SPEED_CONFIGURATION::bDescriptorType

Other_speed_Configuration Type

## ◆ wTotalLength

uint16_t USB_OTHER_SPEED_CONFIGURATION::wTotalLength

Total length of data returned

## ◆ bNumInterfaces

uint8_t USB_OTHER_SPEED_CONFIGURATION::bNumInterfaces

Number of interfaces supported by this speed configuration

## ◆ bConfigurationValue

uint8_t USB_OTHER_SPEED_CONFIGURATION::bConfigurationValue

Value to use to select configuration

## ◆ IConfiguration

uint8_t USB_OTHER_SPEED_CONFIGURATION::IConfiguration

Index of string descriptor

## ◆ bmAttributes

uint8_t USB_OTHER_SPEED_CONFIGURATION::bmAttributes

Same as Configuration descriptor

## ◆ bMaxPower

uint8_t USB_OTHER_SPEED_CONFIGURATION::bMaxPower

Same as Configuration descriptor

The documentation for this struct was generated from the following file:

- mw_usbd/mw_usbd.h