<?xml version='1.0' encoding='UTF-8' standalone='no'?>
<doxygen xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:noNamespaceSchemaLocation="compound.xsd" version="1.8.13">
  <compounddef id="group___u_s_b_d___m_s_c" kind="group">
    <compoundname>USBD_MSC</compoundname>
    <title>Mass Storage Class (MSC) Function Driver</title>
    <innerclass refid="struct_u_s_b_d___m_s_c___i_n_i_t___p_a_r_a_m___t" prot="public">USBD_MSC_INIT_PARAM_T</innerclass>
    <innerclass refid="struct_u_s_b_d___m_s_c___a_p_i___t" prot="public">USBD_MSC_API_T</innerclass>
    <briefdescription>
    </briefdescription>
    <detaileddescription>
<sect1 id="group___u_s_b_d___m_s_c_1Sec_MSCModDescription">
<title>Module Description</title>
<para>MSC Class Function Driver module. This module contains an internal implementation of the USB MSC Class. User applications can use this class driver instead of implementing the MSC class manually via the low-level USBD_HW and USBD_Core APIs.</para><para>This module is designed to simplify the user code by exposing only the required interface needed to interface with Devices using the USB MSC Class. </para></sect1>
    </detaileddescription>
  </compounddef>
</doxygen>
