#

##

##

##

##

##

##

    µVision Build Log
    Tool Versions:
    IDE-Version: ¦ÌVision V5.26.2.0
    Copyright (C) 2018 ARM Ltd and ARM Germany GmbH. All rights reserved.
    License Information: Adision Zhang, NXP, LIC=MGX64-ZKV8L-6BXM8-LVKCH-LP21Y-W1ZVP

    Tool Versions:
    Toolchain:       MDK-ARM Professional  Version: 5.26.2.0
    Toolchain Path:  C:\Keil_v5\ARM\ARMCC\Bin
    C Compiler:      Armcc.exe V5.06 update 6 (build 750)
    Assembler:       Armasm.exe V5.06 update 6 (build 750)
    Linker/Locator:  ArmLink.exe V5.06 update 6 (build 750)
    Library Manager: ArmAr.exe V5.06 update 6 (build 750)
    Hex Converter:   FromElf.exe V5.06 update 6 (build 750)
    CPU DLL:         SARMCM3.DLL V5.26.2.0
    Dialog DLL:      DARMCM1.DLL V1.19.1.0
    Target DLL:      CMSIS_AGDI.dll V1.30.6.0
    Dialog DLL:      TARMCM1.DLL V1.14.0.0

    Project:
    C:\Adision Zhang\0_Main work\10_LPC845_I2C_SPI_SBL\AN_Adision\Final package_SPI\keil_project\LPC845_SPI_SBL_V1.5_2019_01_02_14\LPC845_SPI_SBL\Keil_Projects\LPC804_I2C_SBL\LPC804_I2C_SBL.uvprojx
    Project File Date:  12/27/2018

    Output:
    *** Using Compiler 'V5.06 update 6 (build 750)', folder: 'C:\Keil_v5\ARM\ARMCC\Bin'
    Rebuild target 'flash'
    Clean started - Project: 'LPC804_I2C_SBL'
       deleting intermediate output files for target 'flash'
    compiling system.c...
    assembling Keil_startup.s...
    compiling crc_8xx.c...
    compiling i2c_common_8xx.c...
    compiling i2cs_8xx.c...
    compiling sl_app_entry.c...
    compiling sl_app_entry_place.c...
    compiling sl_crc_check.c...
    compiling sl_flash.c...
    compiling sl_hostif.c...
    compiling sl_hostif_i2c.c...
    compiling sl_main.c...
    ..\..\Source_Code\lpc804_i2c_sbl\sbl\sl_main.c(433): warning:  #2532-D: support for trigraphs is disabled
            startHostIfSPI();                                               //--??--Preload data to TXDATA to response master
    ..\..\Source_Code\lpc804_i2c_sbl\sbl\sl_main.c(465): warning:  #111-D: statement is unreachable
            return 0;
    ..\..\Source_Code\lpc804_i2c_sbl\sbl\sl_main.c(96): warning:  #177-D: variable "pinCfgData"  was declared but never referenced
      static SL_PINSETUP_T *pinCfgData = (SL_PINSETUP_T *) SL_ADDRESS_APPPINDATA;
    ..\..\Source_Code\lpc804_i2c_sbl\sbl\sl_main.c: 3 warnings, 0 errors
    compiling sl_pin_manager.c...
    compiling sl_hostif_spi.c...
    ..\..\Source_Code\lpc804_i2c_sbl\sbl\sl_hostif_spi.c(147): warning:  #550-D: variable "func"  was set but never used
            uint32_t func;
    ..\..\Source_Code\lpc804_i2c_sbl\sbl\sl_hostif_spi.c(271): warning:  #2532-D: support for trigraphs is disabled
            /* Slave assertion, CS pin is pulled low */                                             //--??--CS Low is working state
    ..\..\Source_Code\lpc804_i2c_sbl\sbl\sl_hostif_spi.c: 2 warnings, 0 errors
    compiling spis_8xx.c...
    linking...
    .\Objects\lpc804_i2c_sbl.axf: Warning: L6319W: Ignoring --keep command. Cannot find section sl_app_entry_place.o(sect_reenter).
    ..\..\Source_Code\lpc804_i2c_sbl\support\secondary_loader.sct(16): warning: L6314W: No section matches pattern sl_app_entry_place.o(sect_reenter).
    Program Size: Code=4236 RO-data=440 RW-data=92 ZI-data=2772
    Finished: 0 information, 2 warning and 0 error messages.
    ".\Objects\lpc804_i2c_sbl.axf" - 0 Error(s), 7 Warning(s).

    *** Performing Cross-Module-Optimization:
    compiling system.c...
    compiling crc_8xx.c...
    compiling i2c_common_8xx.c...
    compiling i2cs_8xx.c...
    compiling sl_app_entry.c...
    compiling sl_app_entry_place.c...
    compiling sl_crc_check.c...
    compiling sl_flash.c...
    compiling sl_hostif.c...
    compiling sl_hostif_i2c.c...
    compiling sl_main.c...
    ..\..\Source_Code\lpc804_i2c_sbl\sbl\sl_main.c(433): warning:  #2532-D: support for trigraphs is disabled
            startHostIfSPI();                                               //--??--Preload data to TXDATA to response master
    ..\..\Source_Code\lpc804_i2c_sbl\sbl\sl_main.c(465): warning:  #111-D: statement is unreachable
            return 0;
    ..\..\Source_Code\lpc804_i2c_sbl\sbl\sl_main.c(96): warning:  #177-D: variable "pinCfgData"  was declared but never referenced
      static SL_PINSETUP_T *pinCfgData = (SL_PINSETUP_T *) SL_ADDRESS_APPPINDATA;
    ..\..\Source_Code\lpc804_i2c_sbl\sbl\sl_main.c: 3 warnings, 0 errors
    compiling sl_pin_manager.c...
    compiling sl_hostif_spi.c...
    ..\..\Source_Code\lpc804_i2c_sbl\sbl\sl_hostif_spi.c(147): warning:  #550-D: variable "func"  was set but never used
            uint32_t func;
    ..\..\Source_Code\lpc804_i2c_sbl\sbl\sl_hostif_spi.c(271): warning:  #2532-D: support for trigraphs is disabled
            /* Slave assertion, CS pin is pulled low */                                             //--??--CS Low is working state
    ..\..\Source_Code\lpc804_i2c_sbl\sbl\sl_hostif_spi.c: 2 warnings, 0 errors
    compiling spis_8xx.c...
    linking...
    .\Objects\lpc804_i2c_sbl.axf: Warning: L6319W: Ignoring --keep command. Cannot find section sl_app_entry_place.o(sect_reenter).
    ..\..\Source_Code\lpc804_i2c_sbl\support\secondary_loader.sct(16): warning: L6314W: No section matches pattern sl_app_entry_place.o(sect_reenter).
    Program Size: Code=4236 RO-data=440 RW-data=92 ZI-data=2772
    Finished: 0 information, 2 warning and 0 error messages.
    FromELF: creating hex file...
    After Build - User command #1: C:\Keil_v5\\ARM\BIN\ELFDWT.EXE .\Objects\lpc804_i2c_sbl.axf BASEADDRESS(0x00000000)
    ELFDWT - Signature Creator V1.4.0.0
    COPYRIGHT Copyright (C) 2014-2018, ARM Ldt. and  ARM Germany GmbH
    *** Updated Signature over Range[32] (0x00000000 - 0x00000018): @0x0000001C = 0xEFFFF1F3
    *** Processing completed, no Errors.
    After Build - User command #2: C:\Keil_v5\\ARM\ARMCC\bin\fromelf.exe --bin --output=lpc804_i2c_sbl.bin .\Objects\lpc804_i2c_sbl.axf
    ".\Objects\lpc804_i2c_sbl.axf" - 0 Error(s), 7 Warning(s).
    *** Completed Cross-Module-Optimization after 2 iteration(s).

    Software Packages used:

    Package Vendor: NXP
                    http://mcuxpresso.nxp.com/cmsis_pack/repo/NXP.LPC845_DFP.10.0.3.pack
                    NXP.LPC845_DFP.10.0.3
                    Device Family Pack for LPC845

    Collection of Component include folders:
      .\RTE\_flash
      C:\Keil_v5\ARM\PACK\NXP\LPC845_DFP\10.0.3

    Collection of Component Files used:
    Build Time Elapsed:  00:00:24