| ISF 1.1 Intelligent Sensing Framework

- Main Page
- Data Structures
- Files
- Sensor Adapters

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Defines
Data Fields
NVOPTSTR Union Reference

`#include <fxlc95000.h>`

## Data Fields
byte | Byte
struct {
byte SSC0:1
byte SSC1:1
byte SSW:1
byte __pad0__:1
byte PROTB:1
byte PW:1
byte __pad1__:1
byte __pad2__:1
} | Bits
struct {
byte grpSSC:2
byte __pad0__:1
byte __pad1__:1
byte __pad2__:1
byte __pad3__:1
byte __pad4__:1
byte __pad5__:1
} | MergedBits

## Detailed Description

Definition at line 386 of file fxlc95000.h.

## Field Documentation

byte __pad0__

Definition at line 392 of file fxlc95000.h.

byte __pad1__

Definition at line 395 of file fxlc95000.h.

byte __pad2__

Definition at line 396 of file fxlc95000.h.

byte __pad3__

Definition at line 403 of file fxlc95000.h.

byte __pad4__

Definition at line 404 of file fxlc95000.h.

byte __pad5__

Definition at line 405 of file fxlc95000.h.

struct { ... } Bits

byte Byte

Definition at line 387 of file fxlc95000.h.

byte grpSSC

Definition at line 399 of file fxlc95000.h.

struct { ... } MergedBits

byte PROTB

Definition at line 393 of file fxlc95000.h.

byte PW

Definition at line 394 of file fxlc95000.h.

byte SSC0

Definition at line 389 of file fxlc95000.h.

byte SSC1

Definition at line 390 of file fxlc95000.h.

byte SSW

Definition at line 391 of file fxlc95000.h.

The documentation for this union was generated from the following file:

- Include/psp/fxlc95000.h