| ISF 1.1 Intelligent Sensing Framework

- Main Page
- Data Structures
- Files
- Sensor Adapters

- File List
- Globals

- All
- Functions
- Variables
- Typedefs
- Enumerations
- Enumerator
- Defines

- _
- a
- b
- c
- d
- e
- f
- g
- h
- i
- l
- m
- n
- o
- p
- r
- s
- t
- u
- v
- w
- y

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Defines
Here is a list of all functions, variables, defines, enums, and typedefs with links to the files they belong to:

### - c -

- CI_CMD_LAST : isf_ci.h
- CI_CMD_MAX : isf_ci.h
- CI_CMD_READ_APP_DATA : isf_ci.h
- CI_CMD_READ_APP_STATUS : isf_ci.h
- CI_CMD_READ_CONFIG : isf_ci.h
- CI_CMD_READ_VERSION : isf_ci.h
- CI_CMD_UPDATE_QUICKREAD : isf_ci.h
- CI_CMD_WRITE_CONFIG : isf_ci.h
- ci_commands_enum : isf_ci.h
- CI_ERROR_CB_NOT_REGISTERED : isf_ci.h
- CI_ERROR_COMMAND : isf_ci.h
- CI_ERROR_FIFO_ALLOCATED : isf_ci.h
- CI_ERROR_FIFO_BUSY : isf_ci.h
- CI_ERROR_FIFO_OVERSIZE : isf_ci.h
- CI_ERROR_INVALID_LENGTH : isf_ci.h
- CI_ERROR_MAX : isf_ci.h
- CI_ERROR_NONE : isf_ci.h
- CI_ERROR_PARAM : isf_ci.h
- ci_funcp_t : isf_ci.h
- ci_init() : isf_ci.h
- CI_INVALID_COUNT : isf_ci.h
- ci_response_enum : isf_ci.h
- ci_response_t : isf_ci.h
- ci_rw_enum : isf_ci.h
- CI_RW_NULL : isf_ci.h
- CI_RW_READ : isf_ci.h
- CI_RW_WRITE : isf_ci.h
- ci_status_enum : isf_ci.h
- ci_status_t : isf_ci.h
- CK_OSCTRL : fxlc95000.h
- CK_OSCTRL_FCEN : fxlc95000.h
- CK_OSCTRL_FCEN_MASK : fxlc95000.h
- CK_OSCTRL_FFCEN : fxlc95000.h
- CK_OSCTRL_FFCEN_MASK : fxlc95000.h
- CK_OSCTRL_FFSEN : fxlc95000.h
- CK_OSCTRL_FFSEN_MASK : fxlc95000.h
- CK_OSCTRL_FLE : fxlc95000.h
- CK_OSCTRL_FLE_BITNUM : fxlc95000.h
- CK_OSCTRL_FLE_MASK : fxlc95000.h
- CK_TRIM : fxlc95000.h
- CK_TRIM_TRIMH : fxlc95000.h
- CK_TRIM_TRIMH_BITNUM : fxlc95000.h
- CK_TRIM_TRIMH_MASK : fxlc95000.h
- CK_TRIM_TRIML : fxlc95000.h
- CK_TRIM_TRIML_BITNUM : fxlc95000.h
- CK_TRIM_TRIML_MASK : fxlc95000.h
- CK_TRIMH : fxlc95000.h
- CK_TRIMHL : fxlc95000.h
- CK_TRIMHM : fxlc95000.h
- CK_TRIML : fxlc95000.h
- CK_TRIMLL : fxlc95000.h
- CK_TRIMLM : fxlc95000.h
- comm_Address_t : isf_comm.h
- COMM_CMD_DEFN : isf_comm.h
- comm_Command_t : isf_comm.h
- COMM_ERROR_BUF_SIZE : isf_comm.h
- COMM_ERROR_DEV_CLOSED : isf_comm.h
- COMM_ERROR_INIT : isf_comm.h
- COMM_ERROR_LOCK : isf_comm.h
- COMM_ERROR_NO_ACK : isf_comm.h
- COMM_ERROR_NOEXIST : isf_comm.h
- COMM_ERROR_NULL_PTR : isf_comm.h
- COMM_ERROR_OTHER : isf_comm.h
- COMM_ERROR_STOP : isf_comm.h
- COMM_ERROR_TIME_OUT : isf_comm.h
- comm_Error_vals : isf_comm.h
- comm_Flags_t : isf_comm.h
- comm_Id_t : isf_comm.h
- comm_MessageBuffer_t : isf_comm.h
- COMM_SIZED_BUFFER : isf_comm.h
- COMM_STATE_ARB_LOST : isf_comm.h
- COMM_STATE_ERROR : isf_comm.h
- COMM_STATE_INIT : isf_comm.h
- COMM_STATE_LOCKED : isf_comm.h
- COMM_STATE_NO_INIT : isf_comm.h
- COMM_STATE_OK : isf_comm.h
- COMM_STATE_STOPPED : isf_comm.h
- comm_State_t : isf_comm.h
- comm_State_vals : isf_comm.h
- CRC : fxlc95000.h
- CRC_CRC0 : fxlc95000.h
- CRC_CRC0_MASK : fxlc95000.h
- CRC_CRC1 : fxlc95000.h
- CRC_CRC10 : fxlc95000.h
- CRC_CRC10_MASK : fxlc95000.h
- CRC_CRC11 : fxlc95000.h
- CRC_CRC11_MASK : fxlc95000.h
- CRC_CRC12 : fxlc95000.h
- CRC_CRC12_MASK : fxlc95000.h
- CRC_CRC13 : fxlc95000.h
- CRC_CRC13_MASK : fxlc95000.h
- CRC_CRC14 : fxlc95000.h
- CRC_CRC14_MASK : fxlc95000.h
- CRC_CRC15 : fxlc95000.h
- CRC_CRC15_MASK : fxlc95000.h
- CRC_CRC1_MASK : fxlc95000.h
- CRC_CRC2 : fxlc95000.h
- CRC_CRC2_MASK : fxlc95000.h
- CRC_CRC3 : fxlc95000.h
- CRC_CRC3_MASK : fxlc95000.h
- CRC_CRC4 : fxlc95000.h
- CRC_CRC4_MASK : fxlc95000.h
- CRC_CRC5 : fxlc95000.h
- CRC_CRC5_MASK : fxlc95000.h
- CRC_CRC6 : fxlc95000.h
- CRC_CRC6_MASK : fxlc95000.h
- CRC_CRC7 : fxlc95000.h
- CRC_CRC7_MASK : fxlc95000.h
- CRC_CRC8 : fxlc95000.h
- CRC_CRC8_MASK : fxlc95000.h
- CRC_CRC9 : fxlc95000.h
- CRC_CRC9_MASK : fxlc95000.h
- isf_ci_app_read() : isf_ci.h
- isf_ci_app_write() : isf_ci.h
- isf_ci_assert_int_o() : isf_ci.h
- isf_ci_enable_int_o() : isf_ci.h
- isf_ci_qr_update() : isf_ci.h
- isf_ci_set_int_o_polarity() : isf_ci.h