| ISF 1.1 Intelligent Sensing Framework

- Main Page
- Data Structures
- Files
- Sensor Adapters

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Defines
Data Fields
TPMC0SCSTR Union Reference

`#include <fxlc95000.h>`

## Data Fields
byte | Byte
struct {
byte __pad0__:1
byte __pad1__:1
byte ELS0A:1
byte ELS0B:1
byte MS0A:1
byte MS0B:1
byte CH0IE:1
byte CH0F:1
} | Bits
struct {
byte __pad0__:1
byte __pad1__:1
byte grpELS0x:2
byte grpMS0x:2
byte __pad2__:1
byte __pad3__:1
} | MergedBits

## Detailed Description

Definition at line 3169 of file fxlc95000.h.

## Field Documentation

byte __pad0__

Definition at line 3172 of file fxlc95000.h.

byte __pad1__

Definition at line 3173 of file fxlc95000.h.

byte __pad2__

Definition at line 3186 of file fxlc95000.h.

byte __pad3__

Definition at line 3187 of file fxlc95000.h.

struct { ... } Bits

byte Byte

Definition at line 3170 of file fxlc95000.h.

byte CH0F

Definition at line 3179 of file fxlc95000.h.

byte CH0IE

Definition at line 3178 of file fxlc95000.h.

byte ELS0A

Definition at line 3174 of file fxlc95000.h.

byte ELS0B

Definition at line 3175 of file fxlc95000.h.

byte grpELS0x

Definition at line 3184 of file fxlc95000.h.

byte grpMS0x

Definition at line 3185 of file fxlc95000.h.

struct { ... } MergedBits

byte MS0A

Definition at line 3176 of file fxlc95000.h.

byte MS0B

Definition at line 3177 of file fxlc95000.h.

The documentation for this union was generated from the following file:

- Include/psp/fxlc95000.h