| ISF 1.1 Intelligent Sensing Framework

- Main Page
- Data Structures
- Files
- Sensor Adapters

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Defines
Data Fields
TPMC1SCSTR Union Reference

`#include <fxlc95000.h>`

## Data Fields
byte | Byte
struct {
byte __pad0__:1
byte __pad1__:1
byte ELS1A:1
byte ELS1B:1
byte MS1A:1
byte MS1B:1
byte CH1IE:1
byte CH1F:1
} | Bits
struct {
byte __pad0__:1
byte __pad1__:1
byte grpELS1x:2
byte grpMS1x:2
byte __pad2__:1
byte __pad3__:1
} | MergedBits

## Detailed Description

Definition at line 3239 of file fxlc95000.h.

## Field Documentation

byte __pad0__

Definition at line 3242 of file fxlc95000.h.

byte __pad1__

Definition at line 3243 of file fxlc95000.h.

byte __pad2__

Definition at line 3256 of file fxlc95000.h.

byte __pad3__

Definition at line 3257 of file fxlc95000.h.

struct { ... } Bits

byte Byte

Definition at line 3240 of file fxlc95000.h.

byte CH1F

Definition at line 3249 of file fxlc95000.h.

byte CH1IE

Definition at line 3248 of file fxlc95000.h.

byte ELS1A

Definition at line 3244 of file fxlc95000.h.

byte ELS1B

Definition at line 3245 of file fxlc95000.h.

byte grpELS1x

Definition at line 3254 of file fxlc95000.h.

byte grpMS1x

Definition at line 3255 of file fxlc95000.h.

struct { ... } MergedBits

byte MS1A

Definition at line 3246 of file fxlc95000.h.

byte MS1B

Definition at line 3247 of file fxlc95000.h.

The documentation for this union was generated from the following file:

- Include/psp/fxlc95000.h