| ISF 1.1 Intelligent Sensing Framework

- Main Page
- Data Structures
- Files
- Sensor Adapters

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Defines
Data Fields
TPMSCSTR Union Reference

`#include <fxlc95000.h>`

## Data Fields
byte | Byte
struct {
byte PS0:1
byte PS1:1
byte PS2:1
byte CLKSA:1
byte CLKSB:1
byte CPWMS:1
byte TOIE:1
byte TOF:1
} | Bits
struct {
byte grpPS:3
byte grpCLKSx:2
byte __pad0__:1
byte __pad1__:1
byte __pad2__:1
} | MergedBits

## Detailed Description

Definition at line 3071 of file fxlc95000.h.

## Field Documentation

byte __pad0__

Definition at line 3086 of file fxlc95000.h.

byte __pad1__

Definition at line 3087 of file fxlc95000.h.

byte __pad2__

Definition at line 3088 of file fxlc95000.h.

struct { ... } Bits

byte Byte

Definition at line 3072 of file fxlc95000.h.

byte CLKSA

Definition at line 3077 of file fxlc95000.h.

byte CLKSB

Definition at line 3078 of file fxlc95000.h.

byte CPWMS

Definition at line 3079 of file fxlc95000.h.

byte grpCLKSx

Definition at line 3085 of file fxlc95000.h.

byte grpPS

Definition at line 3084 of file fxlc95000.h.

struct { ... } MergedBits

byte PS0

Definition at line 3074 of file fxlc95000.h.

byte PS1

Definition at line 3075 of file fxlc95000.h.

byte PS2

Definition at line 3076 of file fxlc95000.h.

byte TOF

Definition at line 3081 of file fxlc95000.h.

byte TOIE

Definition at line 3080 of file fxlc95000.h.

The documentation for this union was generated from the following file:

- Include/psp/fxlc95000.h