| ISF 1.1 Intelligent Sensing Framework

- Main Page
- Data Structures
- Files
- Sensor Adapters

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Defines
Data Fields
PMCR0STR Union Reference

`#include <fxlc95000.h>`

## Data Fields
byte | Byte
struct {
byte A4:1
byte __pad0__:1
byte A6:2
byte A7:2
byte A8:1
byte A9:1
} | Bits
struct {
byte grpA_4:1
byte __pad0__:1
byte __pad1__:2
byte __pad2__:2
byte grpA_8:2
} | MergedBits

## Detailed Description

Definition at line 2415 of file fxlc95000.h.

## Field Documentation

byte __pad0__

Definition at line 2419 of file fxlc95000.h.

byte __pad1__

Definition at line 2428 of file fxlc95000.h.

byte __pad2__

Definition at line 2429 of file fxlc95000.h.

byte A4

Definition at line 2418 of file fxlc95000.h.

byte A6

Definition at line 2420 of file fxlc95000.h.

byte A7

Definition at line 2421 of file fxlc95000.h.

byte A8

Definition at line 2422 of file fxlc95000.h.

byte A9

Definition at line 2423 of file fxlc95000.h.

struct { ... } Bits

byte Byte

Definition at line 2416 of file fxlc95000.h.

byte grpA_4

Definition at line 2426 of file fxlc95000.h.

byte grpA_8

Definition at line 2430 of file fxlc95000.h.

struct { ... } MergedBits

The documentation for this union was generated from the following file:

- Include/psp/fxlc95000.h