| ISF 1.1 Intelligent Sensing Framework

- Main Page
- Data Structures
- Files
- Sensor Adapters

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Defines
Data Fields
comm_Command_struct Struct Reference

This structure defines the command sent to a device. More...

`#include <isf_comm.h>`

## Data Fields
uint16 | nWrite
uint16 | nRead
uint8 | cmdWords []

## Detailed Description

This structure defines the command sent to a device.

Definition at line 81 of file isf_comm.h.

## Field Documentation

uint8 cmdWords[]

Command buffer associated with the data.

Definition at line 84 of file isf_comm.h.

uint16 nRead

Number of bytes to read.

Definition at line 83 of file isf_comm.h.

uint16 nWrite

Number of bytes to write.

Definition at line 82 of file isf_comm.h.

The documentation for this struct was generated from the following file:

- Include/isf_comm.h