| ISF 1.1 Intelligent Sensing Framework

- Main Page
- Data Structures
- Files
- Sensor Adapters

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Defines
Data Fields
PCESSC0STR Union Reference

`#include <fxlc95000.h>`

## Data Fields
byte | Byte
struct {
byte FLSH:1
byte PCTRL:1
byte AFE:1
byte IRQ:1
byte T0:1
byte T1:1
byte T2:1
byte __pad0__:1
} | Bits
struct {
byte __pad0__:1
byte __pad1__:1
byte __pad2__:1
byte __pad3__:1
byte grpT:3
byte __pad4__:1
} | MergedBits

## Detailed Description

Definition at line 2273 of file fxlc95000.h.

## Field Documentation

byte __pad0__

Definition at line 2283 of file fxlc95000.h.

byte __pad1__

Definition at line 2287 of file fxlc95000.h.

byte __pad2__

Definition at line 2288 of file fxlc95000.h.

byte __pad3__

Definition at line 2289 of file fxlc95000.h.

byte __pad4__

Definition at line 2291 of file fxlc95000.h.

byte AFE

Definition at line 2278 of file fxlc95000.h.

struct { ... } Bits

byte Byte

Definition at line 2274 of file fxlc95000.h.

byte FLSH

Definition at line 2276 of file fxlc95000.h.

byte grpT

Definition at line 2290 of file fxlc95000.h.

byte IRQ

Definition at line 2279 of file fxlc95000.h.

struct { ... } MergedBits

byte PCTRL

Definition at line 2277 of file fxlc95000.h.

byte T0

Definition at line 2280 of file fxlc95000.h.

byte T1

Definition at line 2281 of file fxlc95000.h.

byte T2

Definition at line 2282 of file fxlc95000.h.

The documentation for this union was generated from the following file:

- Include/psp/fxlc95000.h