| ISF 1.1 Intelligent Sensing Framework

- Main Page
- Data Structures
- Files
- Sensor Adapters

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Defines
Data Fields
ctrl_reg_t Union Reference

The generic control register structure for user applications. More...

`#include <isf_hostproxy.h>`

## Data Fields
uint8 | reg
struct {
uint8 startStop:1
uint8 subState:1
uint8 hostIntEn:1
uint8 quickReadEn:1
uint8 reserved:4
} | Bits

## Detailed Description

The generic control register structure for user applications.

Definition at line 25 of file isf_hostproxy.h.

## Field Documentation

struct { ... } Bits

uint8 hostIntEn

The host interrupt bit. Setting this bit enables the host interrupt. Clearing this bit disables the host interrupt.

Definition at line 30 of file isf_hostproxy.h.

uint8 quickReadEn

The quick read bit for the application. Setting this bit enables the quick read. Clearing this bit disables the quick read.

Definition at line 31 of file isf_hostproxy.h.

uint8 reg

The control byte.

Definition at line 26 of file isf_hostproxy.h.

uint8 reserved

These bits are for future use.

Definition at line 32 of file isf_hostproxy.h.

uint8 startStop

The data streaming bit. When this bit is set, data streaming is enabled. Data streaming is disabled by clearing this bit.

Definition at line 28 of file isf_hostproxy.h.

uint8 subState

The subscription state bit. Setting this bit enables the subscription. Clearing this bit disables the subscription.

Definition at line 29 of file isf_hostproxy.h.

The documentation for this union was generated from the following file:

- Include/isf_hostproxy.h