| ISF 1.1 Intelligent Sensing Framework

- Main Page
- Data Structures
- Files
- Sensor Adapters

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Defines
Data Fields
i2c_State_struct Struct Reference

This structure defines the I2C state. More...

`#include <isf_i2cconf_types.h>`

## Data Fields
uint8 | busState
uint8 | cDriverState
uint8 | writeRead
uint8 | isRestart

## Detailed Description

This structure defines the I2C state.

Definition at line 59 of file isf_i2cconf_types.h.

## Field Documentation

uint8 busState

The bus state.

Definition at line 60 of file isf_i2cconf_types.h.

uint8 cDriverState

The current driver state.

Definition at line 61 of file isf_i2cconf_types.h.

uint8 isRestart

The flag for restart.

Definition at line 63 of file isf_i2cconf_types.h.

uint8 writeRead

The flag for read and write in a single transaction.

Definition at line 62 of file isf_i2cconf_types.h.

The documentation for this struct was generated from the following file:

- Include/isf_i2cconf_types.h