| ISF 1.1 Intelligent Sensing Framework

- Main Page
- Data Structures
- Files
- Sensor Adapters

- File List
- Globals

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Defines
Variables
User/Source/isf_hostproxyconfig.c File Reference

This file defines the host configuration structure. More...

`#include "isf_hostproxy.h"`
`#include "isf_hostproxyconfig.h"`

Go to the source code of this file.

## Variables
hp_Config_t | proxyConfigTable []
| The table defines the Host Proxy configuration. If the user application registers with the Host Proxy, the configuration table should be updated with the proxy instance. For example, if a FXLC95000 accelerometer application registers with the Host Proxy, the proxy number and the user application specific configuration instance should be inserted into the proxy configuration table. hp_Config_t proxyConfigTable[] = { { .proxyNo = APP_PROXY_NO_FXCL95000_ACCEL, .appConfig = &fxlc95000Config } }; uint8 numberOfProxy = sizeof(proxyConfigTable)/sizeof(hp_Config_t);.
uint8 | numberOfProxy = 0
| The number of proxy instances registered with the Host Proxy.

## Detailed Description

This file defines the host configuration structure.

Definition in file isf_hostproxyconfig.c.

## Variable Documentation

uint8 numberOfProxy = 0

The number of proxy instances registered with the Host Proxy.

Definition at line 38 of file isf_hostproxyconfig.c.

hp_Config_t proxyConfigTable[]

Initial value:

     {
                                    {
                                    .proxyNo = 0,
                                    .appConfig = NULL
                                    }
    }

The table defines the Host Proxy configuration. If the user application registers with the Host Proxy, the configuration table should be updated with the proxy instance. For example, if a FXLC95000 accelerometer application registers with the Host Proxy, the proxy number and the user application specific configuration instance should be inserted into the proxy configuration table. hp_Config_t proxyConfigTable[] = { { .proxyNo = APP_PROXY_NO_FXCL95000_ACCEL, .appConfig = &fxlc95000Config } }; uint8 numberOfProxy = sizeof(proxyConfigTable)/sizeof(hp_Config_t);.

Definition at line 30 of file isf_hostproxyconfig.c.