| ISF 1.1 Intelligent Sensing Framework

- Main Page
- Data Structures
- Files
- Sensor Adapters

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Defines
Data Fields
hp_hostUpdate_struct Struct Reference

This is the structure defined for the user application to update the host. More...

`#include <isf_hostproxy.h>`

## Data Fields
uint8 | isQuickReadUpdate
uint8 | isHostInt
uint8 | size
uint8 | AppId
uint8 * | pDataBuffer

## Detailed Description

This is the structure defined for the user application to update the host.

Definition at line 37 of file isf_hostproxy.h.

## Field Documentation

uint8 AppId

The current application ID for the user application.

Definition at line 41 of file isf_hostproxy.h.

uint8 isHostInt

Status indicating whether or not host interrupt is enabled.

Definition at line 39 of file isf_hostproxy.h.

uint8 isQuickReadUpdate

Status indicating whether or not Quick Read is enabled.

Definition at line 38 of file isf_hostproxy.h.

uint8* pDataBuffer

The buffer containing user application data.

Definition at line 42 of file isf_hostproxy.h.

uint8 size

The size of the buffer holding user application data.

Definition at line 40 of file isf_hostproxy.h.

The documentation for this struct was generated from the following file:

- Include/isf_hostproxy.h