| ISF 1.1 Intelligent Sensing Framework

- Main Page
- Data Structures
- Files
- Sensor Adapters

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Defines
Data Fields
sm_SensorConfigSettings_st Struct Reference

This defines the DSA sensor configuration parameter structure configuring the sensor settings by a subscriber task. More...

`#include <isf_sm_dsa_adapter.h>`

## Data Fields
uint32 | nSampleRate
uint8 | nResolution
uint8 | nRange
uint8 | nMode

## Detailed Description

This defines the DSA sensor configuration parameter structure configuring the sensor settings by a subscriber task.

Definition at line 114 of file isf_sm_dsa_adapter.h.

## Field Documentation

uint8 nMode

Sensor specific mode.

Definition at line 123 of file isf_sm_dsa_adapter.h.

uint8 nRange

Sensor dynamic range.

Definition at line 121 of file isf_sm_dsa_adapter.h.

uint8 nResolution

Sample resolution.

Definition at line 119 of file isf_sm_dsa_adapter.h.

uint32 nSampleRate

Sample period in microseconds.

Definition at line 117 of file isf_sm_dsa_adapter.h.

The documentation for this struct was generated from the following file:

- Include/isf_sm_dsa_adapter.h