| ISF 1.1 Intelligent Sensing Framework

- Main Page
- Data Structures
- Files
- Sensor Adapters

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Defines
Data Fields
sm_Dsa_SensorStatus_st Struct Reference

This defines the DSA adapter sensor status bit-field structure. More...

`#include <isf_sm_dsa_adapter.h>`

## Data Fields
uint8 | bAvailable: 1
uint8 | bInitialized: 1
uint8 | bSensorOn: 1
uint8 | bDummy: 5

## Detailed Description

This defines the DSA adapter sensor status bit-field structure.

Definition at line 86 of file isf_sm_dsa_adapter.h.

## Field Documentation

uint8 bAvailable

The current sensor is available for use.

Definition at line 89 of file isf_sm_dsa_adapter.h.

uint8 bDummy

Unused bits.

Definition at line 95 of file isf_sm_dsa_adapter.h.

uint8 bInitialized

The current sensor is initialized.

Definition at line 91 of file isf_sm_dsa_adapter.h.

uint8 bSensorOn

The current sensor is on.

Definition at line 93 of file isf_sm_dsa_adapter.h.

The documentation for this struct was generated from the following file:

- Include/isf_sm_dsa_adapter.h