| ISF 1.1 Intelligent Sensing Framework

- Main Page
- Data Structures
- Files
- Sensor Adapters

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Defines
Data Fields
IICC2STR Union Reference

`#include <fxlc95000.h>`

## Data Fields
byte | Byte
struct {
byte AD8:1
byte AD9:1
byte AD10:1
byte __pad0__:1
byte __pad1__:1
byte __pad2__:1
byte ADEXT:1
byte GCAEN:1
} | Bits
struct {
byte grpAD_8:3
byte __pad0__:1
byte __pad1__:1
byte __pad2__:1
byte __pad3__:1
byte __pad4__:1
} | MergedBits

## Detailed Description

Definition at line 2015 of file fxlc95000.h.

## Field Documentation

byte __pad0__

Definition at line 2021 of file fxlc95000.h.

byte __pad1__

Definition at line 2022 of file fxlc95000.h.

byte __pad2__

Definition at line 2023 of file fxlc95000.h.

byte __pad3__

Definition at line 2032 of file fxlc95000.h.

byte __pad4__

Definition at line 2033 of file fxlc95000.h.

byte AD10

Definition at line 2020 of file fxlc95000.h.

byte AD8

Definition at line 2018 of file fxlc95000.h.

byte AD9

Definition at line 2019 of file fxlc95000.h.

byte ADEXT

Definition at line 2024 of file fxlc95000.h.

struct { ... } Bits

byte Byte

Definition at line 2016 of file fxlc95000.h.

byte GCAEN

Definition at line 2025 of file fxlc95000.h.

byte grpAD_8

Definition at line 2028 of file fxlc95000.h.

struct { ... } MergedBits

The documentation for this union was generated from the following file:

- Include/psp/fxlc95000.h