| ISF 1.1 Intelligent Sensing Framework

- Main Page
- Data Structures
- Files
- Sensor Adapters

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Defines
Data Fields
fxlc9500x_afe_data_t Struct Reference

A single sample set of AFE sensor data. More...

`#include <fxlc95000_util.h>`

## Data Fields
int16 | data [NUM_SENSOR_AXIS]

## Detailed Description

A single sample set of AFE sensor data.

The fxlc9500x_afe_data_t structure is used to contain a set of raw or trimmed AFE sensor data taken during a single AFE sample. A 16 bit signed value is stored for each axis/sensor, where the number of axis/sensors in each sample is defined in the NUM_SENSOR_AXIS macro.

See also:
  fxlc9500x_framerate_set()

Definition at line 58 of file fxlc95000_util.h.

## Field Documentation

int16 data[NUM_SENSOR_AXIS]

Raw or trimmed value for each axis/sensor

Definition at line 59 of file fxlc95000_util.h.

The documentation for this struct was generated from the following file:

- Include/psp/fxlc95000_util.h