| ISF 1.1 Intelligent Sensing Framework

- Main Page
- Data Structures
- Files
- Sensor Adapters

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Defines
Data Fields
fxlc9500x_vars_t Struct Reference

Freescale firmware variables. More...

`#include <fxlc95000_util.h>`

## Data Fields
uint16 | afe_cm_gain
uint8 | afe_fs_shift
fxlc9500x_idle_t | idle

## Detailed Description

Freescale firmware variables.

This structure holds all of the variables that are used by the Freescale firmware. Most of them can be used by the customer firmware to configure and control the operation of the Freescale firmware.

See also:

Definition at line 286 of file fxlc95000_util.h.

## Field Documentation

uint16 afe_cm_gain

AFE trim configuration - do not modify

Definition at line 287 of file fxlc95000_util.h.

uint8 afe_fs_shift

AFE trim configuration - do not modify

Definition at line 288 of file fxlc95000_util.h.

fxlc9500x_idle_t idle

Idle stop mode configuration - see fxlc9500x_idle_t

Definition at line 290 of file fxlc95000_util.h.

The documentation for this struct was generated from the following file:

- Include/psp/fxlc95000_util.h