| ISF 1.1 Intelligent Sensing Framework

- Main Page
- Data Structures
- Files
- Sensor Adapters

- File List
- Globals

- All
- Functions
- Variables
- Typedefs
- Enumerations
- Enumerator
- Defines

- _
- a
- b
- c
- d
- f
- h
- i
- l
- p
- s
- t

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Defines

### - _ -

- _fw_device_info_get() : isf.h

### - a -

- isf_app_callback_dev_info() : isf_ci.h
- isf_app_callback_mbox() : isf_ci.h

### - b -

- bm_get_num_callback() : isf_bm.h
- bm_init() : isf_bm.h
- bm_register_periodic_callback() : isf_bm.h
- bm_start() : isf_bm.h
- bm_stop() : isf_bm.h
- bm_unregister_callback() : isf_bm.h

### - c -

- ci_init() : isf_ci.h
- isf_ci_app_read() : isf_ci.h
- isf_ci_app_write() : isf_ci.h
- isf_ci_assert_int_o() : isf_ci.h
- isf_ci_enable_int_o() : isf_ci.h
- isf_ci_qr_update() : isf_ci.h
- isf_ci_set_int_o_polarity() : isf_ci.h

### - d -

- dm_channel_acquire_lock() : isf_devmsg.h
- dm_channel_configure() : isf_devmsg.h
- dm_channel_get_config() : isf_devmsg.h
- dm_channel_get_descriptor() : isf_devmsg.h
- dm_channel_get_state() : isf_devmsg.h
- dm_channel_init() : isf_devmsg.h
- dm_channel_release_lock() : isf_devmsg.h
- dm_channel_start() : isf_devmsg.h
- dm_channel_stop() : isf_devmsg.h
- dm_device_close() : isf_devmsg.h
- dm_device_open() : isf_devmsg.h
- dm_device_read() : isf_devmsg.h
- dm_device_readx() : isf_devmsg.h
- dm_device_write() : isf_devmsg.h
- dm_device_writex() : isf_devmsg.h

### - f -

- fxlc9500x_afe_conversion_start() : fxlc95000_util.h
- fxlc9500x_afe_csr_get() : fxlc95000_util.h
- fxlc9500x_afe_csr_set() : fxlc95000_util.h
- fxlc9500x_afe_interrupt_clear() : fxlc95000_util.h
- fxlc9500x_afe_interrupt_set() : fxlc95000_util.h
- fxlc9500x_afe_offsets_get() : fxlc95000_util.h
- fxlc9500x_afe_offsets_set() : fxlc95000_util.h
- fxlc9500x_afe_raw_sensor_data_get() : fxlc95000_util.h
- fxlc9500x_afe_raw_sensor_data_trim() : fxlc95000_util.h
- fxlc9500x_afe_trimmed_sensor_data_get() : fxlc95000_util.h
- fxlc9500x_framerate_set() : fxlc95000_util.h
- fxlc9500x_idle() : fxlc95000_util.h

### - h -

- isf_hp_get_proxy_event() : isf_hostproxy.h
- isf_hp_set_proxy_event() : isf_hostproxy.h

### - i -

- i2c_bus_acquire_lock() : isf_i2c.h
- i2c_bus_configure() : isf_i2c.h
- i2c_bus_enumerate() : isf_i2c.h
- i2c_bus_init() : isf_i2c.h
- i2c_bus_release_lock() : isf_i2c.h
- i2c_bus_start() : isf_i2c.h
- i2c_bus_stop() : isf_i2c.h
- i2c_get_bus_config() : isf_i2c.h
- i2c_get_bus_handle() : isf_i2c.h
- i2c_get_bus_state() : isf_i2c.h
- i2c_get_slave_at() : isf_i2c.h
- i2c_read() : isf_i2c.h
- i2c_write() : isf_i2c.h
- isf_init_task() : isf_init.c , isf_init.h

### - l -

- isf_lib_get_info() : isf.h
- isf_lib_init() : isf_init.c , isf_init.h , isf.h

### - p -

- isf_power_get() : isf_pm.h
- isf_power_set() : isf_pm.h
- pm_init() : isf_pm.h

### - s -

- isf_sm_begin_sensor_data() : isf_sm_api.h
- isf_sm_end_sensor_data() : isf_sm_api.h
- isf_sm_get_sensor_data() : isf_sm_api.h
- isf_sm_subscribe_sensor_data() : isf_sm_api.h
- isf_sm_unsubscribe_sensor_data() : isf_sm_api.h
- isf_system_sync() : isf_init.c , isf_init.h
- setup_TPM() : fxlc95000_util.h

### - t -

- task_proxy() : isf_hostproxy.h