| ISF 1.1 Intelligent Sensing Framework

- Main Page
- Data Structures
- Files
- Sensor Adapters

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Defines
Data Fields
SM_SensorSetting_t Struct Reference

`#include <isf_sm_api.h>`

## Data Fields
uint8 | nSettingsToUse
| 1 = current; 2=given; 3=best possible
uint8 | nFifoDepth
| 1 = no FIFO, or another value < SM_MAX_FIFO_DEPTH
uint32 | nCurrentReportRate
| Sample period in microseconds.
uint8 | nCurrentResolution
| Expected sensor resolution.
uint8 | nRange
| Expected sensor dynamic range.
uint8 | nMode
| sensor specific mode

## Detailed Description

Sensor configuration settings used when subscribing to sensor data.

Definition at line 143 of file isf_sm_api.h.

## Field Documentation

uint32 nCurrentReportRate

Sample period in microseconds.

Definition at line 149 of file isf_sm_api.h.

uint8 nCurrentResolution

Expected sensor resolution.

Definition at line 151 of file isf_sm_api.h.

uint8 nFifoDepth

1 = no FIFO, or another value < SM_MAX_FIFO_DEPTH

Definition at line 147 of file isf_sm_api.h.

uint8 nMode

sensor specific mode

Definition at line 153 of file isf_sm_api.h.

uint8 nRange

Expected sensor dynamic range.

Definition at line 152 of file isf_sm_api.h.

uint8 nSettingsToUse

1 = current; 2=given; 3=best possible

Definition at line 146 of file isf_sm_api.h.

The documentation for this struct was generated from the following file:

- Include/isf_sm_api.h