| ISF 1.1 Intelligent Sensing Framework

- Main Page
- Data Structures
- Files
- Sensor Adapters

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Defines
Data Fields
IICA1STR Union Reference

`#include <fxlc95000.h>`

## Data Fields
byte | Byte
union {
union {
struct {
byte __pad0__:1
byte AD1:1
byte AD2:1
byte AD3:1
byte AD4:1
byte AD5:1
byte AD6:1
byte AD7:1
} Bits
struct {
byte __pad0__:1
byte grpAD_1:7
} MergedBits
} IICA1STR
union {
struct {
byte __pad0__:1
byte AD1:1
byte AD2:1
byte AD3:1
byte AD4:1
byte AD5:1
byte AD6:1
byte AD7:1
} Bits
struct {
byte __pad0__:1
byte grpAD_1:7
} MergedBits
} IICASTR
} | SameAddr_STR

## Detailed Description

Definition at line 1746 of file fxlc95000.h.

## Field Documentation

byte __pad0__

Definition at line 1752 of file fxlc95000.h.

byte AD1

Definition at line 1753 of file fxlc95000.h.

byte AD2

Definition at line 1754 of file fxlc95000.h.

byte AD3

Definition at line 1755 of file fxlc95000.h.

byte AD4

Definition at line 1756 of file fxlc95000.h.

byte AD5

Definition at line 1757 of file fxlc95000.h.

byte AD6

Definition at line 1758 of file fxlc95000.h.

byte AD7

Definition at line 1759 of file fxlc95000.h.

struct { ... } Bits

struct { ... } Bits

byte Byte

Definition at line 1747 of file fxlc95000.h.

byte grpAD_1

Definition at line 1763 of file fxlc95000.h.

union { ... } IICA1STR

union { ... } IICASTR

struct { ... } MergedBits

struct { ... } MergedBits

union { ... } SameAddr_STR

The documentation for this union was generated from the following file:

- Include/psp/fxlc95000.h