| ISF 1.1 Intelligent Sensing Framework

- Main Page
- Data Structures
- Files
- Sensor Adapters

- File List
- Globals

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Defines
Variables
User/Source/isf_sensor_configuration.c File Reference

The isf_sensor_configuration.c file contains the list of Digital Sensor Abstraction (DSA) sensor adapters and static definition of individual sensor-specific settings. More...

`#include "isf_sysconf_comms.h"`
`#include <fsl_mag3110_i2c_3D_mag_config_types.h>`
`#include <isf_sensor_configuration.h>`

Go to the source code of this file.

## Variables
SensorConfig_t | gSensorList []
| This is the global DSA sensor adapter list currently supported by the Sensor Manager component. Each array element describes the sensor adapter for the individual sensor located at the specified device channel and the device address.
uint8 | gNumSupportedSensors = sizeof(gSensorList)/sizeof(SensorConfig_t)
| Definition and initialization of the global variable for the total number of digital sensors currently supported by the system. This definition is used by the Sensor Manager and the Digital Sensor Abstraction implementation.

## Detailed Description

The isf_sensor_configuration.c file contains the list of Digital Sensor Abstraction (DSA) sensor adapters and static definition of individual sensor-specific settings.

Copyright:
  Copyright (c) 2012, Freescale Semiconductor, Inc.

Definition in file isf_sensor_configuration.c.

## Variable Documentation

uint8 gNumSupportedSensors = sizeof(gSensorList)/sizeof(SensorConfig_t)

Definition and initialization of the global variable for the total number of digital sensors currently supported by the system.
This definition is used by the Sensor Manager and the Digital Sensor Abstraction implementation.

Definition at line 35 of file isf_sensor_configuration.c.

SensorConfig_t gSensorList[]

Initial value:

    {
            {&fsl_fxlc95000_mmap_3D_accel_adapter,     NULL, NULL,                      INTERNAL_CHAN, 0xFFFEC4 },
            {&fsl_mag3110_i2c_3D_mag_adapter,          NULL, &mag3110SpecificSettings,  I2C_MASTER1,   0x0E },
    }

This is the global DSA sensor adapter list currently supported by the Sensor Manager component. Each array element describes the sensor adapter for the individual sensor located at the specified device channel and the device address.

Definition at line 24 of file isf_sensor_configuration.c.