| ISF 1.1 Intelligent Sensing Framework

- Main Page
- Data Structures
- Files
- Sensor Adapters

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Defines
Data Fields
INTC_WCRSTR Union Reference

`#include <fxlc95000.h>`

## Data Fields
byte | Byte
struct {
byte MASK0:1
byte MASK1:1
byte MASK2:1
byte __pad0__:1
byte __pad1__:1
byte __pad2__:1
byte __pad3__:1
byte ENB:1
} | Bits
struct {
byte grpMASK:3
byte __pad0__:1
byte __pad1__:1
byte __pad2__:1
byte __pad3__:1
byte __pad4__:1
} | MergedBits

## Detailed Description

Definition at line 4492 of file fxlc95000.h.

## Field Documentation

byte __pad0__

Definition at line 4498 of file fxlc95000.h.

byte __pad1__

Definition at line 4499 of file fxlc95000.h.

byte __pad2__

Definition at line 4500 of file fxlc95000.h.

byte __pad3__

Definition at line 4501 of file fxlc95000.h.

byte __pad4__

Definition at line 4510 of file fxlc95000.h.

struct { ... } Bits

byte Byte

Definition at line 4493 of file fxlc95000.h.

byte ENB

Definition at line 4502 of file fxlc95000.h.

byte grpMASK

Definition at line 4505 of file fxlc95000.h.

byte MASK0

Definition at line 4495 of file fxlc95000.h.

byte MASK1

Definition at line 4496 of file fxlc95000.h.

byte MASK2

Definition at line 4497 of file fxlc95000.h.

struct { ... } MergedBits

The documentation for this union was generated from the following file:

- Include/psp/fxlc95000.h