| ISF 1.1 Intelligent Sensing Framework

- Main Page
- Data Structures
- Files
- Sensor Adapters

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Defines
Data Fields
ci_host_cmd_packet_t Struct Reference

This structure contains host command information. More...

`#include <isf_ci.h>`

## Data Fields
uint8 | appId
uint8 | cmd
uint16 | offset
uint8 | byte_cnt

## Detailed Description

This structure contains host command information.

This structure contains the host command and parameters passed to the embedded application for processing.

Definition at line 191 of file isf_ci.h.

## Field Documentation

uint8 appId

Application ID

Definition at line 194 of file isf_ci.h.

uint8 byte_cnt

Number of bytes to read/write

Definition at line 203 of file isf_ci.h.

uint8 cmd

Host command

Definition at line 197 of file isf_ci.h.

uint16 offset

Offset into the application's data

Definition at line 200 of file isf_ci.h.

The documentation for this struct was generated from the following file:

- Include/isf_ci.h