| ISF 1.1 Intelligent Sensing Framework

- Main Page
- Data Structures
- Files
- Sensor Adapters

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Defines
Data Fields
PCERUN0STR Union Reference

`#include <fxlc95000.h>`

## Data Fields
byte | Byte
struct {
byte FLSH:1
byte PCTRL:1
byte AFE:1
byte IRQ:1
byte T0:1
byte T1:1
byte T2:1
byte __pad0__:1
} | Bits
struct {
byte __pad0__:1
byte __pad1__:1
byte __pad2__:1
byte __pad3__:1
byte grpT:3
byte __pad4__:1
} | MergedBits

## Detailed Description

Definition at line 2344 of file fxlc95000.h.

## Field Documentation

byte __pad0__

Definition at line 2354 of file fxlc95000.h.

byte __pad1__

Definition at line 2358 of file fxlc95000.h.

byte __pad2__

Definition at line 2359 of file fxlc95000.h.

byte __pad3__

Definition at line 2360 of file fxlc95000.h.

byte __pad4__

Definition at line 2362 of file fxlc95000.h.

byte AFE

Definition at line 2349 of file fxlc95000.h.

struct { ... } Bits

byte Byte

Definition at line 2345 of file fxlc95000.h.

byte FLSH

Definition at line 2347 of file fxlc95000.h.

byte grpT

Definition at line 2361 of file fxlc95000.h.

byte IRQ

Definition at line 2350 of file fxlc95000.h.

struct { ... } MergedBits

byte PCTRL

Definition at line 2348 of file fxlc95000.h.

byte T0

Definition at line 2351 of file fxlc95000.h.

byte T1

Definition at line 2352 of file fxlc95000.h.

byte T2

Definition at line 2353 of file fxlc95000.h.

The documentation for this union was generated from the following file:

- Include/psp/fxlc95000.h