| ISF 1.1 Intelligent Sensing Framework

- Main Page
- Data Structures
- Files
- Sensor Adapters

- File List
- Globals

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Defines
User/Include/isf_user_config.h
Go to the documentation of this file.

    00001 /**
    00002  * @file isf_user_config.h
    00003  * @brief The \b isf_user_config.h file contains the user configurable settings to either include or
    00004  * exclude an ISF component.
    00005  *
    00006  * @copyright Copyright (c) 2012, Freescale Semiconductor, Inc.
    00007  */
    00008
    00009 #ifndef ISF_USER_CONFIG_H_
    00010 #define ISF_USER_CONFIG_H_
    00011
    00012 /*!
    00013  * @brief When ISF_COMPONENT_SM is defined as 1, the Sensor Manager component
    00014  * is linked to the user application.
    00015  */
    00016 #ifndef ISF_COMPONENT_SM
    00017 #define ISF_COMPONENT_SM                     (1)
    00018 #endif
    00019
    00020
    00021
    00022 /*!
    00023  * @brief When ISF_COMPONENT_CI is defined as 1, the Command Interpreter component
    00024  * is linked to the user application.
    00025  */
    00026 #ifndef ISF_COMPONENT_CI
    00027 #define ISF_COMPONENT_CI                     (1)
    00028 #endif
    00029
    00030 /*!
    00031  * @brief When ISF_COMPONENT_I2C is defined as 1, the I2C component code is
    00032  * compiled.
    00033  * <br>\b Note: The component must be recompiled when this setting is changed.
    00034  */
    00035 #ifndef ISF_COMPONENT_I2C
    00036 #define ISF_COMPONENT_I2C                     (1)
    00037 #define DEVICE_HAS_I2C_CHANNELS                (1)
    00038 #endif
    00039
    00040 /*!
    00041  * @brief When defined as 1, the Device Messaging component\n
    00042  * code will compiled.  The component must be recompiled when
    00043  * this setting is changed.
    00044  */
    00045 #ifndef ISF_COMPONENT_DEVMSG
    00046 #define ISF_COMPONENT_DEVMSG                  (1)
    00047 #endif
    00048
    00049
    00050 /*!
    00051  * @brief When ISF_COMPONENT_BM is defined as 1, the Bus Mangement component
    00052  * code is compiled.
    00053  * <br>\b Note: The component must be recompiled when this setting is changed.
    00054  */
    00055 #ifndef ISF_COMPONENT_BM
    00056 #define ISF_COMPONENT_BM                                        (1)
    00057 #endif
    00058
    00059
    00060
    00061 /*!
    00062  * @brief When defined as 1, the Power Management component\n
    00063  * code will compiled.  The component must be recompiled when
    00064  * this setting is changed.
    00065  */
    00066 #ifndef ISF_COMPONENT_PM
    00067 #define ISF_COMPONENT_PM                     (1)
    00068 #endif
    00069
    00070
    00071
    00072 #endif /* ISF_USER_CONFIG_H_ */