| ISF 1.1 Intelligent Sensing Framework

- Main Page
- Data Structures
- Files
- Sensor Adapters

- File List
- Globals

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Defines
Defines
User/Include/isf_user_config.h File Reference

The isf_user_config.h file contains the user configurable settings to either include or exclude an ISF component. More...

Go to the source code of this file.

## Defines
#define | ISF_COMPONENT_SM (1)
| When ISF_COMPONENT_SM is defined as 1, the Sensor Manager component is linked to the user application.
#define | ISF_COMPONENT_CI (1)
| When ISF_COMPONENT_CI is defined as 1, the Command Interpreter component is linked to the user application.
#define | ISF_COMPONENT_I2C (1)
| When ISF_COMPONENT_I2C is defined as 1, the I2C component code is compiled. Note: The component must be recompiled when this setting is changed.
#define | DEVICE_HAS_I2C_CHANNELS (1)
#define | ISF_COMPONENT_DEVMSG (1)
| When defined as 1, the Device Messaging component code will compiled. The component must be recompiled when this setting is changed.
#define | ISF_COMPONENT_BM (1)
| When ISF_COMPONENT_BM is defined as 1, the Bus Mangement component code is compiled. Note: The component must be recompiled when this setting is changed.
#define | ISF_COMPONENT_PM (1)
| When defined as 1, the Power Management component code will compiled. The component must be recompiled when this setting is changed.

## Detailed Description

The isf_user_config.h file contains the user configurable settings to either include or exclude an ISF component.

Copyright:
  Copyright (c) 2012, Freescale Semiconductor, Inc.

Definition in file isf_user_config.h.

## Define Documentation

#define DEVICE_HAS_I2C_CHANNELS (1)

Definition at line 37 of file isf_user_config.h.

#define ISF_COMPONENT_BM (1)

When ISF_COMPONENT_BM is defined as 1, the Bus Mangement component code is compiled.
Note: The component must be recompiled when this setting is changed.

Definition at line 56 of file isf_user_config.h.

#define ISF_COMPONENT_CI (1)

When ISF_COMPONENT_CI is defined as 1, the Command Interpreter component is linked to the user application.

Definition at line 27 of file isf_user_config.h.

#define ISF_COMPONENT_DEVMSG (1)

When defined as 1, the Device Messaging component
code will compiled. The component must be recompiled when this setting is changed.

Definition at line 46 of file isf_user_config.h.

#define ISF_COMPONENT_I2C (1)

When ISF_COMPONENT_I2C is defined as 1, the I2C component code is compiled.
Note: The component must be recompiled when this setting is changed.

Definition at line 36 of file isf_user_config.h.

#define ISF_COMPONENT_PM (1)

When defined as 1, the Power Management component
code will compiled. The component must be recompiled when this setting is changed.

Definition at line 67 of file isf_user_config.h.

#define ISF_COMPONENT_SM (1)

When ISF_COMPONENT_SM is defined as 1, the Sensor Manager component is linked to the user application.

Definition at line 17 of file isf_user_config.h.