| ISF 1.1 Intelligent Sensing Framework

- Main Page
- Data Structures
- Files
- Sensor Adapters

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Defines
Data Fields
ci_app_resp_packet_t Struct Reference

This structure enables an application to read from or write to the host. More...

`#include <isf_ci.h>`

## Data Fields
ci_rw_enum | rw
uint8 | bytes_xfer
uint8 | bytes_left

## Detailed Description

This structure enables an application to read from or write to the host.

This structure is updated by the application's CI callback as a result of handling a command from the host.

Definition at line 215 of file isf_ci.h.

## Field Documentation

uint8 bytes_left

Number of bytes left to read from or write to the host via the mailboxes.

Definition at line 232 of file isf_ci.h.

uint8 bytes_xfer

Number of bytes actually read from or written to the host via the mailboxes.

Definition at line 227 of file isf_ci.h.

ci_rw_enum rw

Application read from or write to the host:

- CI_RW_READ - application reads from the host.
- CI_RW_WRITE - application writes to the host.

Definition at line 222 of file isf_ci.h.

The documentation for this struct was generated from the following file:

- Include/isf_ci.h