| ISF 2.1 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

- File List
- Globals

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Modules Pages
FXAS21002_1.h
Go to the documentation of this file.
1 /* ###################################################################
2 ** THIS COMPONENT MODULE IS GENERATED BY THE TOOL. DO NOT MODIFY IT.
3 ** Filename : FXAS21002_1.h
4 ** CDE edition : Standard
5 ** Project : ISF_K64F_CW_PROJ
6 ** Processor : MK64FN1M0VLL12
7 ** Component : ISF_Sensor_FXAS21002_Gyrometer
8 ** Version : Component 01.000, Driver 01.00, CPU db: 3.00.000
9 ** Compiler : GNU C Compiler
10 ** Date/Time : 2015-03-03, 11:01, # CodeGen: 0
11 ** Abstract :
12 **
13 ** Settings :
14 ** Contents :
15 ** No public methods
16 **
17 ** (c) Copyright <company/user-name>, 2014
18 http://www.<company>.com
19 mail: info@<company>.com
20 ** ###################################################################*/
21 /*!
22 ** @file FXAS21002_1.h
23 ** @version 01.00
24 ** @brief
25 **
26 */
27 /*!
28 ** @addtogroup FXAS21002_1_module FXAS21002_1 module documentation
29 ** @{
30 */
31
32 #ifndef __FXAS21002_1_H
33 #define __FXAS21002_1_H
34
35 /* MODULE FXAS21002_1. */
36
37 /* Include shared modules, which are used for whole project */
38 #include "PE_Types.h"
39 #include "PE_Error.h"
40 #include "PE_Const.h"
41 #include "IO_Map.h"
42 /* Include inherited components */
43 #include "I2C_CH1.h"
44 #include <isf_sensor_types.h>
45 #include <isf_fifo.h>
46 #include <isf_accelerometer_types.h>
47 #include "fxas21002.h"
48 #include "fsl_fxas21002_i2cspi_3D_gyro.h"
49 #include "fsl_i2c_master_driver.h"
50
51
52 #include "Cpu.h"
53
54 #define FXAS21002_1_DATA_TYPE fxas21002_DataBuffer_t
55 /*!
56 * @brief This allows access to the sensor specific configuration for the target sensor.
57 *
58 */
59 extern fxas21002_Sensor_Specific_Settings_t FXAS21002_1_Sensor_Specific_Config;
60 /*!
61 * @brief This allows access to the sensor adapter instance for the target sensor.
62 *
63 */
64 extern const isf_dsa_Adapter_t FXAS21002_1_Adapter;
65
66 /*!
67 * @brief This allows access to the sensor communications specific configuration.
68 *
69 */
70 extern const i2c_device_t FXAS21002_1_DeviceInfo;
71
72
73 /* END FXAS21002_1. */
74
75 #endif
76 /* ifndef __FXAS21002_1_H */
77 /*!
78 ** @}
79 */
80 /*
81 ** ###################################################################
82 **
83 ** This file was created by Processor Expert 10.3 [05.09]
84 ** for the Freescale Kinetis series of microcontrollers.
85 **
86 ** ###################################################################
87 */
FXAS21002_1_DeviceInfo
const i2c_device_t FXAS21002_1_DeviceInfo
This allows access to the sensor communications specific configuration.
Definition: FXAS21002_1.c:69
fsl_i2c_master_driver.h
fsl_i2c_master_driver.h defines structures and types for the i2c master driver.
fsl_fxas21002_i2cspi_3D_gyro.h
The fsl_fxas21002_i2cspi_3D_gyro.h file contains the definitions and functions supporting the FXAS210...
I2CDeviceInfo
Information necessary to communicate with an I2C slave device.
Definition: fsl_i2c_master_driver.h:30
fxas21002.h
The fxas21002.h file contains the FXAS21002 Magnetometer register definitions, access macros...
I2C_CH1.h
isf_sensor_types.h
The isf_sensor_types.h contains the enumerated list of sensor types used by ISF.
isf_dsa_Adapter_st
This defines the DSA adapter structure required for static initialization of the concrete instance of...
Definition: isf_dsa_adapter.h:144
FXAS21002_1_Adapter
const isf_dsa_Adapter_t FXAS21002_1_Adapter
This allows access to the sensor adapter instance for the target sensor.
Definition: FXAS21002_1.c:54
fxas21002_Sensor_Specific_Settings_t
Definition: fxas21002.h:213
isf_fifo.h
isf_accelerometer_types.h
The isf_accelerometer_types.h file contains the ISF data type definitions for use with the ISF generi...
FXAS21002_1_Sensor_Specific_Config
fxas21002_Sensor_Specific_Settings_t FXAS21002_1_Sensor_Specific_Config
This allows access to the sensor specific configuration for the target sensor.
Definition: FXAS21002_1.c:36
- © Freescale Semiconductor, Inc. 2015. All Rights Reserved.