| ISF 2.1 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Modules Pages
Functions
RLI1 module documentation

## Functions
void | rli_app_task (void)
void | TaskRLI1_task (uint32_t task_init_data)

## Detailed Description

## Function Documentation

void rli_app_task | ( | void |  | ) |

Definition at line 127 of file rli_project.c.

References rliAppState_t::CfgBuffer, rliConfigRegister_t::channelID, COMM_CHANNEL_I2C_CH1, device_connect(), rliConfigRegister_t::deviceAddress, isf_rli_init(), and rliAppState_t::pChannelDescriptor.

Referenced by TaskRLI1_task().

Here is the call graph for this function:

Here is the caller graph for this function:

void TaskRLI1_task | ( | uint32_t | task_init_data | ) |

Definition at line 45 of file RLI1.c.

References isf_system_sync(), and rli_app_task().

Here is the call graph for this function:
- © Freescale Semiconductor, Inc. 2015. All Rights Reserved.