| ISF 2.1 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Modules Pages
Data Structures | Macros | Typedefs | Enumerations | Functions | Variables
fsl_fxos8700_i2cspi_6D_AccMag module documentation

## Data Structures
struct | fxos8700_ODR_Table_tag
| the structure defines the ODR table between Hybrid and normal mode of device operation. More...
struct | fxos8700_ConfigTable_tag
| the structure defines the configuration table. More...
struct | fxos8700_DataBuffer_t
| This structure defines the dummy DSA data buffer format. More...

## Macros
#define | FXOS8700_WHO_AM_I_VALUE1 0xC7
| FXOS8700 expected WHO_AM_I value. More...
#define | FXOS8700_WHO_AM_I_VALUE2 0xC9

## Typedefs
typedef int32 | fxos8700_Status_t
| FXOS8700 internal return codes. More...
typedef enum fxos8700_Power_tag | fxos8700_Power_t
| Enumeration for the FXOS8700 power modes. More...
typedef enum fxos8700_InternalState_tag | fxos8700_InternalState_t
| Enumeration for the FXOS8700 driver internal states. More...
typedef enum fxos8700_Mode_tag | fxos8700_Mode_t
| The enumeration, fxos8700_Mode_tag, defines the operational modes of the FXOS8700. More...
typedef enum fxos8700_Range_tag | fxos8700_Range_t
| The enumeration, fxos8700_Range_tag, defines the acceleration range of the FXOS8700. More...
typedef enum fxos8700_Resolution_tag | fxos8700_Resolution_t
| The enumeration, fxos8700_Resolution_tag, defines the bit resolution of the FXOS8700. More...
typedef struct fxos8700_ODR_Table_tag | fxo8700_ODR_Table_t
| the structure defines the ODR table between Hybrid and normal mode of device operation. More...
typedef struct fxos8700_ConfigTable_tag | fxos8700_ConfigTable_t
| the structure defines the configuration table. More...

## Enumerations
enum | fxos8700_Error_tag { FXOS8700_ERROR_WHOAMI = 1, FXOS8700_ERROR_WAITFORACTIVE, FXOS8700_ERROR_BURSTWRITE, FXOS8700_ERROR_CONFIG, FXOS8700_ERROR_SETPOWER, FX0S8700_ERRO_WRITE, FX0S8700_ERRO_READ }
| Enumeration for the FXOS8700 internal error codes. More...
enum | fxos8700_Power_tag { FXOS8700_POWER_STANDBY = 0, FXOS8700_POWER_ACTIVE = 1 }
| Enumeration for the FXOS8700 power modes. More...
enum | fxos8700_InternalState_tag { FXOS8700_STATE_UNINTIALIZED, FXOS8700_STATE_INITIALIZED, FXOS8700_STATE_CONFIGURED, FXOS8700_STATE_STARTED }
| Enumeration for the FXOS8700 driver internal states. More...
enum | fxos8700_Mode_tag { FXOS8700_MODE_ACCELEROMETER = 0, FXOS8700_MODE_MAGNETOMETER = 1, FXOS8700_MODE_HYBRID = 3, FXOS8700_MODE_EXTEND = 4 }
| The enumeration, fxos8700_Mode_tag, defines the operational modes of the FXOS8700. More...
enum | fxos8700_Range_tag { FXOS8700_RANGE_2G = 0, FXOS8700_RANGE_4G = 1, FXOS8700_RANGE_8G = 2, FXOS8700_RANGE_MAX = FXOS8700_RANGE_8G }
| The enumeration, fxos8700_Range_tag, defines the acceleration range of the FXOS8700. More...
enum | fxos8700_Resolution_tag { FXOS8700_RESOLUTION_8_BIT = 1, FXOS8700_RESOLUTION_NORMAL = 2 }
| The enumeration, fxos8700_Resolution_tag, defines the bit resolution of the FXOS8700. More...

## Functions
isf_dsa_status_t | fsl_fxos8700_i2cspi_6D_AccMag_Initialize (isf_SensorHandle_t *pSensorHandle)
| This is the concrete implementation of the FXOS8700 sensor adapter initialization. More...
isf_dsa_status_t | fsl_fxos8700_i2cspi_6D_AccMag_ValidateSettings (isf_SensorHandle_t *pSensorHandle, isf_dsa_SensorSettings_t *pSensorSettings)
| This is the concrete implementation of the FXOS8700 sensor adapter for validating current settings. More...
isf_dsa_status_t | fsl_fxos8700_i2cspi_6D_AccMag_Configure (isf_SensorHandle_t *pSensorHandle, isf_dsa_SensorSettings_t *pSensorSettings)
| This is the concrete implementation of the FXOS8700 sensor adapter for configuration. More...
isf_dsa_status_t | fsl_fxos8700_i2cspi_6D_AccMag_StartData (isf_SensorHandle_t *pSensorHandle)
| This is the concrete implementation of the FXOS8700 sensor adapter for start Data. More...
isf_dsa_status_t | fsl_fxos8700_i2cspi_6D_AccMag_EndData (isf_SensorHandle_t *pSensorHandle)
| This is the concrete implementation of the FXOS8700 sensor adapter for End Data. More...
isf_dsa_status_t | fsl_fxos8700_i2cspi_6D_AccMag_Calibrate (isf_SensorHandle_t *pSensorHandle, void *pCalData)
| This is the concrete implementation of the FXOS8700 sensor adapter for calibration . More...
isf_dsa_status_t | fsl_fxos8700_i2cspi_6D_AccMag_Shutdown (isf_SensorHandle_t *pSensorHandle)
| This is the concrete implementation of the FXOS8700 sensor adapter for shutdown . More...
isf_dsa_status_t | fsl_fxos8700_i2cspi_6D_AccMag_Convert (volatile isf_SensorHandle_t *pSensorHandle, isf_SensorDataTypes_t convertToType, isf_dsa_result_types_t resultType, void *nativeSample, void *convertedSample, int32 *numBytes)
| This function coverts the raw sample data to the desired output type. More...
void | fsl_fxos8700_i2cspi_6D_AccMag_PeriodicCallback (void *pSensorHandle)
| The callback function for the Bus Manager(BM). More...

## Variables
isf_SensorTypes_t | fxos8700_SupportedSensorTypes []
| Supported sensor and data types for fxos8700. More...
isf_SensorDataTypes_t | fxos8700_SupportedDataTypes []

## Detailed Description

## Macro Definition Documentation

#define FXOS8700_WHO_AM_I_VALUE1 0xC7

FXOS8700 expected WHO_AM_I value.

Definition at line 30 of file fsl_fxos8700_i2cspi_6D_AccMag.h.

Referenced by fsl_fxos8700_i2cspi_6D_AccMag_Initialize().

#define FXOS8700_WHO_AM_I_VALUE2 0xC9

Definition at line 31 of file fsl_fxos8700_i2cspi_6D_AccMag.h.

Referenced by fsl_fxos8700_i2cspi_6D_AccMag_Initialize().

## Typedef Documentation

typedef struct fxos8700_ODR_Table_tag fxo8700_ODR_Table_t

the structure defines the ODR table between Hybrid and normal mode of device operation.

typedef struct fxos8700_ConfigTable_tag fxos8700_ConfigTable_t

the structure defines the configuration table.

typedef enum fxos8700_InternalState_tag fxos8700_InternalState_t

Enumeration for the FXOS8700 driver internal states.

typedef enum fxos8700_Mode_tag fxos8700_Mode_t

The enumeration, fxos8700_Mode_tag, defines the operational modes of the FXOS8700.

typedef enum fxos8700_Power_tag fxos8700_Power_t

Enumeration for the FXOS8700 power modes.

typedef enum fxos8700_Range_tag fxos8700_Range_t

The enumeration, fxos8700_Range_tag, defines the acceleration range of the FXOS8700.

typedef enum fxos8700_Resolution_tag fxos8700_Resolution_t

The enumeration, fxos8700_Resolution_tag, defines the bit resolution of the FXOS8700.

typedef int32 fxos8700_Status_t

FXOS8700 internal return codes.

Definition at line 37 of file fsl_fxos8700_i2cspi_6D_AccMag.h.

## Enumeration Type Documentation

enum fxos8700_Error_tag

Enumeration for the FXOS8700 internal error codes.

Enumerator
FXOS8700_ERROR_WHOAMI | Error occurred while reading FXOS8700_WHO_AM_I or the value was incorrect.
FXOS8700_ERROR_WAITFORACTIVE | Error occurred while attempting to put device into active mode.
FXOS8700_ERROR_BURSTWRITE | Error occurred while attempting to write a block of memory to the device.
FXOS8700_ERROR_CONFIG | Error occurred while attempting to configure the device.
FXOS8700_ERROR_SETPOWER | Error occurred while attempting to set the power mode of the device.
FX0S8700_ERRO_WRITE | Error occurred while attempting to write the registers directly.
FX0S8700_ERRO_READ | Error occurred while attempting to read the registers directly.

Definition at line 41 of file fsl_fxos8700_i2cspi_6D_AccMag.h.

enum fxos8700_InternalState_tag

Enumeration for the FXOS8700 driver internal states.

Enumerator
FXOS8700_STATE_UNINTIALIZED | initial state of the device.
FXOS8700_STATE_INITIALIZED | FXOS8700_WHO_AM_I has been verified.
FXOS8700_STATE_CONFIGURED | Device has been reset and configured.
FXOS8700_STATE_STARTED | Device is in active mode and measuring data.

Definition at line 60 of file fsl_fxos8700_i2cspi_6D_AccMag.h.

enum fxos8700_Mode_tag

The enumeration, fxos8700_Mode_tag, defines the operational modes of the FXOS8700.

Enumerator
FXOS8700_MODE_ACCELEROMETER |
FXOS8700_MODE_MAGNETOMETER |
FXOS8700_MODE_HYBRID |
FXOS8700_MODE_EXTEND |

Definition at line 68 of file fsl_fxos8700_i2cspi_6D_AccMag.h.

enum fxos8700_Power_tag

Enumeration for the FXOS8700 power modes.

Enumerator
FXOS8700_POWER_STANDBY | Device in Standby mode. Less power consumption during the mode.
FXOS8700_POWER_ACTIVE | Device in active mode.

Definition at line 53 of file fsl_fxos8700_i2cspi_6D_AccMag.h.

enum fxos8700_Range_tag

The enumeration, fxos8700_Range_tag, defines the acceleration range of the FXOS8700.

Enumerator
FXOS8700_RANGE_2G |
FXOS8700_RANGE_4G |
FXOS8700_RANGE_8G |
FXOS8700_RANGE_MAX |

Definition at line 78 of file fsl_fxos8700_i2cspi_6D_AccMag.h.

enum fxos8700_Resolution_tag

The enumeration, fxos8700_Resolution_tag, defines the bit resolution of the FXOS8700.

Enumerator
FXOS8700_RESOLUTION_8_BIT |
FXOS8700_RESOLUTION_NORMAL |

Definition at line 85 of file fsl_fxos8700_i2cspi_6D_AccMag.h.

## Function Documentation

isf_dsa_status_t fsl_fxos8700_i2cspi_6D_AccMag_Calibrate | ( | isf_SensorHandle_t * | pSensorHandle,
|  | void * | pCalData
| ) |  |

This is the concrete implementation of the FXOS8700 sensor adapter for calibration .

The FXAS21000 does not provide the capability to be dynamically calibrated. Therefore, this function simply returns success.

Parameters

  [in] | pSensorHandle | This is a pointer to the instance of the FXOS8700 sensor adapter.
  [in] | pCalData | This is a void pointer to the instance of the FXOS8700 calibration data.

Returns
  fsl_fxos8700_i2cspi_6D_AccMag_Calibrate() returns a value of type isf_dsa_status_t indicating the success or failure of the function call.

Return values

  ISF_SUCCESS | is returned when the device is calibrated properly. Note: Currently, there is no return error type defined for this API.

Constraints:
  None

Reentrant: Yes

Link Libraries:
  fsl_fxos8700_i2cspi_6D_AccMag.lib

Definition at line 541 of file fsl_fxos8700_i2cspi_6D_AccMag.c.

References ISF_SUCCESS.

isf_dsa_status_t fsl_fxos8700_i2cspi_6D_AccMag_Configure | ( | isf_SensorHandle_t * | pSensorHandle,
|  | isf_dsa_SensorSettings_t * | pSensorSettings
| ) |  |

This is the concrete implementation of the FXOS8700 sensor adapter for configuration.

This function resets the sensor, applies the settings, and registers a callback with the Bus Manager(BM) timer. It does not yet start the timer, as this is done by fsl_fxos8700_i2cspi_6D_AccMag_StartData().

Parameters

  [in] | pSensorHandle | This is a pointer to the instance of the FXAS21000 sensor adapter.
  [in] | pSensorSettings | The reference to the sensor configuration settings.

Returns
  fsl_fxos8700_i2cspi_6D_AccMag_Configure() returns a value of type isf_dsa_status_t indicating the success or failure of the function call.

Return values

  ISF_SUCCESS | is returned when the device is configured successfully.
  DSA_ERR_CONFIGURE | is returned when the provided configuration settings could not be applied.

Constraints:
  None

Reentrant: Yes

Link Libraries:
  fsl_fxos8700_i2cspi_6D_AccMag.lib

Definition at line 286 of file fsl_fxos8700_i2cspi_6D_AccMag.c.

References isf_SensorHandle_st::adapterStatus, BM_ERROR, bm_register_periodic_callback(), DeviceDescriptor_struct::cDescriptor, isf_SensorHandle_st::controlData, DeviceDescriptor_struct::deviceHandle, DeviceDescriptor_struct::deviceSemaphore, dm_channel_acquire_lock(), dm_channel_release_lock(), dm_device_read(), dm_device_write(), DSA_ERR_CONFIGURE, DSA_ERR_PARAM, DSA_STATE_CONFIGURED_STOPPED, DSA_STATE_INITIALIZED, fsl_fxos8700_i2cspi_6D_AccMag_PeriodicCallback(), FXOS8700_ACTIVE_MASK, FXOS8700_CTRL_REG1, FXOS8700_MODE_HYBRID, FXOS8700_SET_FIELD, GET_ODR_CONFIG, ISF_SUCCESS, isf_dsa_SensorSettings_st::nSamplePeriod, isf_SensorHandle_st::pDeviceDescriptor, SensorConfig_st::pSensorSpecificSettings, isf_SensorHandle_st::pSensorStaticConfig, fxos8700_Sensor_Specific_Reg_t::regAddr, fxos8700_Sensor_Specific_Settings_t::regCount, fxos8700_Sensor_Specific_Settings_t::regPairs, fxos8700_Sensor_Specific_Reg_t::regValue, isf_dsa_ControlData_st::sensorSettings, and DeviceDescriptor_struct::token.

Here is the call graph for this function:

isf_dsa_status_t fsl_fxos8700_i2cspi_6D_AccMag_Convert | ( | volatile isf_SensorHandle_t * | pSensorHandle,
|  | isf_SensorDataTypes_t | convertToType,
|  | isf_dsa_result_types_t | resultType,
|  | void * | nativeSample,
|  | void * | convertedSample,
|  | int32 * | numBytes
| ) |  |

This function coverts the raw sample data to the desired output type.

Definition at line 732 of file fsl_fxos8700_i2cspi_6D_AccMag.c.

References DSA_ERR_BAD_RESULT_TYPE, DSA_ERR_BAD_SENSOR_DATA_TYPE, DSA_RESULT_TYPE_ENG_FIXED, DSA_RESULT_TYPE_ENG_FLOAT, SensorConfig_st::pSensorSpecificSettings, isf_SensorHandle_st::pSensorStaticConfig, TYPE_MAGNETIC_FIELD_STRENGTH_3D, and TYPE_RAW_ACCELERATION_3D.

Referenced by fsl_fxos8700_i2cspi_6D_AccMag_PeriodicCallback().

Here is the caller graph for this function:

isf_dsa_status_t fsl_fxos8700_i2cspi_6D_AccMag_EndData | ( | isf_SensorHandle_t * | pSensorHandle | ) |

This is the concrete implementation of the FXOS8700 sensor adapter for End Data.

This function tells the Bus Manager to stop the callbacks and disable data collection.

Parameters

  [in] | pSensorHandle | This is a pointer to the instance of the FXOS8700 sensor adapter.

Returns
  fsl_fxos8700_i2cspi_6D_AccMag_EndData() returns a value of type isf_dsa_status_t indicating the success or failure of the function call.

Return values

  ISF_SUCCESS | is returned when the data collection stopped successfully.
  DSA_ERR_PARAM | is returned when a wrong parameter is passed into the function such as an invalid or NULL parameter.

Constraints:
  None

Reentrant: Yes

Link Libraries:
  fsl_fxos8700_i2cspi_6D_AccMag.lib

Definition at line 477 of file fsl_fxos8700_i2cspi_6D_AccMag.c.

References isf_SensorHandle_st::adapterStatus, BM_ERROR, bm_stop(), DeviceDescriptor_struct::deviceHandle, DeviceDescriptor_struct::deviceSemaphore, DSA_ERR_END_DATA, DSA_ERR_PARAM, DSA_STATE_CONFIGURED_STARTED, DSA_STATE_CONFIGURED_STOPPED, FXOS8700_POWER_STANDBY, ISF_SUCCESS, isf_SensorHandle_st::pDeviceDescriptor, and DeviceDescriptor_struct::token.

Here is the call graph for this function:

isf_dsa_status_t fsl_fxos8700_i2cspi_6D_AccMag_Initialize | ( | isf_SensorHandle_t * | pSensorHandle | ) |

This is the concrete implementation of the FXOS8700 sensor adapter initialization.

This function allocates memory for the device descriptor.

Parameters

  [in] | pSensorHandle | This is a void pointer to the instance of the FXOS8700 sensor adapter.

Returns
  fsl_fxos8700_i2cspi_6D_AccMag_Initialize() returns a value of type isf_dsa_status_t indicating the success or failure of the function call.

Return values

  ISF_SUCCESS | is returned when the device is initialized properly.
  DSA_ERR_PARAM | is returned when a wrong parameter was passed into the function, i.e. an invalid or NULL parameter.
  DSA_ERR_INITIALIZE | is returned when the driver could not be initialized successfully.

Constraints:
  None

Reentrant: Yes

Link Libraries:
  fsl_fxos8700_i2cspi_6D_AccMag.lib

Definition at line 155 of file fsl_fxos8700_i2cspi_6D_AccMag.c.

References fxos8700_DataBuffer_t::accel, isf_SensorHandle_st::adapterStatus, fxos8700_DataBuffer_t::addr, DeviceDescriptor_struct::cDescriptor, SensorConfig_st::channelId, COMM_STATE_OK, SensorConfig_st::commInfo, DeviceDescriptor_struct::deviceHandle, DeviceDescriptor_struct::deviceSemaphore, dm_channel_get_state(), dm_channel_init(), dm_channel_start(), dm_device_open(), DSA_ERR_INITIALIZE, DSA_ERR_PARAM, DSA_STATE_INITIALIZED, DSA_STATE_NOT_INITIALIZED, FXOS8700_WHO_AM_I_VALUE1, FXOS8700_WHO_AM_I_VALUE2, ISF_SUCCESS, fxos8700_DataBuffer_t::mag, DeviceDescriptor_struct::pCurrentSample, isf_SensorHandle_st::pDeviceDescriptor, isf_SensorHandle_st::pSensorStaticConfig, DeviceDescriptor_struct::skipFramecnt, and fxos8700_DataBuffer_t::timeStamp.

Here is the call graph for this function:

void fsl_fxos8700_i2cspi_6D_AccMag_PeriodicCallback | ( | void * | pSensorHandle | ) |

The callback function for the Bus Manager(BM).

The Bus Manager calls this function periodically based on the period configured for the FXOS8700.

Parameters

  [in] | pSensorHandle | This is a void pointer to the instance of the FXOS8700 sensor adapter.

Returns
  Void There is no return value.

Constraints:
  None

Reentrant: Yes

Link Libraries:
  fsl_fxos8700_i2cspi_6D_AccMag.lib

Definition at line 584 of file fsl_fxos8700_i2cspi_6D_AccMag.c.

References fxos8700_DataBuffer_t::accel, isf_SensorHandle_st::adapterStatus, isf_SensorHandle_st::controlData, DeviceDescriptor_struct::deviceHandle, DeviceDescriptor_struct::deviceSemaphore, dm_device_read(), DSA_STATE_CONFIGURED_STARTED, fsl_fxos8700_i2cspi_6D_AccMag_Convert(), FXOS8700_M_OUT_X_MSB, FXOS8700_MODE_ACCELEROMETER, FXOS8700_MODE_HYBRID, FXOS8700_MODE_MAGNETOMETER, FXOS8700_OUT_X_MSB, isf_fifo_el_get_insert_pointer(), isf_fifo_el_increment(), ISF_FIFO_FULL, isf_fifo_lock(), isf_fifo_unlock(), isf_time_util_get_usec(), fxos8700_DataBuffer_t::mag, isf_dsa_ControlData_st::nEventFieldIndex, DeviceDescriptor_struct::pCurrentSample, isf_SensorHandle_st::pDeviceDescriptor, isf_dsa_ControlData_st::pEventGroup, isf_dsa_SensorSettings_st::pSampleBufferInfo, SensorConfig_st::pSensorSpecificSettings, isf_SensorHandle_st::pSensorStaticConfig, isf_dsa_SensorSettings_st::resultFormat, isf_dsa_SensorSettings_st::resultType, isf_dsa_ControlData_st::sensorSettings, DeviceDescriptor_struct::skipFramecnt, fxos8700_DataBuffer_t::timeStamp, and TYPE_NATIVE_SENSOR_DATA_TYPE.

Referenced by fsl_fxos8700_i2cspi_6D_AccMag_Configure().

Here is the call graph for this function:

Here is the caller graph for this function:

isf_dsa_status_t fsl_fxos8700_i2cspi_6D_AccMag_Shutdown | ( | isf_SensorHandle_t * | pSensorHandle | ) |

This is the concrete implementation of the FXOS8700 sensor adapter for shutdown .

Parameters

  [in] | pSensorHandle | This is a pointer to the instance of the FXOS8700 sensor adapter.

Returns
  fsl_fxos8700_i2cspi_6D_AccMag_Shutdown() returns a value of type isf_dsa_status_t indicating the success or failure of the function call.

Return values

  ISF_SUCCESS | is returned when the device is calibrated properly. Note: Currently, there is no return error type defined for this API.

Constraints:
  None

Reentrant: Yes

Link Libraries:
  fsl_fxos8700_i2cspi_6D_AccMag.lib

Definition at line 558 of file fsl_fxos8700_i2cspi_6D_AccMag.c.

References isf_SensorHandle_st::adapterStatus, bm_unregister_callback(), DSA_ERR_PARAM, DSA_STATE_INITIALIZED, ISF_SUCCESS, isf_SensorHandle_st::pDeviceDescriptor, and DeviceDescriptor_struct::token.

Here is the call graph for this function:

isf_dsa_status_t fsl_fxos8700_i2cspi_6D_AccMag_StartData | ( | isf_SensorHandle_t * | pSensorHandle | ) |

This is the concrete implementation of the FXOS8700 sensor adapter for start Data.

This function tells the Bus Manager to start the callbacks periodically as defined in the bus configuration and enable the data collection.

Parameters

  [in] | pSensorHandle | This is a pointer to the instance of the FXOS8700 sensor adapter.

Returns
  fsl_fxos8700_i2cspi_6D_AccMag_StartData() returns a value of type isf_dsa_status_t indicating the success or failure of the function call.

Return values

  ISF_SUCCESS | is returned when the data collection callback triggered successfully.
  DSA_ERR_PARAM | is returned when a wrong parameter is passed into the function such as an invalid or NULL parameter.

Constraints:
  None

Reentrant: Yes

Link Libraries:
  fsl_fxos8700_i2cspi_6D_AccMag.lib

Definition at line 412 of file fsl_fxos8700_i2cspi_6D_AccMag.c.

References isf_SensorHandle_st::adapterStatus, BM_ERROR, bm_start(), DeviceDescriptor_struct::deviceHandle, DeviceDescriptor_struct::deviceSemaphore, DSA_ERR_PARAM, DSA_ERR_START_DATA, DSA_STATE_CONFIGURED_STARTED, DSA_STATE_CONFIGURED_STOPPED, FALSE, FXOS8700_POWER_ACTIVE, ISF_SUCCESS, fxos8700_Sensor_Specific_Settings_t::mode, isf_SensorHandle_st::pDeviceDescriptor, SensorConfig_st::pSensorSpecificSettings, isf_SensorHandle_st::pSensorStaticConfig, and DeviceDescriptor_struct::token.

Here is the call graph for this function:

isf_dsa_status_t fsl_fxos8700_i2cspi_6D_AccMag_ValidateSettings | ( | isf_SensorHandle_t * | pSensorHandle,
|  | isf_dsa_SensorSettings_t * | pSensorSettings
| ) |  |

This is the concrete implementation of the FXOS8700 sensor adapter for validating current settings.

This function is responsible for validating the current settings and if the current settings are not valid settings, it provides the best suitable settings.

Parameters

  [in] | pSensorHandle | This is a pointer to the instance of the FXOS8700 sensor adapter.
  [in] | pSensorSettings | The reference to the sensor settings.

Returns
  fsl_fxos8700_i2cspi_6D_AccMag_ValidateSettings() returns a value of type isf_dsa_status_t indicating the success or failure of the function call.

Return values

  ISF_SUCCESS | is returned when the device settings are successfully validated.
  DSA_RET_SETTINGS_CHANGED | is returned when the current settings have been changed.

Constraints:
  None

Reentrant: Yes

Link Libraries:
  fsl_fxos8700_i2cspi_6D_AccMag.lib

Definition at line 245 of file fsl_fxos8700_i2cspi_6D_AccMag.c.

References DSA_ERR_PARAM, DSA_RET_SETTINGS_CHANGED, GET_ODR_VALUE, ISF_SUCCESS, fxos8700_Sensor_Specific_Settings_t::mode, isf_dsa_SensorSettings_st::nSamplePeriod, SensorConfig_st::pSensorSpecificSettings, and isf_SensorHandle_st::pSensorStaticConfig.

## Variable Documentation

isf_SensorDataTypes_t fxos8700_SupportedDataTypes[]

Definition at line 59 of file fsl_fxos8700_i2cspi_6D_AccMag.c.

isf_SensorTypes_t fxos8700_SupportedSensorTypes[]

Supported sensor and data types for fxos8700.

Supported sensor and data types for fxos8700.

Definition at line 58 of file fsl_fxos8700_i2cspi_6D_AccMag.c.

- © Freescale Semiconductor, Inc. 2015. All Rights Reserved.