| ISF 2.1 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Modules Pages
Data Fields
uart_instance_PEx Struct Reference

This structure contains i2c LLD function pointers. More...

`#include <isf_fsl_uart_PEx.h>`

Collaboration diagram for uart_instance_PEx:

## Data Fields
fnUARTInit_t | fnUARTLLDInit
fnUARTRead_t | fnUARTCLLDRead
fnUARTWrite_t | fnUARTLLDWrite

## Detailed Description

This structure contains i2c LLD function pointers.

Definition at line 26 of file isf_fsl_uart_PEx.h.

## Field Documentation

fnUARTRead_t fnUARTCLLDRead

Read from a device.

Definition at line 28 of file isf_fsl_uart_PEx.h.

Referenced by uart_receive_data().

fnUARTInit_t fnUARTLLDInit

Initialize a UART LDD component.

Definition at line 27 of file isf_fsl_uart_PEx.h.

Referenced by uart_init().

fnUARTWrite_t fnUARTLLDWrite

Write to a device.

Definition at line 29 of file isf_fsl_uart_PEx.h.

Referenced by uart_send_data().

The documentation for this struct was generated from the following file:

- ISF/ProtocolAdapter/Include/isf_fsl_uart_PEx.h

- © Freescale Semiconductor, Inc. 2015. All Rights Reserved.