| ISF 2.1 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Modules Pages
Data Fields
UartUserConfig Struct Reference
Uart_driver

User configuration structure for UART driver. More...

`#include <fsl_uart_driver.h>`

Collaboration diagram for UartUserConfig:

## Data Fields
uint32_t | baudRate
uart_parity_mode_t | parityMode
uart_stop_bit_count_t | stopBitCount
uart_bit_count_per_char_t | bitCountPerChar

## Detailed Description

User configuration structure for UART driver.

Use an instance of this struct with uart_init(). This allows you to configure the most common settings of the UART peripheral with a single function call. Settings include: UART baud rate; UART parity mode: disabled (default), or even or odd; the number of stop bits; the number of bits per data word.

Definition at line 58 of file fsl_uart_driver.h.

## Field Documentation

uint32_t baudRate

UART baud rate

Definition at line 59 of file fsl_uart_driver.h.

Referenced by uart_adapter_configure().

uart_bit_count_per_char_t bitCountPerChar

number of bits, 8-bit (default) or 9-bit in a word (up to 10-bits in some UART instances)

Definition at line 63 of file fsl_uart_driver.h.

Referenced by uart_adapter_configure().

uart_parity_mode_t parityMode

parity mode, disabled (default), even, odd

Definition at line 60 of file fsl_uart_driver.h.

Referenced by uart_adapter_configure().

uart_stop_bit_count_t stopBitCount

number of stop bits, 1 stop bit (default) or 2 stop bits

Definition at line 61 of file fsl_uart_driver.h.

Referenced by uart_adapter_configure().

The documentation for this struct was generated from the following file:

- ISF/ProtocolAdapter/Include/fsl_uart_driver.h

- © Freescale Semiconductor, Inc. 2015. All Rights Reserved.