| ISF 2.1 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Modules Pages
Macros | Typedefs | Functions | Variables
ISFCore1 module documentation

## Macros
#define | __CDEUserType_ISFCore1_Type

## Typedefs
typedef char | ISFCore1_Type

## Functions
ci_response_enum | rli_ci_app_callback (ci_host_cmd_packet_t *, ci_app_resp_packet_t *)
ci_response_enum | App1_ci_app_callback (ci_host_cmd_packet_t *, ci_app_resp_packet_t *)
void | PM_task (uint32_t task_init_data)
void | CI_task (uint32_t task_init_data)

## Variables
const ci_funcp_t | ci_callback []
| Command interpreter callbacks. The array index is the application ID. More...

## Detailed Description

## Macro Definition Documentation

#define __CDEUserType_ISFCore1_Type

Definition at line 62 of file ISFCore1.h.

## Typedef Documentation

typedef char ISFCore1_Type

Definition at line 63 of file ISFCore1.h.

## Function Documentation

ci_response_enum App1_ci_app_callback | ( | ci_host_cmd_packet_t * | ,
|  | ci_app_resp_packet_t * |
| ) |  |

Definition at line 313 of file App1.c.

References App1_GotoState(), App1_STATE_STOPPED_UNSUBSCRIBED, App1AppInstance_t::appId, ci_host_cmd_packet_t::appId, ci_host_cmd_packet_t::byte_cnt, ci_app_resp_packet_t::bytes_xfer, CI_CMD_READ_APP_DATA, CI_CMD_READ_CONFIG, CI_CMD_RESET_APP, CI_CMD_UPDATE_QUICKREAD, CI_CMD_WRITE_CONFIG, CI_ERROR_COMMAND, CI_ERROR_NONE, CI_INVALID_COUNT, ci_host_cmd_packet_t::cmd, App1AppSettings_t::control, CTRL_POWER_MASK, CTRL_STATE_MASK, App1AppInstance_t::data, GET_FIELD, App1AppInstance_t::instance, isf_ci_app_read(), isf_ci_app_write(), isf_ci_qr_update(), isf_power_set(), isf_SubscriptionSettings_t::nSamplePeriod, ci_host_cmd_packet_t::offset, App1AppSettings_t::OrientSettings_Sub0, App1AppInstance_t::outputBufferLock, App1AppSettings_t::PressSettings_Sub1, SET_FIELD, App1AppInstance_t::settings, and startof.

Here is the call graph for this function:

void CI_task | ( | uint32_t | task_init_data | ) |

Definition at line 94 of file ISFCore1.c.

References isf_system_sync(), and task_ci().

Here is the call graph for this function:

void PM_task | ( | uint32_t | task_init_data | ) |

Definition at line 71 of file ISFCore1.c.

References isf_system_sync(), and task_idle().

Here is the call graph for this function:

ci_response_enum rli_ci_app_callback | ( | ci_host_cmd_packet_t * | ,
|  | ci_app_resp_packet_t * |
| ) |  |

Definition at line 151 of file rli_project.c.

References device_cmd_packet_t::appId, ci_host_cmd_packet_t::appId, ci_host_cmd_packet_t::byte_cnt, ci_app_resp_packet_t::bytes_xfer, rliAppState_t::CfgBuffer, rliAppStatus_t::channel, CI_CMD_DEVICE_READ, CI_CMD_DEVICE_WRITE, CI_CMD_READ_APP_DATA, CI_CMD_READ_APP_STATUS, CI_CMD_READ_CONFIG, CI_CMD_RESET_APP, CI_CMD_UPDATE_QUICKREAD, CI_CMD_WRITE_CONFIG, CI_ERROR_COMMAND, CI_ERROR_NONE, CI_INVALID_COUNT, CI_RW_READ, CI_RW_WRITE, close_channel(), device_cmd_packet_t::cmd, ci_host_cmd_packet_t::cmd, rliAppState_t::cmdBuffer, cmdBuffer_t, rliAppStatus_t::device, device_connect(), device_disconnect(), rliAppStatus_t::error, FSL_RLI_APP_ID, isf_ci_app_read(), isf_ci_app_write(), isf_ci_qr_update(), isf_rli_read(), isf_rli_write(), ISF_SUCCESS, device_cmd_packet_t::nRead, device_cmd_packet_t::nWrite, ci_host_cmd_packet_t::offset, open_channel(), rliAppState_t::pHandle, rliAppState_t::rcvBuffer, rcvBuffer_t, RLI_APP_STATE_OPEN, ci_app_resp_packet_t::rw, and rliAppState_t::status.

Here is the call graph for this function:

## Variable Documentation

const ci_funcp_t ci_callback[]

Initial value:
=
{
ISF_APP_CALLBACKS
rli_ci_app_callback,
App1_ci_app_callback,
0
}
App1_ci_app_callback
ci_response_enum App1_ci_app_callback(ci_host_cmd_packet_t *, ci_app_resp_packet_t *)
Definition: App1.c:313
ISF_APP_CALLBACKS
#define ISF_APP_CALLBACKS
This macro defines the ISF application Command Interpreter callback(s). Note: The user must put thes...
Definition: isf_init.h:343
rli_ci_app_callback
ci_response_enum rli_ci_app_callback(ci_host_cmd_packet_t *, ci_app_resp_packet_t *)
Definition: rli_project.c:151

Command interpreter callbacks. The array index is the application ID.

Definition at line 49 of file ISFCore1.c.

Referenced by ci_mbox_init(), ci_protocol_CB_mbox(), and ci_qr_update().

- © Freescale Semiconductor, Inc. 2015. All Rights Reserved.