| ISF 2.1 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

- File List
- Globals

- All
- Functions
- Variables
- Typedefs
- Enumerations
- Enumerator
- Macros

- _
- a
- b
- c
- d
- e
- f
- g
- h
- i
- k
- l
- m
- n
- o
- p
- q
- r
- s
- t
- u
- v
- w
- x
- y
- z

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Modules Pages
Here is a list of all functions, variables, defines, enums, and typedefs with links to the files they belong to:

### - k -

- kI2CAddress7bitMask : fsl_i2c_master_driver.c
- kI2CNoStart : fsl_i2c_master_driver.h
- kI2CNoStop : fsl_i2c_master_driver.h
- kI2CRead : fsl_i2c_master_driver.h
- kI2CWrite : fsl_i2c_master_driver.h
- kSpiClockPhase_FirstEdge : fsl_spi_hal.h
- kSpiClockPhase_SecondEdge : fsl_spi_hal.h
- kSpiClockPolarity_ActiveHigh : fsl_spi_hal.h
- kSpiClockPolarity_ActiveLow : fsl_spi_hal.h
- kSpiLsbFirst : fsl_spi_hal.h
- kSpiMaster : fsl_spi_hal.h
- kSpiMsbFirst : fsl_spi_hal.h
- kSpiPinMode_Input : fsl_spi_hal.h
- kSpiPinMode_Normal : fsl_spi_hal.h
- kSpiPinMode_Output : fsl_spi_hal.h
- kSpiSlave : fsl_spi_hal.h
- kSpiSlaveSelect_AsGpio : fsl_spi_hal.h
- kSpiSlaveSelect_AutomaticOutput : fsl_spi_hal.h
- kSpiSlaveSelect_FaultInput : fsl_spi_hal.h
- kSpiWaitForever : fsl_spi_master_driver.h
- kStatus_I2C_AribtrationLost : fsl_i2c_hal.h
- kStatus_I2C_Busy : fsl_i2c_hal.h
- kStatus_I2C_Fail : fsl_i2c_hal.h
- kStatus_I2C_InvalidArgument : fsl_i2c_hal.h
- kStatus_I2C_OutOfRange : fsl_i2c_hal.h
- kStatus_I2C_ReceivedNak : fsl_i2c_hal.h
- kStatus_I2C_SlaveRxOverrun : fsl_i2c_hal.h
- kStatus_I2C_SlaveTxUnderrun : fsl_i2c_hal.h
- kStatus_I2C_Success : fsl_i2c_hal.h
- kStatus_I2C_Timeout : fsl_i2c_hal.h
- kStatus_SPI_Busy : fsl_spi_hal.h
- kStatus_SPI_Error : fsl_spi_hal.h
- kStatus_SPI_NoTransferInProgress : fsl_spi_hal.h
- kStatus_SPI_SlaveRxOverrun : fsl_spi_hal.h
- kStatus_SPI_SlaveTxUnderrun : fsl_spi_hal.h
- kStatus_SPI_Success : fsl_spi_hal.h
- kStatus_SPI_Timeout : fsl_spi_hal.h
- kStatus_UART_BaudRateCalculationError : fsl_uart_hal.h
- kStatus_UART_BaudRatePercentDiffExceeded : fsl_uart_hal.h
- kStatus_UART_BitCountNotSupported : fsl_uart_hal.h
- kStatus_UART_BothEdgeNotSupported : fsl_uart_hal.h
- kStatus_UART_ClearStatusFlagError : fsl_uart_hal.h
- kStatus_UART_Error : fsl_uart_hal.h
- kStatus_UART_InvalidBitSetting : fsl_uart_hal.h
- kStatus_UART_InvalidInstanceNumber : fsl_uart_hal.h
- kStatus_UART_MSBFirstNotSupported : fsl_uart_hal.h
- kStatus_UART_NoReceiveInProgress : fsl_uart_hal.h
- kStatus_UART_NoTransmitInProgress : fsl_uart_hal.h
- kStatus_UART_OverSamplingNotSupported : fsl_uart_hal.h
- kStatus_UART_ResyncNotSupported : fsl_uart_hal.h
- kStatus_UART_RxBusy : fsl_uart_hal.h
- kStatus_UART_RxNotDisabled : fsl_uart_hal.h
- kStatus_UART_RxStandbyModeError : fsl_uart_hal.h
- kStatus_UART_StopBitCountNotSupported : fsl_uart_hal.h
- kStatus_UART_Success : fsl_uart_hal.h
- kStatus_UART_Timeout : fsl_uart_hal.h
- kStatus_UART_TxBusy : fsl_uart_hal.h
- kStatus_UART_TxNotDisabled : fsl_uart_hal.h
- kStatus_UART_TxOrRxNotDisabled : fsl_uart_hal.h
- kUart10BitsPerChar : fsl_uart_hal.h
- kUart8BitsPerChar : fsl_uart_hal.h
- kUart9BitsPerChar : fsl_uart_hal.h
- kUartAddrMarkWake : fsl_uart_hal.h
- kUartBreakChar10BitMinimum : fsl_uart_hal.h
- kUartBreakChar13BitMinimum : fsl_uart_hal.h
- kUartIdleLineAfterStartBit : fsl_uart_hal.h
- kUartIdleLineAfterStopBit : fsl_uart_hal.h
- kUartIdleLineWake : fsl_uart_hal.h
- kUartOneStopBit : fsl_uart_hal.h
- kUartOperates : fsl_uart_hal.h
- kUartParityDisabled : fsl_uart_hal.h
- kUartParityEven : fsl_uart_hal.h
- kUartParityOdd : fsl_uart_hal.h
- kUartStops : fsl_uart_hal.h
- kUartTwoStopBit : fsl_uart_hal.h

- © Freescale Semiconductor, Inc. 2015. All Rights Reserved.