| ISF 2.1 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

- File List
- Globals

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Modules Pages
Macros | Functions | Variables
FXLS8471_1.c File Reference
`#include "FXLS8471_1.h"`
`#include "isf_target.h"`
`#include "isf.h"`
`#include "isf_spi_master_types.h"`
`#include "isf_util.h"`
`#include "GPIO1.h"`
Include dependency graph for FXLS8471_1.c:

Go to the source code of this file.

## Macros
#define | FSL_SENSOR_SPI_CMD_LENG 0x2

## Functions
isf_status_t | fsl_veryon_spi_slave_init (void)
isf_status_t | fsl_veryon_spi_slave_write_preprocess (void *pCmdOut, uint32 offset, uint32 size, void *pWritebuffer)
isf_status_t | fsl_veryon_spi_slave_write_postprocess (void *pCmdOut)
isf_status_t | fsl_veryon_spi_slave_read_preprocess (void *pCmdOut, uint32 offset, uint32 size)
isf_status_t | fsl_veryon_spi_slave_read_postprocess (void *pCmdOut, void *pDataOut)

## Variables
fxls8471_Sensor_Specific_Settings_t | FXLS8471_1_Sensor_Specific_Config
| This allows access to the sensor specific configuration for the target sensor. More...
const isf_dsa_Adapter_t | FXLS8471_1_Adapter
| This creates the sensor adapter instance for the target sensor. More...
spi_master_slaveInfo_t | fsl_spi_sensor_type
const spi_master_CommSpecificInfo_t | FXLS8471_1_DeviceInfo
| This allows access to the sensor communications specific configuration. More...

## Detailed Description

Version
  01.00

Definition in file FXLS8471_1.c.

- © Freescale Semiconductor, Inc. 2015. All Rights Reserved.